{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["ORIGINAL1"],"not_rendered":{"charts":0,"images":372,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ORIGINAL1","index":0,"n_rows":1586,"n_cols":7,"rows_kept":1586,"cut":false,"hidden":false,"merged":[]}
[null,"DESCRIPCION","REFERENCIA","P.V.P.","EAN","Enlace foto","Foto"]
[1,"Pack 5 ud. boquillas exteriores Nº 1 espesor 2-10 mm.","70119101P",49.71,8430133541620,"https://galagar.com/wp-content/uploads/2022/01/Boquillas-CorteExterior.jpg",{"$error":"#VALUE!"}]
[2,"Pack 5 ud. boquillas exteriores Nº 2 espesor 10-25 mm.","70119102P",49.71,8430133585211,"https://galagar.com/wp-content/uploads/2022/01/Boquillas-CorteExterior.jpg",{"$error":"#VALUE!"}]
[3,"Pack 5 ud. boquillas exteriores Nº 3 espesor 25-100 mm.","70119103P",49.71,8430133585198,"https://galagar.com/wp-content/uploads/2022/01/Boquillas-CorteExterior.jpg",{"$error":"#VALUE!"}]
[4,"Pack 5 ud. boquillas exteriores Nº 4 espesor 100-300 mm.","70119104P",49.71,8430133541651,"https://galagar.com/wp-content/uploads/2022/01/Boquillas-CorteExterior.jpg",{"$error":"#VALUE!"}]
[5,"Pack 5 ud. boquillas interiores Nº 1 espesor 4-9 mm.","70119201P",29.19,8430133541668,"https://galagar.com/wp-content/uploads/2022/01/Boquillas-CorteInterior.jpg",{"$error":"#VALUE!"}]
[6,"Pack 5 ud. boquillas interiores Nº 2 espesor 9-25 mm.","70119202P",29.19,8430133585204,"https://galagar.com/wp-content/uploads/2022/01/Boquillas-CorteInterior.jpg",{"$error":"#VALUE!"}]
[7,"Pack 5 ud. boquillas interiores Nº 3 espesor 25-50 mm.","70119203P",29.19,8430133541682,"https://galagar.com/wp-content/uploads/2022/01/Boquillas-CorteInterior.jpg",{"$error":"#VALUE!"}]
[8,"Pack 5 ud. boquillas interiores Nº 4 espesor 50-75 mm.","70119204P",29.19,8430133585228,"https://galagar.com/wp-content/uploads/2022/01/Boquillas-CorteInterior.jpg",{"$error":"#VALUE!"}]
[9,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 1 espesor 4-9 mm.","71400201P",49.71,8430133580575,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[10,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 2 espesor 9-25 mm.","71400202P",49.71,8430133580582,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[11,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 3 espesor 25-50 mm.","71400203P",49.71,8430133580599,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[12,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 4 espesor 50-75 mm.","71400204P",49.71,8430133580605,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[13,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 5 espesor 75-150 mm.","71400205P",49.71,8430133580612,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[14,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 6 espesor 150-200 mm.","71400206P",49.71,8430133580629,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[15,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 7 espesor 200-300 mm.","71400207P",49.71,8430133580636,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[16,"Dispositivo de corte oxígeno / acetileno",70100000,110.28,8430133305031,"https://galagar.com/wp-content/uploads/2022/01/Dispositivo-Corte-AC.jpg",{"$error":"#VALUE!"}]
[17,"Dispositivo de corte oxígeno / acetileno / propano Tipo H",70100030,110.28,8430133305048,"https://galagar.com/wp-content/uploads/2022/01/Dispositivo-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[18,"Mango universal oxígeno / acetileno / propano",70200100,122.67,8430133579579,"https://galagar.com/wp-content/uploads/2022/01/MangoUniersal.jpg",{"$error":"#VALUE!"}]
[19,"Conjunto 5 m. manguera con racor universal para oxígeno / acetileno",78000705,63.01,8430133340971,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[20,"Conjunto 10 m. manguera con racor universal para oxígeno / acetileno",78000710,112.21,8430133340988,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[21,"Conjunto 15 m. manguera con racor universal para oxígeno / acetileno",78000715,143.84,8430133340995,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[22,"Válvula seguridad oxígeno para mango",73000000,22.99,8430133580032,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[23,"Válvula seguridad gas combustible para mango",73100020,22.99,8430133580094,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_AC1.jpg",{"$error":"#VALUE!"}]
[24,"Válvula seguridad oxígeno para regulador",76000000,25.31,8430133580223,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[25,"Válvula seguridad gas combustible para regulador",76200000,25.31,8430133580278,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[26,"Válvula seguridad oxígeno manguera Ø 6-8 mm.",77000000,25.31,8430133300494,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[27,"Válvula seguridad oxígeno manguera Ø 8-10 mm.",77000009,25.31,8430133334123,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[28,"Válvula seguridad gas combustible manguera Ø 6-9 mm.",77100008,25.31,8430133334161,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[29,"Válvula seguridad gas combustible manguera Ø 8-10 mm.",77100000,25.31,8430133300500,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[30,"Regulador EN 2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[31,"Regulador EN 2000 acetileno",37500000,133.13,8430133577797,"https://galagar.com/wp-content/uploads/2022/01/EN2000-AC.jpg",{"$error":"#VALUE!"}]
[32,"Pack 5 ud. boquillas de corte propano Nº 1 espesor 4-9 mm.","75600201P",49.71,8430133580643,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[33,"Pack 5 ud. boquillas de corte propano Nº 2 espesor 9-25 mm.","75600202P",49.71,8430133580650,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[34,"Pack 5 ud. boquillas de corte propano Nº 3 espesor 25-50 mm.","75600203P",49.71,8430133580667,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[35,"Pack 5 ud. boquillas de corte propano Nº 4 espesor 50-75 mm.","75600204P",49.71,8430133580674,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[36,"Pack 5 ud. boquillas de corte propano Nº 5 espesor 75-150 mm.","75600205P",49.71,8430133580681,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[37,"Pack 5 ud. boquillas de corte propano Nº 6 espesor 150-200 mm.","75600206P",49.71,8430133580698,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[38,"Pack 5 ud. boquillas de corte propano Nº 7 espesor 200-300 mm.","75600207P",49.71,8430133580704,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[39,"Dispositivo de corte oxígeno / propano",70100030,110.28,8430133305048,"https://galagar.com/wp-content/uploads/2022/01/Dispositivo-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[40,"Mango universal oxígeno / acetileno / propano",70200100,122.67,8430133579579,"https://galagar.com/wp-content/uploads/2022/01/MangoUniersal.jpg",{"$error":"#VALUE!"}]
[41,"Conjunto   5 m. manguera con racor universal para oxígeno / propano",78000805,67.150000000000006,8430133597467,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[42,"Conjunto 10 m. manguera con racor universal para oxígeno / propano",78000810,112.21,8430133597399,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[43,"Conjunto 15 m. manguera con racor universal para oxígeno / propano",78000815,159.47,8430133602451,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[44,"Válvula seguridad oxígeno para mango",73000000,22.99,8430133580032,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[45,"Válvula seguridad gas combustible para mango",73100020,22.99,8430133580094,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_AC1.jpg",{"$error":"#VALUE!"}]
[46,"Válvula seguridad oxígeno para regulador",76000000,25.31,8430133580223,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[47,"Válvula seguridad gas combustible para regulador",76200000,25.31,8430133580278,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[48,"Válvula seguridad oxígeno manguera Ø 6-8 mm.",77000000,25.31,8430133300494,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[49,"Válvula seguridad oxígeno manguera Ø 8-10 mm.",77000009,25.31,8430133334123,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[50,"Válvula seguridad gas combustible manguera Ø 6-9 mm.",77100008,25.31,8430133334161,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[51,"Válvula seguridad gas combustible manguera Ø 8-10 mm.",77100000,25.31,8430133300500,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[52,"Regulador EN 2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[53,"Regulador EN 2000 propano",37300000,133.13,8430133439330,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Prop.jpg",{"$error":"#VALUE!"}]
[54,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 1 espesor 4-9 mm.","71400201P",49.71,8430133580575,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[55,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 2 espesor 9-25 mm.","71400202P",49.71,8430133580582,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[56,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 3 espesor 25-50 mm","71400203P",49.71,8430133580599,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[57,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 4 espesor 50-75 mm.","71400204P",49.71,8430133580605,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[58,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 5 espesor 75-150 mm.","71400205P",49.71,8430133580612,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[59,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 6 espesor 150-200 mm.","71400206P",49.71,8430133580629,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[60,"Pack 5 ud. boquillas de corte Tipo H acetileno Nº 7 espesor 200-300 mm.","71400207P",49.71,8430133580636,"https://galagar.com/wp-content/uploads/2022/01/BoquillaCorte-TipoH.jpg",{"$error":"#VALUE!"}]
[61,"Soplete cortador para acetileno H-Optimus 90º 460 mm.",75800001,120.73,8430133426125,"https://galagar.com/wp-content/uploads/2022/07/Soplete-H-Op.jpg",{"$error":"#VALUE!"}]
[62,"Soplete cortador para acetileno H-Optimus 90º 1 metro",75801009,303.33,8430133601751,"https://galagar.com/wp-content/uploads/2022/07/Soplete-H-Op.jpg",{"$error":"#VALUE!"}]
[63,"Conjunto   5 m. manguera con racor universal para oxígeno / acetileno",78000705,63.01,8430133340971,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[64,"Conjunto 10 m. manguera con racor universal para oxígeno / acetileno",78000710,112.21,8430133340988,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[65,"Conjunto 15 m. manguera con racor universal para oxígeno / acetileno",78000715,143.84,8430133340995,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[66,"Válvula seguridad oxígeno para mango",73000000,22.99,8430133580032,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[67,"Válvula seguridad gas combustible para mango",73100020,22.99,8430133580094,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_AC1.jpg",{"$error":"#VALUE!"}]
[68,"Válvula seguridad oxígeno para regulador",76000000,25.31,8430133580223,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[69,"Válvula seguridad gas combustible para regulador",76200000,25.31,8430133580278,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[70,"Válvula seguridad oxígeno manguera Ø 6-8 mm.",77000000,25.31,8430133300494,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[71,"Válvula seguridad oxígeno manguera Ø 8-10 mm.",77000009,25.31,8430133334123,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[72,"Válvula seguridad gas combustible manguera Ø 6-9 mm.",77100008,25.31,8430133334161,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[73,"Válvula seguridad gas combustible manguera Ø 8-10 mm.",77100000,25.31,8430133300500,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[74,"Regulador EN 2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[75,"Regulador EN 2000 acetileno",37500000,133.13,8430133577797,"https://galagar.com/wp-content/uploads/2022/01/EN2000-AC.jpg",{"$error":"#VALUE!"}]
[76,"Pack 5 ud. boquillas de corte propano Nº 1 espesor 4-9 mm.","75600201P",49.71,8430133580643,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[77,"Pack 5 ud. boquillas de corte propano Nº 2 espesor 9-25 mm.","75600202P",49.71,8430133580650,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[78,"Pack 5 ud. boquillas de corte propano Nº 3 espesor 25-50 mm.","75600203P",49.71,8430133580667,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[79,"Pack 5 ud. boquillas de corte propano Nº 4 espesor 50-75 mm.","75600204P",49.71,8430133580674,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[80,"Pack 5 ud. boquillas de corte propano Nº 5 espesor 75-150 mm.","75600205P",49.71,8430133580681,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[81,"Pack 5 ud. boquillas de corte propano Nº 6 espesor 150-200 mm.","75600206P",49.71,8430133580698,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[82,"Pack 5 ud. boquillas de corte propano Nº 7 espesor 200-300 mm.","75600207P",49.71,8430133580704,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Corte-Prop.jpg",{"$error":"#VALUE!"}]
[83,"Soplete cortador para propano H-Optimus 90º 460 mm.",75800011,120.73,8430133551728,"https://galagar.com/wp-content/uploads/2022/07/Soplete-H-Op.jpg",{"$error":"#VALUE!"}]
[84,"Soplete cortador para propano H-Optimus 90º 1 metro",75801010,303.33,8430133580216,"https://galagar.com/wp-content/uploads/2022/07/Soplete-H-Op.jpg",{"$error":"#VALUE!"}]
[85,"Conjunto   5 m. manguera con racor universal para oxígeno / aceileno",78000805,67.150000000000006,8430133597467,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[86,"Conjunto 10 m. manguera con racor universal para oxígeno / propano",78000810,112.21,8430133597399,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[87,"Conjunto 15 m. manguera con racor universal para oxígeno / propano",78000815,159.47,8430133602451,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[88,"Válvula seguridad oxígeno para mango",73000000,22.99,8430133580032,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[89,"Válvula seguridad gas combustible para mango",73100020,22.99,8430133580094,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_AC1.jpg",{"$error":"#VALUE!"}]
[90,"Válvula seguridad oxígeno para regulador",76000000,25.31,8430133580223,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[91,"Válvula seguridad gas combustible para regulador",76200000,25.31,8430133580278,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[92,"Válvula seguridad oxígeno manguera Ø 6-8 mm.",77000000,25.31,8430133300494,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[93,"Válvula seguridad oxígeno manguera Ø 8-10 mm.",77000009,25.31,8430133334123,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[94,"Válvula seguridad gas combustible manguera Ø 6-9 mm.",77100008,25.31,8430133334161,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[95,"Válvula seguridad gas combustible manguera Ø 8-10 mm.",77100000,25.31,8430133300500,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[96,"Regulador EN 2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[97,"Regulador EN 2000 propano",37300000,133.13,8430133439330,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Prop.jpg",{"$error":"#VALUE!"}]
[98,"Pack 5 ud. boquillas de corte acetileno Nº 1 espesor 4-9 mm.","75510100P",63.92,8430133567774,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-AC.jpg",{"$error":"#VALUE!"}]
[99,"Pack 5 ud. boquillas de corte acetileno Nº 2 espesor 9-25 mm.","75510200P",63.92,8430133567767,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-AC.jpg",{"$error":"#VALUE!"}]
[100,"Pack 5 ud. boquillas de corte acetileno Nº 3 espesor 25-50 mm.","75510300P",63.92,8430133567781,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-AC.jpg",{"$error":"#VALUE!"}]
[101,"Pack 5 ud. boquillas de corte acetileno Nº 4 espesor 50-75 mm.","75510400P",63.92,8430133567798,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-AC.jpg",{"$error":"#VALUE!"}]
[102,"Pack 5 ud. boquillas de corte acetileno Nº 5 espesor 75-150 mm.","75510500P",63.92,8430133567804,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-AC.jpg",{"$error":"#VALUE!"}]
[103,"Pack 5 ud. boquillas de corte acetileno Nº 6 espesor 150-200 mm.","75510600P",63.92,8430133567811,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-MonoB_2.jpg",{"$error":"#VALUE!"}]
[104,"Pack 5 ud. boquillas de corte acetileno Nº 7 espesor 200-300 mm.","75510700P",63.92,8430133567828,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-AC.jpg",{"$error":"#VALUE!"}]
[105,"Pack 5 ud. boquillas de corte propano Nº 1 espesor 4-9 mm.","75501100P",63.92,8430133567835,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-Prop.jpg",{"$error":"#VALUE!"}]
[106,"Pack 5 ud. boquillas de corte propano Nº 2 espesor 9-25 mm.","75501200P",63.92,8430133567842,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-Prop.jpg",{"$error":"#VALUE!"}]
[107,"Pack 5 ud. boquillas de corte propano Nº 3 espesor 25-50 mm.","75501300P",63.92,8430133567859,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-MonoB_2.jpg",{"$error":"#VALUE!"}]
[108,"Pack 5 ud. boquillas de corte propano Nº 4 espesor 50-75 mm.","75501400P",63.92,8430133567866,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-Prop.jpg",{"$error":"#VALUE!"}]
[109,"Pack 5 ud. boquillas de corte propano Nº 5 espesor 75-150 mm.","75501500P",63.92,8430133567873,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-Prop.jpg",{"$error":"#VALUE!"}]
[110,"Pack 5 ud. boquillas de corte propano Nº 6 espesor 150-200 mm.","75501600P",63.92,8430133567880,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-Prop.jpg",{"$error":"#VALUE!"}]
[111,"Pack 5 ud. boquillas de corte propano Nº 7 espesor 200-300 mm.","75501700P",63.92,8430133567897,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-MonoB-Prop.jpg",{"$error":"#VALUE!"}]
[112,"Soplete Monoblock compacto 90º 460 mm. acetileno / propano",75500010,233.98,8430133301347,"https://galagar.com/wp-content/uploads/2022/01/Soplete-Monoblock.jpg",{"$error":"#VALUE!"}]
[113,"Conjunto  5 m. manguera M16x1,5 para acetileno",78000704,63.01,8430133801786,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[114,"Conjunto 10 m. manguera M16x1,5 para acetileno",78000712,112.21,8430133801793,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[115,"Conjunto 15 m. manguera M16x1,5 para acetileno",78000714,143.84,8430133801809,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[116,"Conjunto   5 m. manguera M16x1,5 para propano",78000804,67.150000000000006,8430133801861,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[117,"Conjunto 10 m. manguera M16x1,5 para propano",78000812,112.21,8430133801878,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[118,"Conjunto 15 m. manguera M16x1,5 para propano",78000814,159.47,8430133801885,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[119,"Válvula seguridad oxígeno M16x1,5 izda. para soplete",73100119,21.57,8430133615932]
[120,"Válvula seguridad combustible M16x1,5 dcha. para soplete",73000119,21.57,8430133615925,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[121,"Válvula seguridad oxígeno para regulador",76000000,25.31,8430133580223,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[122,"Válvula seguridad gas combustible para regulador",76200000,25.31,8430133580278,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[123,"Válvula seguridad oxígeno manguera Ø 6-8 mm.",77000000,25.31,8430133300494,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[124,"Válvula seguridad oxígeno manguera Ø 8-10 mm.",77000009,25.31,8430133334123,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[125,"Válvula seguridad gas combustible manguera Ø 6-9 mm.",77100008,25.31,8430133334161,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[126,"Válvula seguridad gas combustible manguera Ø 8-10 mm.",77100000,25.31,8430133300500,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[127,"Regulador EN 2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[128,"Regulador EN 2000 propano",37300000,133.13,8430133439330,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Prop.jpg",{"$error":"#VALUE!"}]
[129,"Regulador EN 2000 acetileno",37500000,133.13,8430133577797,"https://galagar.com/wp-content/uploads/2022/01/EN2000-AC.jpg",{"$error":"#VALUE!"}]
[130,"Boquilla para lanza de acetileno Nº 0 Consumo l/h. 75",70419001,9.81,8430133305369,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxAC.jpg",{"$error":"#VALUE!"}]
[131,"Boquilla para lanza de acetileno Nº 1 Consumo l/h. 150",70419101,10.46,8430133305376,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxAC.jpg",{"$error":"#VALUE!"}]
[132,"Boquilla para lanza de acetileno Nº 2 Consumo l/h. 300",70419201,12.52,8430133305383,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxAC.jpg",{"$error":"#VALUE!"}]
[133,"Boquilla para lanza de acetileno Nº 3 Consumo l/h. 500",70419301,13.18,8430133305390,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxAC.jpg",{"$error":"#VALUE!"}]
[134,"Boquilla para lanza de acetileno Nº 4 Consumo l/h. 750",70419401,17.690000000000001,8430133305406,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxAC.jpg",{"$error":"#VALUE!"}]
[135,"Boquilla para lanza de acetileno Nº 5 Consumo l/h. 1.200",70419501,22.21,8430133305413,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxAC.jpg",{"$error":"#VALUE!"}]
[136,"Boquilla para lanza de acetileno Nº 6 Consumo l/h. 1.700",70419601,23.63,8430133305420,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxAC.jpg",{"$error":"#VALUE!"}]
[137,"Boquilla para lanza de acetileno Nº 7 Consumo l/h. 2.500",70419701,24.79,8430133305437,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxAC.jpg",{"$error":"#VALUE!"}]
[138,"Boquilla para lanza de propano Nº 0 Consumo l/h. 75",70419005,14.08,8430133337698,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxProp.jpg",{"$error":"#VALUE!"}]
[139,"Boquilla para lanza de propano Nº 1 Consumo l/h. 150",70419105,14.72,8430133337704,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxProp.jpg",{"$error":"#VALUE!"}]
[140,"Boquilla para lanza de propano Nº 2 Consumo l/h. 300",70419205,16.79,8430133337711,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxProp.jpg",{"$error":"#VALUE!"}]
[141,"Boquilla para lanza de propano Nº 3 Consumo l/h. 500",70419305,17.43,8430133337735,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxProp.jpg",{"$error":"#VALUE!"}]
[142,"Boquilla para lanza de propano Nº 4 Consumo l/h. 750",70419405,21.95,8430133337766,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxProp.jpg",{"$error":"#VALUE!"}]
[143,"Boquilla para lanza de propano Nº 5 Consumo l/h. 1.200",70419505,19.36,8430133337780,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxProp.jpg",{"$error":"#VALUE!"}]
[144,"Boquilla para lanza de propano Nº 6 Consumo l/h. 1.700",70419605,27.89,8430133337803,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxProp.jpg",{"$error":"#VALUE!"}]
[145,"Boquilla para lanza de propano Nº 7 Consumo l/h. 2.500",70419705,29.05,8430133337810,"https://galagar.com/wp-content/uploads/2022/06/Boquilla-Sodar-OxProp.jpg",{"$error":"#VALUE!"}]
[146,"Lanza de acetileno Nº 0 Consumo l/h. 75",70400000,43.51,8430133579630,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[147,"Lanza de acetileno Nº 1 Consumo l/h. 150",70400100,47,8430133585402,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[148,"Lanza de acetileno Nº 2 Consumo l/h. 300",70400200,48.93,8430133579647,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[149,"Lanza de acetileno Nº 3 Consumo l/h. 500",70400300,51.26,8430133579654,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[150,"Lanza de acetileno Nº 4 Consumo l/h. 750",70400400,54.11,8430133579661,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[151,"Lanza de acetileno Nº 5 Consumo l/h. 1.200",70400500,65.459999999999994,8430133305338,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[152,"Lanza de acetileno Nº 6 Consumo l/h. 1.700",70400600,69.86,8430133305345,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[153,"Lanza de acetileno Nº 7 Consumo l/h. 2.500",70400700,77.349999999999994,8430133305352,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[154,"Lanza de propano Nº 0 Consumo l/h. 75",70400005,45.72,8430133585594,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[155,"Lanza de propano Nº 1 Consumo l/h. 150",70400105,48.81,8430133585600,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[156,"Lanza de propano Nº 2 Consumo l/h. 300",70400205,50.88,8430133585617,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[157,"Lanza de propano Nº 3 Consumo l/h. 500",70400305,55.79,8430133337421,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[158,"Lanza de propano Nº 4 Consumo l/h. 750",70400405,63.92,8430133337438,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[159,"Lanza de propano Nº 5 Consumo l/h. 1.200",70400505,64.819999999999993,8430133541316,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[160,"Lanza de propano Nº 6 Consumo l/h. 1.700",70400605,77.739999999999995,8430133337490,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[161,"Lanza de propano Nº 7 Consumo l/h. 2.500",70400705,87.03,8430133337506,"https://galagar.com/wp-content/uploads/2022/01/LanzaSoldar-Universal.jpg",{"$error":"#VALUE!"}]
[162,"Mango universal oxígeno / acetileno / propano",70200100,122.67,8430133579579,"https://galagar.com/wp-content/uploads/2022/01/MangoUniersal.jpg",{"$error":"#VALUE!"}]
[163,"Conjunto   5 m. manguera con racor universal para oxígeno / acetileno",78000705,63.01,8430133340971,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[164,"Conjunto 10 m. manguera con racor universal para oxígeno / acetileno",78000710,112.21,8430133340988,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[165,"Conjunto 15 m. manguera con racor universal para oxígeno / acetileno",78000715,143.84,8430133340995,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[166,"Conjunto   5 m. manguera con racor universal para oxígeno / propano",78000805,67.150000000000006,8430133597467,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[167,"Conjunto 10 m. manguera con racor universal para oxígeno / propano",78000810,112.21,8430133597399,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[168,"Conjunto 15 m. manguera con racor universal para oxígeno / propano",78000815,159.47,8430133602451,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[169,"Válvula seguridad oxígeno para mango",73000000,22.99,8430133580032,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[170,"Válvula seguridad gas combustible para mango",73100020,22.99,8430133580094,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_AC1.jpg",{"$error":"#VALUE!"}]
[171,"Válvula seguridad oxígeno para regulador",76000000,25.31,8430133580223,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[172,"Válvula seguridad gas combustible para regulador",76200000,25.31,8430133580278,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[173,"Válvula seguridad oxígeno manguera Ø 6-8 mm.",77000000,25.31,8430133300494,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[174,"Válvula seguridad oxígeno manguera Ø 8-10 mm.",77000009,25.31,8430133334123,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[175,"Válvula seguridad gas combustible manguera Ø 6-9 mm.",77100008,25.31,8430133334161,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[176,"Válvula seguridad gas combustible manguera Ø 8-10 mm.",77100000,25.31,8430133300500,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[177,"Regulador EN 2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[178,"Regulador EN 2000 acetileno",37500000,133.13,8430133577797,"https://galagar.com/wp-content/uploads/2022/01/EN2000-AC.jpg",{"$error":"#VALUE!"}]
[179,"Regulador EN 2000 propano",37300000,133.13,8430133439330,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Prop.jpg",{"$error":"#VALUE!"}]
[180,"Pack 5 ud. boquillas de soldar Minor Nº 1 de acetileno consumo 50 l/h.","10501117P",34.61,8430133541613,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[181,"Pack 5 ud. boquillas de soldar Minor Nº 2 de acetileno consumo 70 l/h.","10501217P",34.61,8430133585433,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[182,"Pack 5 ud. boquillas de soldar Minor Nº 3 de acetileno consumo 100 l/h.","10501317P",34.61,8430133585440,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[183,"Pack 5 ud. boquillas de soldar Minor Nº 4 de acetileno consumo 140 l/h.","10501417P",34.61,8430133585457,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[184,"Pack 5 ud. boquillas de soldar Minor Nº 5 de acetileno consumo 200 l/h.","10501517P",34.61,8430133585464,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[185,"Pack 5 ud. boquillas de soldar Minor Nº 6 de acetileno consumo 400 l/h.","10501617P",34.61,8430133585471,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[186,"Pack 5 ud. boquillas de soldar Minor Nº 1 de propano consumo 50 l/h.","10509124P",34.61,8430133585532,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[187,"Pack 5 ud. boquillas de soldar Minor Nº 2 de propano consumo 70 l/h.","10509224P",34.61,8430133585549,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[188,"Pack 5 ud. boquillas de soldar Minor Nº 3 de propano consumo 100 l/h.","10509324P",34.61,8430133585556,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[189,"Pack 5 ud. boquillas de soldar Minor Nº 4 de propano consumo 140 l/h.","10509424P",34.61,8430133585563,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[190,"Pack 5 ud. boquillas de soldar Minor Nº 5 de propano consumo 200 l/h.","10509524P",34.61,8430133585570,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[191,"Pack 5 ud. boquillas de soldar Minor Nº 6 de propano consumo 400 l/h.","10509624P",34.61,8430133585587,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Sodar-Minor.jpg",{"$error":"#VALUE!"}]
[192,"Lanza soplete soldador minor Oxígeno / acetileno / propano",10502015,30.47,8430133301231,"https://galagar.com/wp-content/uploads/2022/01/DispositivoCorte-Minor.jpg",{"$error":"#VALUE!"}]
[193,"Soplete soldador Minor Oxígeno / acetileno completo",10500000,71.02,8430133577223,"https://galagar.com/wp-content/uploads/2022/01/Conjunto-MInor-1.jpg",{"$error":"#VALUE!"}]
[194,"Soplete soldador Minor Oxígeno / propano completo",10500200,71.02,8430133302498,"https://galagar.com/wp-content/uploads/2022/01/Conjunto-MInor-1.jpg",{"$error":"#VALUE!"}]
[195,"Dispositivo de corte Minor para acetileno (sin boquillas)",10100160,161.41,8430133542351,"https://galagar.com/wp-content/uploads/2022/01/DispCorte-Minor.jpg",{"$error":"#VALUE!"}]
[196,"Dispositivo de corte Minor para propano (sin boquillas)",10500160,161.41,8430133898304,"https://galagar.com/wp-content/uploads/2022/01/DispCorte-Minor.jpg",{"$error":"#VALUE!"}]
[197,"Boquilla de corte Minor para acetileno Nº 1 Espesor de 3 a 15 mm.",70600501,38.35,8430133300067,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Cortar-Minor.jpg",{"$error":"#VALUE!"}]
[198,"Boquilla de corte Minor para acetileno Nº 2 Espesor de 15 a 25 mm.",70600502,38.35,8430133300074,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Cortar-Minor.jpg",{"$error":"#VALUE!"}]
[199,"Boquilla de corte Minor para acetileno Nº 3 Espesor de 25 a 50 mm.",70600503,38.35,8430133300081,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Cortar-Minor.jpg",{"$error":"#VALUE!"}]
[200,"Boquilla de corte Minor para propano Nº 1 Espesor de 3 a 15 mm.",70600511,38.35,8430133300098,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Cortar-Minor.jpg",{"$error":"#VALUE!"}]
[201,"Boquilla de corte Minor para propano Nº 2 Espesor de 15 a 25 mm.",70600512,38.35,8430133300104,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Cortar-Minor.jpg",{"$error":"#VALUE!"}]
[202,"Boquilla de corte Minor para propano Nº 3 Espesor de 25 a 50 mm.",70600513,38.35,8430133300111,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Cortar-Minor.jpg",{"$error":"#VALUE!"}]
[203,"Conjunto   5 m. manguera Ø 6 + 6 x 12 mm. acetileno / propano",78000605,63.01,8430133952532,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[204,"Conjunto 10 m. manguera Ø 6 + 6 x 12 mm. acetileno / propano",78000610,112.21,8430133611149,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[205,"Conjunto 15 m. manguera Ø 6 + 6 x 12 mm. acetileno / propano",78000615,143.84,8430133611163,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[206,"Válvula seguridad oxígeno para mango",73000000,22.99,8430133580032,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[207,"Válvula seguridad gas combustible para mango",73100020,22.99,8430133580094,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_AC1.jpg",{"$error":"#VALUE!"}]
[208,"Válvula seguridad oxígeno para regulador",76000000,25.31,8430133580223,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[209,"Válvula seguridad gas combustible para regulador",76200000,25.31,8430133580278,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[210,"Válvula seguridad oxígeno manguera Ø 6-8 mm.",77000000,25.31,8430133300494,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[211,"Válvula seguridad oxígeno manguera Ø 8-10 mm.",77000009,25.31,8430133334123,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[212,"Válvula seguridad gas combustible manguera Ø 6-9 mm.",77100008,25.31,8430133334161,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[213,"Válvula seguridad gas combustible manguera Ø 8-10 mm.",77100000,25.31,8430133300500,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[214,"Regulador EN 2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[215,"Regulador EN 2000 actileno",37500000,133.13,8430133577797,"https://galagar.com/wp-content/uploads/2022/01/EN2000-AC.jpg",{"$error":"#VALUE!"}]
[216,"Regulador EN 2000 propano",37300000,133.13,8430133439330,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Prop.jpg",{"$error":"#VALUE!"}]
[217,"Boquilla calentamiento acetileno Nº 1 consumo l/h 3.700",72419501,38.35,8430133302269,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Calentar-Prop.jpg"]
[218,"Boquilla calentamiento acetileno Nº 2 consumo l/h 4.600",72419502,38.35,8430133579982]
[219,"Boquilla calentamiento propano Nº 1 - S-150 consumo l/h 3.700",72419511,38.35,8430133302283]
[220,"Boquilla calentamiento propano Nº 2 - S-150 consumo l/h 4.600",72419512,38.35,8430133302290,null,{"$error":"#VALUE!"}]
[221,"Boquilla calentamiento NG Nº 2 consumo l/h 1.830",75500200,52.3,8430133302351,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Calentar-NG-2.jpg",{"$error":"#VALUE!"}]
[222,"Boquilla calentamiento NG Nº 3 consumo l/h 3.600",75500300,62.37,8430133302368,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Calentar-NG-2.jpg",{"$error":"#VALUE!"}]
[223,"Boquilla calentamiento NG Nº 4 consumo l/h 4.050",75500400,83.94,8430133302375,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Calentar-NG-2.jpg",{"$error":"#VALUE!"}]
[224,"Boquilla calentamiento NG Nº 5 consumo l/h 4.800",75500500,87.81,8430133655068,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Calentar-NG-2.jpg",{"$error":"#VALUE!"}]
[225,"Lanza calentamiento acetileno/propano 400 mm.",72400400,52.56,8430133579975,"https://galagar.com/wp-content/uploads/2022/01/LanzaCalentar-Universal.jpg",{"$error":"#VALUE!"}]
[226,"Lanza calentamiento acetileno/propano 700 mm.",72400700,84.84,8430133305475,"https://galagar.com/wp-content/uploads/2022/01/LanzaCalentar-Universal.jpg",{"$error":"#VALUE!"}]
[227,"Lanza calentamiento NG 260 mm. propano",75500020,81.349999999999994,8430133302313,"https://galagar.com/wp-content/uploads/2022/01/LanzaCalentar-NG.jpg",{"$error":"#VALUE!"}]
[228,"Lanza calentamiento NG 400 mm. propano",75500040,92.97,8430133302320,"https://galagar.com/wp-content/uploads/2022/01/LanzaCalentar-NG.jpg",{"$error":"#VALUE!"}]
[229,"Lanza calentamiento NG 700 mm. propano",75500070,102.01,8430133302337,"https://galagar.com/wp-content/uploads/2022/01/LanzaCalentar-NG.jpg",{"$error":"#VALUE!"}]
[230,"Lanza calentamiento NG 900 mm. propano",75500090,109.76,8430133302344,"https://galagar.com/wp-content/uploads/2022/01/LanzaCalentar-NG.jpg",{"$error":"#VALUE!"}]
[231,"Mango universal oxígeno / acetileno / propano",70200100,122.67,8430133579579,"https://galagar.com/wp-content/uploads/2022/01/MangoUniersal.jpg",{"$error":"#VALUE!"}]
[232,"Conjunto   5 m. manguera con racor universal para oxígeno / acetileno",78000705,63.01,8430133340971,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[233,"Conjunto 10 m. manguera con racor universal para oxígeno / acetileno",78000710,112.21,8430133340988,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[234,"Conjunto 15 m. manguera con racor universal para oxígeno / acetileno",78000715,143.84,8430133340995,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[235,"Conjunto   5 m. manguera con racor universal para oxígeno / propano",78000805,67.150000000000006,8430133597467,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[236,"Conjunto 10 m. manguera con racor universal para oxígeno / propano",78000810,112.21,8430133597399,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[237,"Conjunto 15 m. manguera con racor universal para oxígeno / propano",78000815,159.47,8430133602451,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[238,"Válvula seguridad oxígeno para mango",73000000,22.99,8430133580032,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[239,"Válvula seguridad gas combustible para mango",73100020,22.99,8430133580094,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_AC1.jpg",{"$error":"#VALUE!"}]
[240,"Válvula seguridad oxígeno para regulador",76000000,25.31,8430133580223,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[241,"Válvula seguridad gas combustible para regulador",76200000,25.31,8430133580278,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[242,"Válvula seguridad oxígeno manguera Ø 6-8 mm.",77000000,25.31,8430133300494,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[243,"Válvula seguridad oxígeno manguera Ø 8-10 mm.",77000009,25.31,8430133334123,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[244,"Válvula seguridad gas combustible manguera Ø 6-9 mm.",77100008,25.31,8430133334161,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[245,"Válvula seguridad gas combustible manguera Ø 8-10 mm.",77100000,25.31,8430133300500,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[246,"Regulador EN 2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[247,"Regulador EN 2000 acetileno",37500000,133.13,8430133577797,"https://galagar.com/wp-content/uploads/2022/01/EN2000-AC.jpg",{"$error":"#VALUE!"}]
[248,"Regulador EN 2000 propano",37300000,133.13,8430133439330,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Prop.jpg",{"$error":"#VALUE!"}]
[249,"KIT Universal 300 - Conjunto soplete modular con accesorios de soldadura y corte",10300440,920.94,8430133639341,"https://galagar.com/wp-content/uploads/2024/02/Meletin-Conjunto.jpg",{"$error":"#VALUE!"}]
[250,"KIT Universal Corte - Conjunto de soplete + dispositivo de corte hasta 25 mm.",10400310,304.61,8430133638917,"https://galagar.com/wp-content/uploads/2022/01/Caja-KIT-Univ.jpg",{"$error":"#VALUE!"}]
[251,"KIT Tipo-H - Conjunto soplete modular soldadura/corte, boquillas de asiento plano",70300750,557.45000000000005,8430133634353,"https://galagar.com/wp-content/uploads/2022/01/Maletin-KITs.jpg",{"$error":"#VALUE!"}]
[252,"KIT Caribe - Conjunto soplete modular soldadura/corte, boquillas de asiento cónico",70300600,1136.72,8430133333430,"https://galagar.com/wp-content/uploads/2022/01/Maletin-KITs.jpg",{"$error":"#VALUE!"}]
[253,"Válvula seguridad oxígeno para soplete Monoblock",73000119,21.57,8430133615925,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg"]
[254,"Válvula seguridad gas combustible para soplete Monoblock",73100119,21.57,8430133615932,null,{"$error":"#VALUE!"}]
[255,"Válvula seguridad oxígeno Soplete Tipo-H",73000010,21.57,8430133580049,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[256,"Válvula seguridad gas combustible Soplete Tipo-H",73100010,21.57,8430133580087,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_AC1.jpg",{"$error":"#VALUE!"}]
[257,"Válvula seguridad oxígeno Mango Universal",73000000,22.99,8430133580032,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_OX1.jpg",{"$error":"#VALUE!"}]
[258,"Válvula seguridad gas combustible Mango Universal",73100020,22.99,8430133580094,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Mango_AC1.jpg",{"$error":"#VALUE!"}]
[259,"Válvula seguridad regulador oxígeno",76000000,25.31,8430133580223,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[260,"Válvula seguridad regulador gas combustible",76200000,25.31,8430133580278,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[261,"Válvula regulador oxígeno Tipo-H",76000009,25.39,8430133333980,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[262,"Válvula regulador gas combustible Tipo-H",76100009,25.39,8430133580254,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[263,"Válvula regulador oxígeno Ø 8-10",76000119,29.83,8430133670771,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_OX1.jpg",{"$error":"#VALUE!"}]
[264,"Válvula regulador gas combustible Ø 8-10",76200119,29.83,8430133670788,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Regulador_AC1.jpg",{"$error":"#VALUE!"}]
[265,"Válvula manguera oxígeno Ø 6-8 mm.",77000000,25.31,8430133300494,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[266,"Válvula manguera oxígeno Ø 8-10 mm.",77000009,25.31,8430133334123,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_OX1.jpg",{"$error":"#VALUE!"}]
[267,"Válvula manguera gas combustible Ø 6-9 mm.",77100008,25.31,8430133334161,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[268,"Válvula manguera gas combustible Ø 8-10 mm.",77100000,25.31,8430133300500,"https://galagar.com/wp-content/uploads/2023/06/Valvula-Manguera_AC1.jpg",{"$error":"#VALUE!"}]
[269,"Clavija enchufe rápido oxígeno 8 mm.",81000214,14.33,8430133634094,"https://galagar.com/wp-content/uploads/2022/02/Conexiones-Rapidas-NEW.jpg",{"$error":"#VALUE!"}]
[270,"Cuerpo enchufe rápido oxígeno 8 mm. G1/4” RH",81000314,26.04,8430133634070,"https://galagar.com/wp-content/uploads/2022/02/Conexiones-Rapidas-NEW.jpg",{"$error":"#VALUE!"}]
[271,"Clavija enchufe rápido gas combustible",81000238,14.33,8430133634100,"https://galagar.com/wp-content/uploads/2022/02/Conexiones-Rapidas-NEW.jpg",{"$error":"#VALUE!"}]
[272,"Cuerpo enchufe rápido gas combustible  G3/8” LH",81000338,24.79,8430133634087,"https://galagar.com/wp-content/uploads/2022/02/Conexiones-Rapidas-NEW.jpg",{"$error":"#VALUE!"}]
[273,"Clavija enchufe rápido oxígeno G1/4” RH",81000514,20.02,8430133665012,"https://galagar.com/wp-content/uploads/2022/02/Conexiones-Rapidas-NEW.jpg",{"$error":"#VALUE!"}]
[274,"Cuerpo enchufe rápido oxígeno 8 mm.",81000414,33.450000000000003,8430133664992,"https://galagar.com/wp-content/uploads/2022/02/Conexiones-Rapidas-NEW.jpg",{"$error":"#VALUE!"}]
[275,"Clavija enchufe rápido gas combustible G3/8” LH",81000538,20.02,8430133665029,"https://galagar.com/wp-content/uploads/2022/02/Conexiones-Rapidas-NEW.jpg",{"$error":"#VALUE!"}]
[276,"Cuerpo enchufe rápido gas combustible 8 mm.",81000438,33.450000000000003,8430133665005,"https://galagar.com/wp-content/uploads/2022/02/Conexiones-Rapidas-NEW.jpg",{"$error":"#VALUE!"}]
[277,"Manguera simple rollos de 100 m. oxígeno (Ø int/ext. 8 x 15)",77200000,4.78,8430133300517,"https://galagar.com/wp-content/uploads/2022/01/Manguera-Simple_OX.jpg",{"$error":"#VALUE!"}]
[278,"Manguera simple rollos de 100 m. acetileno (Ø int/ext. 8 x 15)",77300000,4.78,8430133300524,"https://galagar.com/wp-content/uploads/2022/01/Manguera-Simple_AC.jpg",{"$error":"#VALUE!"}]
[279,"Manguera simple rollos de 100 m. propano (Ø int/ext. 9 x 16)",77400000,4.78,8430133338947,"https://galagar.com/wp-content/uploads/2022/01/Manguera-Simple_Prop.jpg",{"$error":"#VALUE!"}]
[280,"Doble manguera rollos de 100 m. oxígeno - acetileno/propano (Ø int/ext. 8+8 x 15)",77500000,7.49,8430133300531,"https://galagar.com/wp-content/uploads/2022/02/MangueraRollo100m.jpg",{"$error":"#VALUE!"}]
[281,"Doble manguera rollos de 100 m. oxígeno - acetileno (Ø int/ext. 8+8 x 15)",77600000,7.49,8430133300548,"https://galagar.com/wp-content/uploads/2022/02/MangueraRollo100m.jpg",{"$error":"#VALUE!"}]
[282,"Doble manguera rollos de 100 m. oxígeno - propano (Ø int/ext. 8+8 x 15)",77900000,7.49,8430133566685,"https://galagar.com/wp-content/uploads/2022/02/MangueraRollo100m.jpg",{"$error":"#VALUE!"}]
[283,"Doble manguera rácores universales   5 m. Oxígeno / Actileno",78000705,63.01,8430133340971,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[284,"Doble manguera rácores universales 10 m. Oxígeno / Actileno",78000710,112.21,8430133340988,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[285,"Doble manguera rácores universales 15 m. Oxígeno / Actileno",78000715,143.84,8430133340995,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[286,"Doble manguera rácores universales   5 m. Oxígeno / Propano",78000805,67.150000000000006,8430133597467,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[287,"Doble manguera rácores universales 10 m. Oxígeno / Propano",78000810,112.21,8430133597399,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[288,"Doble manguera rácores universales 15 m. Oxígeno / Propano",78000815,159.47,8430133602451,"https://galagar.com/wp-content/uploads/2022/01/MangueraDoble-Racores-P.jpg",{"$error":"#VALUE!"}]
[289,"Alargadera desmontable oxígeno",72000000,16.39,8430133300326,"https://galagar.com/wp-content/uploads/2022/01/Alargaderas.jpg",{"$error":"#VALUE!"}]
[290,"Alargadera desmontable acetileno",72100005,17.05,8430133541187,"https://galagar.com/wp-content/uploads/2022/01/Alargaderas.jpg",{"$error":"#VALUE!"}]
[291,"Alargadera fija oxígeno Ø 6-8",72400000,16.39,8430133300340,"https://galagar.com/wp-content/uploads/2022/01/Alargaderas.jpg",{"$error":"#VALUE!"}]
[292,"Alargadera fija acetileno / propano Ø 8-10",72500000,17.05,8430133300357,"https://galagar.com/wp-content/uploads/2022/01/Alargaderas.jpg",{"$error":"#VALUE!"}]
[293,"Caja de escariadores",88888810,13.78,8430133569204]
[294,"Mechero cazoleta",200041,6.9,8430133610425]
[295,"Piedra mechero",200042,1.5,8430133637798]
[296,"Carro cortador con anillo",75600315,34,8430133920937]
[297,"Grupo autónomo GAP-OB (Oxígeno-Butano)",78000068,"CONSULTAR",8430133639068,"https://galagar.com/wp-content/uploads/2022/02/GAP-78000068.jpg",{"$error":"#VALUE!"}]
[298,"Soplete soldador Minor con SET de boquillas",10500200,71.02,8430133302498,"https://galagar.com/wp-content/uploads/2022/01/Conjunto-MInor-1.jpg",{"$error":"#VALUE!"}]
[299,"Conjunto de 3 m. de manguera Ø 6 + 6x12 mm.",78000603,67.150000000000006,8430133341671]
[300,"Regulador Gasweld oxígeno",30500001,109.53,8430133650780,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[301,"GAP-OB sin botellas",78000460,295.45,8430133301897,"https://galagar.com/wp-content/uploads/2022/01/GAP-Carro-SinBotellas.jpg",{"$error":"#VALUE!"}]
[302,"Cortador Minor propano sin boquillas",10500160,161.41,8430133898304,"https://galagar.com/wp-content/uploads/2022/01/DispCorte-Minor.jpg",{"$error":"#VALUE!"}]
[303,"Boquilla corte agil propano Nº 2",70600512,38.35,8430133300104,"https://galagar.com/wp-content/uploads/2022/01/Boquilla-Cortar-Minor.jpg",{"$error":"#VALUE!"}]
[304,"Carro Grupo Autónomo GAP OB",71500100,127.83,8430133579821,"https://galagar.com/wp-content/uploads/2022/01/GAP-Carro.jpg",{"$error":"#VALUE!"}]
[305,"Botella oxigeno 5 litros llena",91000006,"CONSULTAR",8430133605971]
[306,"Botella propano 2,8 kg. llena",91000027,"CONSULTAR",8430133302030,"https://galagar.com/wp-content/uploads/2022/02/Botella_campingaz_907.jpg",{"$error":"#VALUE!"}]
[307,"Botella chemtane 3 kg. llena",91000004,"CONSULTAR",8430133776268,"https://galagar.com/wp-content/uploads/2022/02/Botella_campingaz_907.jpg",{"$error":"#VALUE!"}]
[308,"Carga botella oxígeno",91000115,"CONSULTAR",8430133549398]
[309,"Carga botella propano 2,8 kg.",91000127,"CONSULTAR",8430133923938]
[310,"Carga botella chemtane 3 kg.",91000104,"CONSULTAR",8430133776275]
[311,"Grupo autónomo GAP O lanza térmica",78000038,"CONSULTAR",8430133786144,"https://galagar.com/wp-content/uploads/2022/01/GAP-O-LanzaTermica.jpg",{"$error":"#VALUE!"}]
[312,"Botella oxígeno 5 litros llena",91000006,"CONSULTAR",8430133605971]
[313,"Porta lanza térmica",13000050,272.08,8430133785017]
[314,"Tubo goma oxígeno",77200000,4.78,8430133300517,"https://galagar.com/wp-content/uploads/2022/01/Manguera-Simple_OX.jpg",{"$error":"#VALUE!"}]
[315,"Regulador EN 2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[316,"Carro grupo autónomo oxígeno + lanza térmica",71500138,161.41,8430133804053]
[317,"Batería 12 V 44 AH 360 Amp.",13020001,216.94,8430133786151]
[318,"Lanza térmica Ø 10x1000 mm. (consumible)",13010100,36.93,8430133798154,"https://galagar.com/wp-content/uploads/2022/01/Varillas-LanzaTermica.jpg",{"$error":"#VALUE!"}]
[319,"Boquilla soldadura fuerte Propano N.4",14600534,27.76,8430133200046,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[320,"Boquilla soldadura fuerte Propano N.5",14600535,28.02,8430133200053,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[321,"Boquilla soldadura fuerte Propano N.6",14600536,28.93,8430133200060,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[322,"Boquilla soldadura fuerte Propano N.7",14600537,29.95,8430133200077,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[323,"Boquilla soldadura fuerte Propano N.8",14600538,53.72,8430133200084,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[324,"Boquilla calentamiento 50 mm.",73400530,30.47,8430133200213,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Calent.jpg",{"$error":"#VALUE!"}]
[325,"Boquilla calentamiento 60 mm.",73400630,30.47,8430133200220,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Calent.jpg",{"$error":"#VALUE!"}]
[326,"Boquilla calentamiento 70 mm.",73400730,31.51,8430133200237,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Calent.jpg",{"$error":"#VALUE!"}]
[327,"Boquilla calentamiento 80 mm.",73400830,32.659999999999997,8430133200244,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Calent.jpg",{"$error":"#VALUE!"}]
[328,"Lanza corta 50 mm. soldadura fuerte",14600330,27.89,8430133200138,"https://galagar.com/wp-content/uploads/2022/01/Blister-Lanzas-Aerob.jpg",{"$error":"#VALUE!"}]
[329,"Lanza larga 200 mm. soldadura fuerte",14600430,29.7,8430133200145,"https://galagar.com/wp-content/uploads/2022/01/Blister-Lanzas-Aerob.jpg",{"$error":"#VALUE!"}]
[330,"Lanza calentamiento 330 mm.",73400130,29.95,8430133200114,"https://galagar.com/wp-content/uploads/2022/01/Blister-Lanzas-Aerob.jpg",{"$error":"#VALUE!"}]
[331,"Lanza calentamiento 500 mm.",73400230,31.76,8430133200121,"https://galagar.com/wp-content/uploads/2022/01/Blister-Lanzas-Aerob.jpg",{"$error":"#VALUE!"}]
[332,"Mango aerobutánico Gala PLUS con economizador (¡Nuevo!)",14600275,30,8430133841058,"https://galagar.com/wp-content/uploads/2024/07/Mango-AeroB-ECO-2025.jpg",{"$error":"#VALUE!"}]
[333,"Mango aerobutánico Gala PLUS sin economizador (¡Nuevo!)",14600175,26,8430133841041,"https://galagar.com/wp-content/uploads/2024/07/Mango-AeroB-SIN-2025.jpg",{"$error":"#VALUE!"}]
[334,"Conjunto tuerca y racor para mango aerobutánico",14600126,13.04,8430133603854,"https://galagar.com/wp-content/uploads/2022/01/Blister-Mangos-Aerob.jpg",{"$error":"#VALUE!"}]
[335,"Rastrillo 2 boquillas chamuscador",73400321,45.97,8430133338466,"https://galagar.com/wp-content/uploads/2022/01/Rastrillos.jpg",{"$error":"#VALUE!"}]
[336,"Rastrillo 4 boquillas chamuscador",73400340,127.83,8430133338480,"https://galagar.com/wp-content/uploads/2022/01/Rastrillos.jpg",{"$error":"#VALUE!"}]
[337,"Lira blindada 8x14 de 2,5 m.",72500230,38.35,8430133200411,"https://galagar.com/wp-content/uploads/2022/01/Blister-Liras.jpg",{"$error":"#VALUE!"}]
[338,"Lira blindada 5x10,5 de 2,5 m.",72500130,38.35,8430133200404,"https://galagar.com/wp-content/uploads/2022/01/Blister-Liras.jpg",{"$error":"#VALUE!"}]
[339,"Lira sin blindar 6x12 - 2,5 m.",72500330,38.35,8430133200428,"https://galagar.com/wp-content/uploads/2022/01/Blister-Liras.jpg",{"$error":"#VALUE!"}]
[340,"Grifo escape libre sin racor",73200203,22.73,8430133200251,"https://galagar.com/wp-content/uploads/2022/01/Grifo-Aerob.jpg",{"$error":"#VALUE!"}]
[341,"Tuerca-racor escape libre",73211116,11.36,8430133200312,"https://galagar.com/wp-content/uploads/2022/01/Racor-Grifo-Aerob.jpg",{"$error":"#VALUE!"}]
[342,"Botella propano 2,8 kg. llena",91000027,"CONSULTAR",8430133302030,"https://galagar.com/wp-content/uploads/2022/02/Botella_campingaz_907.jpg",{"$error":"#VALUE!"}]
[343,"Botella chemtane 3 kg. llena",91000004,"CONSULTAR",8430133776268,"https://galagar.com/wp-content/uploads/2022/02/Botella_campingaz_907.jpg",{"$error":"#VALUE!"}]
[344,"Lanza de 350 mm. para chamuscador",14600420,35.380000000000003,8430133336424,"https://galagar.com/wp-content/uploads/2022/01/Lanza500mm.jpg",{"$error":"#VALUE!"}]
[345,"Lanza soldadura fuerte propano 600 mm.",14600460,42.09,8430133336431,"https://galagar.com/wp-content/uploads/2022/01/Lanza500mm.jpg",{"$error":"#VALUE!"}]
[346,"Soplete Turbo Gala PRO 3 (¡Nuevo!)",15100600,57,8430133835903,"https://galagar.com/wp-content/uploads/2024/07/SopleteTurboGala_1.jpg",{"$error":"#VALUE!"}]
[347,"Soplete Aerogala Eco",15100000,31.25,8430133931889,"https://galagar.com/wp-content/uploads/2022/02/SopleteAerogala.jpg",{"$error":"#VALUE!"}]
[348,"Estuche Aerogala gas propano",15100350,"CONSULTAR",8430133577261,"https://galagar.com/wp-content/uploads/2022/02/Maletin-Chemtane.jpg",{"$error":"#VALUE!"}]
[349,"Estuche Aerogala gas chemtane",15100450,"CONSULTAR",8430133777968,"https://galagar.com/wp-content/uploads/2022/02/Maletin-Aerogala.jpg",{"$error":"#VALUE!"}]
[350,"Cartucho soplete Aerogala gas propano",15100300,"CONSULTAR",8430133541583,"https://galagar.com/wp-content/uploads/2022/02/CartuchoDesechable-Propano-1.jpg",{"$error":"#VALUE!"}]
[351,"Cartucho soplete Aerogala gas chemtane",15100400,"CONSULTAR",8430133777951,"https://galagar.com/wp-content/uploads/2022/01/GasChemtane.jpg",{"$error":"#VALUE!"}]
[352,"KIT aerogala con botella",15100150,"CONSULTAR",8430133673413,"https://galagar.com/wp-content/uploads/2022/01/Blister-Soplete-Autonomo.jpg",{"$error":"#VALUE!"}]
[353,"Boquilla soldadura fuerte propano Nº 4",14600534,27.76,8430133200046,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[354,"Boquilla soldadura fuerte propano Nº 5",14600535,28.02,8430133200053,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[355,"Boquilla soldadura fuerte propano Nº 6",14600536,28.93,8430133200060,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[356,"Boquilla soldadura fuerte propano Nº 7",14600537,29.95,8430133200077,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[357,"Boquilla soldadura fuerte propano Nº 8",14600538,53.72,8430133200084,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[358,"Boquilla calentamiento Ø 50 mm.",73400530,30.47,8430133200213,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Calent.jpg",{"$error":"#VALUE!"}]
[359,"Boquilla calentamiento Ø 60 mm.",73400630,30.47,8430133200220,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Calent.jpg",{"$error":"#VALUE!"}]
[360,"Boquilla calentamiento Ø 70 mm.",73400730,31.51,8430133200237,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Calent.jpg",{"$error":"#VALUE!"}]
[361,"Boquilla calentamiento Ø 80 mm.",73400830,32.659999999999997,8430133200244,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Calent.jpg",{"$error":"#VALUE!"}]
[362,"Lanza corta soldura fuerte",14600330,27.89,8430133200138,"https://galagar.com/wp-content/uploads/2022/01/Blister-Lanzas-Aerob.jpg",{"$error":"#VALUE!"}]
[363,"Lanza larga soldura fuerte",14600430,29.7,8430133200145,"https://galagar.com/wp-content/uploads/2022/01/Blister-Lanzas-Aerob.jpg",{"$error":"#VALUE!"}]
[364,"Soplete chamuscador Plus (¡Nuevo!)",14800200,45,8430133835897,"https://galagar.com/wp-content/uploads/2024/07/Chanuscador_New_3.jpg",{"$error":"#VALUE!"}]
[365,"Grifo escape libre sin racor",73200203,22.73,8430133200251,"https://galagar.com/wp-content/uploads/2022/01/Grifo-Aerob.jpg",{"$error":"#VALUE!"}]
[366,"Mango aerobutánico Gala PLUS sin economizador (¡Nuevo!)",14600175,26,8430133841041,"https://galagar.com/wp-content/uploads/2024/07/Mango-AeroB-ECO-2025.jpg",{"$error":"#VALUE!"}]
[367,"Mango aerobutánico Gala PLUS con economizador (¡Nuevo!)",14600275,30,8430133841058,"https://galagar.com/wp-content/uploads/2024/07/Mango-AeroB-SIN-2025.jpg",{"$error":"#VALUE!"}]
[368,"Lira blindada 8x14 de 2,5 m.",72500230,38.35,8430133200411,"https://galagar.com/wp-content/uploads/2022/01/Blister-Liras.jpg",{"$error":"#VALUE!"}]
[369,"Lira sin blindar 6x12 2,5 m.",72500330,38.35,8430133200428,"https://galagar.com/wp-content/uploads/2022/01/Blister-Liras.jpg",{"$error":"#VALUE!"}]
[370,"Lira blindada 5x10,5 de 2,5 m.",72500130,38.35,8430133200404,"https://galagar.com/wp-content/uploads/2022/01/Blister-Liras.jpg",{"$error":"#VALUE!"}]
[371,"Conjunto instalador Nº 1 - Para fontanero pintor y bricolaje",15000030,35.51,8430133200152,"https://galagar.com/wp-content/uploads/2022/01/Conjunto-Instalador_1.jpg",{"$error":"#VALUE!"}]
[372,"Conjunto instalador Nº 2 - Para fontanero pintor y bricolaje",14600203,103.04,8430133302658,"https://galagar.com/wp-content/uploads/2022/01/Conjunto-Instalador_2.jpg",{"$error":"#VALUE!"}]
[373,"Mango aerobutánico Gala PLUS con economizador",14600275,20.86,8430133841058,"https://galagar.com/wp-content/uploads/2024/07/Mango-AeroB-ECO-2025.jpg",{"$error":"#VALUE!"}]
[374,"Lanza larga de soldadura",14600430,29.7,8430133200145,"https://galagar.com/wp-content/uploads/2022/01/Blister-Lanzas-Aerob.jpg",{"$error":"#VALUE!"}]
[375,"Boquilla para solsadura de propano Nº 5",14600535,28.02,8430133200053,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[376,"Boquilla para solsadura de propano Nº 6",14600536,28.93,8430133200060,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[377,"Boquilla para solsadura de propano Nº 7",14600537,29.95,8430133200077,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[378,"Lira sin blindar 6x12 2,5 m.",72500330,38.35,8430133200428,"https://galagar.com/wp-content/uploads/2022/01/Blister-Liras.jpg",{"$error":"#VALUE!"}]
[379,"Conjunto instalador Nº 4 - Para fontanero pintor y bricolaje",14600602,76.040000000000006,8430133302818,"https://galagar.com/wp-content/uploads/2022/01/Conjunto-Instalador_4.jpg",{"$error":"#VALUE!"}]
[380,"Mango aerobutánico Gala PLUS sin economizador",14600175,26,8430133841041,"https://galagar.com/wp-content/uploads/2024/07/Mango-AeroB-SIN-2025.jpg",{"$error":"#VALUE!"}]
[381,"Lanza corta de soldadura",14600330,27.89,8430133200138,"https://galagar.com/wp-content/uploads/2022/01/Blister-Lanzas-Aerob.jpg",{"$error":"#VALUE!"}]
[382,"Grifo escape libre sin racor",73200203,22.73,8430133200251,"https://galagar.com/wp-content/uploads/2022/01/Grifo-Aerob.jpg",{"$error":"#VALUE!"}]
[383,"Boquilla soldadura propano Nº 4",14600534,27.76,8430133200046,"https://galagar.com/wp-content/uploads/2022/01/Blister-Boquillas-Aerob-Fuerte.jpg",{"$error":"#VALUE!"}]
[384,"Lira sin blindar 6x12 1,5 m.",72500335,31.69,8430133338091,"https://galagar.com/wp-content/uploads/2022/01/Blister-Liras.jpg",{"$error":"#VALUE!"}]
[385,"Regulador EN-2000 oxígeno",37000000,133.13,8430133577711,"https://galagar.com/wp-content/uploads/2022/01/EN2000-OX.jpg",{"$error":"#VALUE!"}]
[386,"Regulador EN-2000 acetileno",37500000,133.13,8430133577797,"https://galagar.com/wp-content/uploads/2022/01/EN2000-AC.jpg",{"$error":"#VALUE!"}]
[387,"Regulador EN-2000 acetileno acoplamiento con brida",37500004,167.18,8430133333188,"https://galagar.com/wp-content/uploads/2022/01/EN2000-AC.jpg",{"$error":"#VALUE!"}]
[388,"Regulador EN-2000 argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[389,"Regulador EN-2000 argón-Co2 con rotámetro",37600500,155.62,8430133577919,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[390,"Regulador EN-2000 nitrógeno con rotámetro",37600510,155.62,8430133540869,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Neutro.jpg",{"$error":"#VALUE!"}]
[391,"Regulador EN-2000 nitrógeno",37100500,133.13,8430133577766,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Neutro.jpg",{"$error":"#VALUE!"}]
[392,"Regulador EN-2000 hidrógeno",37100020,133.13,8430133545383,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Neutro.jpg",{"$error":"#VALUE!"}]
[393,"Regulador EN-2000 propano",37300000,133.13,8430133439330,"https://galagar.com/wp-content/uploads/2022/01/EN2000-Prop.jpg",{"$error":"#VALUE!"}]
[394,"Regulador Gasweld oxígeno",30500001,109.53,8430133650780,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[395,"Regulador Gasweld acetileno",31400001,109.53,8430133650797]
[396,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[397,"Regulador Gasweld propano",32200001,109.53,8430133667948,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[398,"Regulador Gasweld nitrógeno",36100001,109.53,8430133670764,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[399,"Regulador Gasweld argón-Co2 con rotámetro",36500501,109.53,8430133681722,"https://galagar.com/wp-content/uploads/2022/01/Gasweld-Rotametro.jpg",{"$error":"#VALUE!"}]
[400,"Regulador ARMOR argón-Co2 (¡Nuevo!)",35400500,120.06,8430133836955,"https://galagar.com/wp-content/uploads/2025/02/Modelo-Armor_2.jpg",{"$error":"#VALUE!"}]
[401,"Regulador ARMOR oxígeno (¡Nuevo!)",30400500,120.06,8430133836931,"https://galagar.com/wp-content/uploads/2025/02/Modelo-Armor_2.jpg",{"$error":"#VALUE!"}]
[402,"Regulador ARMOR acetileno (¡Nuevo!)",31500500,120.06,8430133836948,"https://galagar.com/wp-content/uploads/2025/02/Modelo-Armor_2.jpg",{"$error":"#VALUE!"}]
[403,"Regulador ARMOR propano (¡Nuevo!)",35100500,120.06,8430133836962,"https://galagar.com/wp-content/uploads/2025/02/Modelo-Armor_2.jpg",{"$error":"#VALUE!"}]
[404,"Regulador Reducido oxígeno",30600000,109.53,8430133301453,"https://galagar.com/wp-content/uploads/2022/01/Mod-Reducido-OX.jpg",{"$error":"#VALUE!"}]
[405,"Regulador Reducido acetileno",31600000,109.53,8430133301538,"https://galagar.com/wp-content/uploads/2022/01/Mod-Reducido-AC.jpg",{"$error":"#VALUE!"}]
[406,"Regulador Reducido argón-Co2",35600000,109.53,8430133577582,"https://galagar.com/wp-content/uploads/2022/01/Mod-Reducido-ARg.jpg",{"$error":"#VALUE!"}]
[407,"Regulador Reducido nitrógeno",33600000,109.53,8430133326678,"https://galagar.com/wp-content/uploads/2022/01/Mod-Reducido-Neutro.jpg",{"$error":"#VALUE!"}]
[408,"Regulador Sferic oxígeno 300 bar",37000308,158.52000000000001,8430133791179,"https://galagar.com/wp-content/uploads/2022/01/Sferic300-OX.jpg",{"$error":"#VALUE!"}]
[409,"Regulador Sferic nitrógeno 300 bar",37100308,158.52000000000001,8430133791186,"https://galagar.com/wp-content/uploads/2022/01/Sferic300.jpg",{"$error":"#VALUE!"}]
[410,"Regulador Sferic argón-Co2 300 bar",37600338,158.52000000000001,8430133788926,"https://galagar.com/wp-content/uploads/2022/01/Sferic300-AR.jpg",{"$error":"#VALUE!"}]
[411,"Regulador media presión nitrógeno 20 bar",35300420,240.16,8430133326807,"https://galagar.com/wp-content/uploads/2022/01/MediaPresion.jpg",{"$error":"#VALUE!"}]
[412,"Regulador media presión nitrógeno 40 bar",35300440,240.16,8430133326821,"https://galagar.com/wp-content/uploads/2022/01/MediaPresion.jpg",{"$error":"#VALUE!"}]
[413,"Regulador media presión nitrógeno 60 bar",35300460,240.16,8430133577520,"https://galagar.com/wp-content/uploads/2022/01/MediaPresion.jpg",{"$error":"#VALUE!"}]
[414,"Regulador alta presión nitrógeno 200 bar",35300200,596.88,8430133541095,"https://galagar.com/wp-content/uploads/2022/01/AltaPresion.jpg",{"$error":"#VALUE!"}]
[415,"Regulador R80 oxígeno",30700000,259.38,8430133301460,"https://galagar.com/wp-content/uploads/2022/01/Modelo-R80-OX.jpg",{"$error":"#VALUE!"}]
[416,"Regulador R80 acetileno",31700010,259.38,8430133301545,"https://galagar.com/wp-content/uploads/2022/01/Modelo-R80-AC.jpg",{"$error":"#VALUE!"}]
[417,"Regulador R80 aire comprimido",32700000,259.38,8430133577445,"https://galagar.com/wp-content/uploads/2022/01/Modelo-R80-Neu.jpg",{"$error":"#VALUE!"}]
[418,"Regulador R80 nitrógeno",33700000,259.38,8430133301590,"https://galagar.com/wp-content/uploads/2022/01/Modelo-R80-Neu.jpg",{"$error":"#VALUE!"}]
[419,"Regulador R80 hidrógeno",34700000,259.38,8430133301613,"https://galagar.com/wp-content/uploads/2022/01/Modelo-R80-Neu.jpg",{"$error":"#VALUE!"}]
[420,"Regulador R80 argón-Co2",35700000,259.38,8430133577599,"https://galagar.com/wp-content/uploads/2022/01/Modelo-R80-AR.jpg",{"$error":"#VALUE!"}]
[421,"Regulador gran caudal oxígeno - Caudal nominal 150 Nm3/h.",30300000,720.73,8430133326180,"https://galagar.com/wp-content/uploads/2022/01/GranCaudal.jpg",{"$error":"#VALUE!"}]
[422,"Regulador gran caudal acetileno - Caudal nominal 25 Nm3/h.",31300000,720.73,8430133326418,"https://galagar.com/wp-content/uploads/2022/01/GranCaudal.jpg",{"$error":"#VALUE!"}]
[423,"Regulador gran caudal argón-Co2 - Caudal nominal 150 Nm3/h.",30300500,720.73,8430133577377,"https://galagar.com/wp-content/uploads/2022/01/GranCaudal.jpg",{"$error":"#VALUE!"}]
[424,"Regulador gran caudal nitrógeno - Caudal nominal 150 Nm3/h.",33300000,720.73,8430133326623,"https://galagar.com/wp-content/uploads/2022/01/GranCaudal.jpg",{"$error":"#VALUE!"}]
[425,"Regulador gran caudal hidrógeno - Caudal nominal 200 Nm3/h.",34300000,720.73,8430133577476,"https://galagar.com/wp-content/uploads/2022/01/GranCaudal.jpg",{"$error":"#VALUE!"}]
[426,"Regulador gran caudal oxígeno - Caudal nominal 300 Nm3/h.",30300055,833.03,8430133541057,"https://galagar.com/wp-content/uploads/2022/01/GranCaudal.jpg",{"$error":"#VALUE!"}]
[427,"Regulador gran caudal nitrógeno - Caudal nominal 300 Nm3/h.",33300050,833.03,8430133541071,"https://galagar.com/wp-content/uploads/2022/01/GranCaudal.jpg",{"$error":"#VALUE!"}]
[428,"Regulador economizador argón con rotámetro",35600520,311.63,8430133938727,"https://galagar.com/wp-content/uploads/2022/01/Puesto-Trabajo_ECO.jpg",{"$error":"#VALUE!"}]
[429,"Válvula economizadora con regulación integrada",35500050,116.19,8430133626921,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Regulable.jpg",{"$error":"#VALUE!"}]
[430,"Válvula economizadora fija",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[431,"Rotámetro argón-Co2 - Presión 2,5 - 8 mm. 1/4”",35700525,55.14,8430133577612,"https://galagar.com/wp-content/uploads/2022/01/Rotametro.jpg",{"$error":"#VALUE!"}]
[432,"Rotámetro argón-Co2 - Presión atmosférica - 8 mm. 1/4”",35700535,55.14,8430133577643,"https://galagar.com/wp-content/uploads/2022/01/Rotametro.jpg",{"$error":"#VALUE!"}]
[433,"Manómetro 2,5 bar Ø 63 mm. G1/4\" acetileno",31516033,18.84,8430133301514,"https://galagar.com/wp-content/uploads/2022/07/Manometro.jpg",{"$error":"#VALUE!"}]
[434,"Manómetro 16 bar Ø 63 mm. G1/4\" oxígeno",30416024,18.84,8430133301439,"https://galagar.com/wp-content/uploads/2022/07/Manometro.jpg",{"$error":"#VALUE!"}]
[435,"Manómetro 40 bar Ø 63 mm. G1/4\" acetileno",31516034,18.84,8430133301521,"https://galagar.com/wp-content/uploads/2022/07/Manometro.jpg",{"$error":"#VALUE!"}]
[436,"Manómetro 315 bar Ø 63 mm. G1/4\" oxígeno",30416025,18.84,8430133301446,"https://galagar.com/wp-content/uploads/2022/07/Manometro.jpg",{"$error":"#VALUE!"}]
[437,"Manómetro 34 L/min. Ø 63 mm. G1/4\" Ø 0,6-10 bar Argón-Co2",35716054,18.84,8430133577698,"https://galagar.com/wp-content/uploads/2022/07/Manometro.jpg",{"$error":"#VALUE!"}]
[438,"Manómetro 315 Bar-PSI G1/4\" s-gas",30416225,18.84,8430133331436]
[439,"Protección manómetro negra Ø 63",30416050,2.39,8430133326289,"https://galagar.com/wp-content/uploads/2022/01/Proteccion-Manometro_2.jpg",{"$error":"#VALUE!"}]
[440,"Protección manómetro negra Ø 50",38016050,2.89,8430133640026,"https://galagar.com/wp-content/uploads/2022/01/Proteccion-Manometro_2.jpg",{"$error":"#VALUE!"}]
[441,"Calentador para regulador Co2",600000,174.09,8430133800369,"https://galagar.com/wp-content/uploads/2022/01/Calentador-Co2_600000.jpg",{"$error":"#VALUE!"}]
[442,"Calentador Co2 eléctrico centrales 250 w.",600001,1155.8399999999999,8430133645908,"https://galagar.com/wp-content/uploads/2022/01/Precalentador-Electrico_600001.jpg",{"$error":"#VALUE!"}]
[443,"Calentador Co2 hidrotérmico central 1500 w.",600002,1450.76,8430133645915,"https://galagar.com/wp-content/uploads/2022/01/Precalentador-Hidro_600002.jpg",{"$error":"#VALUE!"}]
[444,"Latiguillo flexible 1 m. G1/4” RH oxígeno",71900100,299.33999999999997,8430133341244,"https://galagar.com/wp-content/uploads/2022/01/Latiguillo.jpg",{"$error":"#VALUE!"}]
[445,"Latiguillo flexible 1 m. G1/4” RH Argón-Co2",71900101,299.33999999999997,8430133341251,"https://galagar.com/wp-content/uploads/2022/01/Latiguillo.jpg",{"$error":"#VALUE!"}]
[446,"Latiguillo flexible 1 m. G1/4” RH acetileno",71900102,299.33999999999997,8430133341268,"https://galagar.com/wp-content/uploads/2022/01/Latiguillo.jpg",{"$error":"#VALUE!"}]
[447,"Válvula canalización oxígeno-térmica G 3/4\"",76000666,674.23,8430133587840,"https://galagar.com/wp-content/uploads/2023/06/Multivalvulas-Hor.jpg",{"$error":"#VALUE!"}]
[448,"Válvula canalización acetileno H2-térmica G 3/4\"",76200666,674.23,8430133588052,"https://galagar.com/wp-content/uploads/2022/01/Multivalvulas-Hor_AC.jpg",{"$error":"#VALUE!"}]
[449,"Colector 2 entradas - Izquierda",71200091,140.43,8430133341190,"https://galagar.com/wp-content/uploads/2022/01/Colector_2.jpg",{"$error":"#VALUE!"}]
[450,"Colector 2 entradas - Intermedia",71200095,140.43,8430133547356,"https://galagar.com/wp-content/uploads/2022/01/Colector_2.jpg",{"$error":"#VALUE!"}]
[451,"Colector 2 entradas - Derecha",71200092,140.43,8430133341206,"https://galagar.com/wp-content/uploads/2022/01/Colector_2.jpg",{"$error":"#VALUE!"}]
[452,"Colector 2 entradas - Izquierda con manómetro",71200093,150.97999999999999,8430133341213,"https://galagar.com/wp-content/uploads/2022/01/Colector.jpg",{"$error":"#VALUE!"}]
[453,"Colector 2 entradas - Intermedia con manómetro",71200096,150.97999999999999,8430133547363,"https://galagar.com/wp-content/uploads/2022/01/Colector.jpg",{"$error":"#VALUE!"}]
[454,"Colector 2 entradas - Derecha con manómetro",71200094,150.97999999999999,8430133341220,"https://galagar.com/wp-content/uploads/2022/01/Colector.jpg",{"$error":"#VALUE!"}]
[455,"Manguera 0,35 m. 200 bar G 1/4”",71999035,205.44,8430133341282,"https://galagar.com/wp-content/uploads/2022/01/Manguera.jpg",{"$error":"#VALUE!"}]
[456,"Manguera 0,65 m. 200 bar G 1/4\"",71999060,234.78,8430133341299,"https://galagar.com/wp-content/uploads/2022/01/Manguera.jpg",{"$error":"#VALUE!"}]
[457,"Manguera 1 m. 300 bar G 1/4\"",71999100,264.13,8430133341305,"https://galagar.com/wp-content/uploads/2022/01/Manguera_2.jpg",{"$error":"#VALUE!"}]
[458,"Cambio manual oxígeno 150 M3/h.",71200021,899.73,8430133341046,"https://galagar.com/wp-content/uploads/2022/01/cambioManual.jpg",{"$error":"#VALUE!"}]
[459,"Cambio manual argón-Co2 150 M3/h.",71200022,899.73,8430133341053,"https://galagar.com/wp-content/uploads/2022/01/cambioManual.jpg",{"$error":"#VALUE!"}]
[460,"Cambio manual acetileno 25 M3/h.",71200023,899.73,8430133341060,"https://galagar.com/wp-content/uploads/2022/01/cambioManual.jpg",{"$error":"#VALUE!"}]
[461,"Cambio mecánico oxígeno 150m. 3/h.",71200051,2261.81,8430133341107,"https://galagar.com/wp-content/uploads/2022/01/CambioMacanico.jpg",{"$error":"#VALUE!"}]
[462,"Cambio mecánico argón-Co2 150 m. 3/h.",71200052,2261.81,8430133341114,"https://galagar.com/wp-content/uploads/2022/01/CambioMacanico.jpg",{"$error":"#VALUE!"}]
[463,"Cambio mecánico acetileno 25 m. 3/h.",71200053,2261.81,8430133341121,"https://galagar.com/wp-content/uploads/2022/01/CambioMacanico.jpg",{"$error":"#VALUE!"}]
[464,"Cambio electrónico oxígeno 150m. 3/h.",71200081,3408.6,8430133341169,"https://galagar.com/wp-content/uploads/2022/01/CambioElectronico.jpg",{"$error":"#VALUE!"}]
[465,"Cambio electrónico argón-Co2 150 m. 3/h.",71200082,3408.6,8430133341176,"https://galagar.com/wp-content/uploads/2022/01/CambioElectronico.jpg",{"$error":"#VALUE!"}]
[466,"Cambio electrónico acetileno 25 m. 3/h.",71200083,3408.6,8430133341183,"https://galagar.com/wp-content/uploads/2022/01/CambioElectronico.jpg",{"$error":"#VALUE!"}]
[467,"Puesto trabajo oxígeno simple cromado",71600127,214.41,8430133625795,"https://galagar.com/wp-content/uploads/2022/01/PuestoSimple.jpg",{"$error":"#VALUE!"}]
[468,"Puesto trabajo argón-Co2 simple cromado",71600726,214.41,8430133625702,"https://galagar.com/wp-content/uploads/2022/01/PuestoSimple.jpg",{"$error":"#VALUE!"}]
[469,"Puesto trabajo nitrógeno - Simple cromado",71600801,214.41,8430133625801,"https://galagar.com/wp-content/uploads/2022/01/PuestoSimple.jpg",{"$error":"#VALUE!"}]
[470,"Puesto trabajo acetileno - Simple cromado",71700126,214.41,8430133625696,"https://galagar.com/wp-content/uploads/2022/01/PuestoSimple.jpg",{"$error":"#VALUE!"}]
[471,"Puesto trabajo propano - Simple cromado",71700701,214.41,8430133625719,"https://galagar.com/wp-content/uploads/2022/01/PuestoSimple.jpg",{"$error":"#VALUE!"}]
[472,"Puesto trabajo argón-Co2 con rotámetro - Simple cromado",71600733,271.31,8430133625733,"https://galagar.com/wp-content/uploads/2022/01/PuestoRotametro.jpg",{"$error":"#VALUE!"}]
[473,"Puesto trabajo oxígeno-acetileno - Doble cromado",71700801,411.24,8430133625771,"https://galagar.com/wp-content/uploads/2022/01/PuestodeTrabajo.jpg",{"$error":"#VALUE!"}]
[474,"Puesto trabajo oxígeno-propano - Doble cromado",71700901,411.24,8430133625788,"https://galagar.com/wp-content/uploads/2022/01/PuestodeTrabajo.jpg",{"$error":"#VALUE!"}]
[475,"Regulador reducido argón-Co2 con rotámetro",35600520,311.63,8430133938727,"https://galagar.com/wp-content/uploads/2022/01/Puesto-Trabajo_ECO.jpg",{"$error":"#VALUE!"}]
[476,"Panel descompresión Oxicorte oxígeno-acetileno",71200510,1305.68,8430133668228,"https://galagar.com/wp-content/uploads/2022/01/Panel-Oxicorte.jpg",{"$error":"#VALUE!"}]
[477,"Panel descompresión Oxicorte oxígeno-propano",71200520,1305.68,8430133668235,"https://galagar.com/wp-content/uploads/2022/01/Panel-Oxicorte.jpg",{"$error":"#VALUE!"}]
[478,"Panel descompresión Oxicorte oxígeno-gas natural",71200530,1305.68,8430133668242,"https://galagar.com/wp-content/uploads/2022/01/Panel-Oxicorte.jpg",{"$error":"#VALUE!"}]
[479,"Panel descompresión Corte por plasma oxígeno-nitrógeno-Argón-Co2",71200540,3537.09,8430133668259,"https://galagar.com/wp-content/uploads/2022/01/Panel-Plasma.jpg",{"$error":"#VALUE!"}]
[480,"Panel descompresión Corte por plasma - oxígeno-nitrógeno-hidrógeno",71200550,2362.67,8430133668266]
[481,"Panel descompresión Corte por láser oxígeno-nitrógeno",71200560,2839.35,8430133668211,"https://galagar.com/wp-content/uploads/2022/01/Panel-Laser.jpg",{"$error":"#VALUE!"}]
[482,"Regulador Modelo Simple Etapa Níquel GPR-1N",34500000,314.02,8430133583996,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPR-1.jpg",{"$error":"#VALUE!"}]
[483,"Regulador Modelo Simple Etapa Inoxidable GPR-1S",34100000,760.77,8430133583576,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPR-1.jpg",{"$error":"#VALUE!"}]
[484,"Regulador Modelo Doble Etapa Níquel GPR-11N",34200000,439.63,8430133583989,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPR-11.jpg",{"$error":"#VALUE!"}]
[485,"Regulador Modelo Doble Etapa Inoxidable GPR-11S",34000000,1960.91,8430133583569,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPR-11.jpg",{"$error":"#VALUE!"}]
[486,"Regulador Modelo Canalización Níquel GPR-1LN",35000000,524.70000000000005,8430133585266,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPR-1L.jpg",{"$error":"#VALUE!"}]
[487,"Regulador Modelo Canalización Inoxidable GPR-1LS",34800000,621.76,8430133585259,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPR-1L.jpg",{"$error":"#VALUE!"}]
[488,"Regulador Modelo Doble Etapa Níquel GPR-141",34200141,"CONSULTAR",8430133820923,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPR-141.jpg",{"$error":"#VALUE!"}]
[489,"Regulador Modelo Gran Caudal Níquel GPR-2HF",34500500,"CONSULTAR",8430133615253,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPR-2HF.jpg",{"$error":"#VALUE!"}]
[490,"Panel de descompresión 2 entradas Níquel GPP-2G",34500550,"CONSULTAR",8430133818494,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPP-2G.jpg",{"$error":"#VALUE!"}]
[491,"Panel de descompresión 2 entradas Níquel GPP-762",34500555,"CONSULTAR",8430133820930,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPP-762.jpg",{"$error":"#VALUE!"}]
[492,"Panel de descompresión 2 entradas Níquel GPP-2G HF",34500560,"CONSULTAR",8430133820145,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPP-2GHF.jpg",{"$error":"#VALUE!"}]
[493,"Panel de descompresión Semi-automática Níquel GPP-4G",34500570,"CONSULTAR",8430133820947,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPP-4G.jpg",{"$error":"#VALUE!"}]
[494,"Panel de descompresión Semi-automática Níquel GPP-4G HF",34500575,"CONSULTAR",8430133820954,"https://galagar.com/wp-content/uploads/2022/01/GasPuro-GPP-4GHF.jpg",{"$error":"#VALUE!"}]
[495,"Regulador panelable  RB-GG-410 4bar G1/4”",35000410,284.63,8430133615482,"https://galagar.com/wp-content/uploads/2022/01/Panelable-RP-GG.jpg",{"$error":"#VALUE!"}]
[496,"Regulador panelable de cabina RC-GG-910 10bar G1/4”",35000910,483.59,8430133627270,"https://galagar.com/wp-content/uploads/2022/01/Panelable-Cabina-RC-GG.jpg",{"$error":"#VALUE!"}]
[497,"Smart 120 MMA MINI-SYNER (equipo con maletín)","22300120MS",202.96,8430133824631,"https://galagar.com/wp-content/uploads/2022/11/MiniSyner-120_1.jpg",{"$error":"#VALUE!"}]
[498,"Smart 160 MMA (equipo con maletín)","22300160MMA",311.13,8430133791582,"https://galagar.com/wp-content/uploads/2023/03/Smart-160MMA-22.jpg",{"$error":"#VALUE!"}]
[499,"Smart 200 MMA (equipo con voltímetro y maletín)","22300200MMAVI",392.72,8430133791087,"https://galagar.com/wp-content/uploads/2022/07/Smart-200MMA-22.jpg",{"$error":"#VALUE!"}]
[500,"Paquete electrodos de rutilo Ø 3,25 mm. (85 uds.)","23301632PQ",14.97,8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[501,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[502,"Antorcha TIG SR17 V - 4 metros","19051704P",142.36000000000001,8430133652838,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[503,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[504,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[505,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[506,"Atlantic 180 MMA (equipo + masa y pinza portaelectrodos)","22290180AC",393.67,8430133646899,"https://galagar.com/wp-content/uploads/2022/03/Atlantic-180MMA.jpg",{"$error":"#VALUE!"}]
[507,"Atlantic 200 MMA (equipo + masa y pinza portaelectrodos)","22290202AC",461.49,8430133646905,"https://galagar.com/wp-content/uploads/2022/03/Atlantic-200MMA.jpg",{"$error":"#VALUE!"}]
[508,"Paquete electrodos de rutilo Ø 3,25 mm. (85 uds.)","23301632PQ",14.97,8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[509,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[510,"Antorcha TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[511,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[512,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[513,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[514,"Kennedy 160 SYNER (equipo + maletín)","22300160DGT",603.69000000000005,8430133804077,"https://galagar.com/wp-content/uploads/2022/03/Kennedy-160-Syner.jpg",{"$error":"#VALUE!"}]
[515,"Kennedy 200 SYNER (equipo + maletín)","22300200DGT",664.06,8430133804084,"https://galagar.com/wp-content/uploads/2022/03/Kennedy-200-Syner.jpg",{"$error":"#VALUE!"}]
[516,"Paquete electrodos de rutilo Ø 3,25 mm. (85 uds.)","23301632PQ",14.97,8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[517,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[518,"Antorcha TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[519,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[520,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[521,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[522,"Smart 160 PFC (equipo + masa y pinza portaelectrodos)","22300160PFC",724.81,8430133682774,"https://galagar.com/wp-content/uploads/2022/01/Smart-160PFC.jpg",{"$error":"#VALUE!"}]
[523,"Paquete electrodos de rutilo Ø 3,25 mm. (85 uds.)","23301632PQ",14.97,8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[524,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[525,"Antorcha TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[526,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[527,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[528,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[529,"Smart 150 MMA Battery (equipo + Batería y cargador + masa y pinza portaelectrodos)","22300150BT",3137.71,8430133823023,"https://galagar.com/wp-content/uploads/2022/07/Smart-150-Batt.jpg",{"$error":"#VALUE!"}]
[530,"Paquete electrodos de rutilo Ø 3,25 mm. (85 uds.)","23301632PQ",14.97,8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[531,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[532,"Smart PRO 5.0 PFC - MMA-TIG DC (equipo + masa y pinza portaelectrodos)",22300315,1850,8430133629533,"https://galagar.com/wp-content/uploads/2022/01/SmartPRO5.jpg",{"$error":"#VALUE!"}]
[533,"Paquete electrodos de rutilo Ø 3,25 mm. (85 uds.)","23301632PQ",14.97,8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[534,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[535,"Antorcha TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[536,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[537,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[538,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[539,"Smart 400 MMA (equipo + mando a distancia + masa y pinza portaelectrodos)","22300400E",1800,8430133790837,"https://galagar.com/wp-content/uploads/2022/07/Smart400MMA.jpg",{"$error":"#VALUE!"}]
[540,"Paquete electrodos de rutilo Ø 3,25 mm. (85 uds.)","23301632PQ",14.97,8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[541,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[542,"Antorcha TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[543,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[544,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[545,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[546,"Smart 210 TIG Pulse DC - INOX (equipo + tubo de gas y toma de masa)","22300210TS",950,8430133826710,"https://galagar.com/wp-content/uploads/2023/03/Smart-210TIG-Pulse.jpg",{"$error":"#VALUE!"}]
[547,"Smart 200 TIG Pulse AC/DC - INOX/ALUMINIO (equipo + tubo de gas y toma de masa)","22300200TACDC",1800,8430133662653,"https://galagar.com/wp-content/uploads/2022/05/Smart200-TIGp-ACDC.jpg",{"$error":"#VALUE!"}]
[548,"Antorcha TIG SR26 E - 4 metros","19052614P",173.55,8430133652869,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[549,"Estuche consumibles TIG","ETIG",34.159999999999997,8430133682934,"https://galagar.com/wp-content/uploads/2022/01/Estuche_TIG.jpg",{"$error":"#VALUE!"}]
[550,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[551,"Máscara electrónica Galaxy - Para TIG 1/1/1/1","51259B",170.1,8430133667641,"https://galagar.com/wp-content/uploads/2022/01/Galaxy_2.jpg",{"$error":"#VALUE!"}]
[552,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[553,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[554,"Smart 400 TIG Pulse DC (equipo + refrigeración + carro + Pedal de control)","22300400T",3750,8430133790011,"https://galagar.com/wp-content/uploads/2022/05/Smart400TIGp.jpg",{"$error":"#VALUE!"}]
[555,"Smart 315 TIG Pulse AC/DC (equipo + refrigeración + carro + Pedal de control)","22300315ACDCKIT",4493,8430133820886,"https://galagar.com/wp-content/uploads/2022/05/Smart315TIGp.jpg",{"$error":"#VALUE!"}]
[556,"Antorcha TIG SR18 - 4 metros","19051814P",214.96,8430133652876,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[557,"Estuche consumibles TIG","ETIG",34.159999999999997,8430133682934,"https://galagar.com/wp-content/uploads/2022/01/Estuche_TIG.jpg",{"$error":"#VALUE!"}]
[558,"Líquido refrigerante 10 litros",39200094,112.47,8430133658298,"https://galagar.com/wp-content/uploads/2022/07/Refrigerante.jpg",{"$error":"#VALUE!"}]
[559,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[560,"Máscara electrónica Galaxy - Para TIG 1/1/1/1","51259B",170.1,8430133667641,"https://galagar.com/wp-content/uploads/2022/01/Galaxy_2.jpg",{"$error":"#VALUE!"}]
[561,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[562,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[563,"Smart 200 MP SYNER (¡Nueva!)  (equipo + masa y pinza portaelectrodos)","22300200MPS",755,8430133838720,"https://galagar.com/wp-content/uploads/2025/02/Smart200MPsyner-2.jpg",{"$error":"#VALUE!"}]
[564,"Antorcha MIG 25 - 4 metros","880025P",120.67,8430133652807,"https://galagar.com/wp-content/uploads/2022/01/7xm-25.jpg",{"$error":"#VALUE!"}]
[565,"Estuche consumibles para antorcha MIG","EMIG25",37.57,8430133682972,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG25.jpg",{"$error":"#VALUE!"}]
[566,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[567,"Estuche consumibles TIG","ETIG",34.159999999999997,8430133682934,"https://galagar.com/wp-content/uploads/2022/01/Estuche_TIG.jpg",{"$error":"#VALUE!"}]
[568,"Ver catálogo de consumibles hilo - Página 103"]
[569,"Antorcha TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[570,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[571,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[572,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[573,"Smart MIG 350 MP (equipo + masa y tubo de gas + carro de transporte)","22300350MPV1",2450.5500000000002,8430133826130,"https://galagar.com/wp-content/uploads/2023/01/SmartMIG350_New.jpg",{"$error":"#VALUE!"}]
[574,"Antorcha MIG 36 - 4 metros","880036P",163.69,8430133652814,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[575,"Estuche consumibles para antorcha MIG","EMIG36",50.64,8430133682989,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG36-M8.jpg",{"$error":"#VALUE!"}]
[576,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[577,"Ver catálogo de consumibles hilo - Página 103"]
[578,"Antorcha TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[579,"Caja de tungstenos negro Ø 3,2 mm.","750324C",100.07,8430133569020,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[580,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[581,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[582,"Smart MIG 500 MP - 5 metros (Cable masa + tubo de gas)","22300500MPKIT",5073.67,8430133809133,"https://galagar.com/wp-content/uploads/2022/01/SmartMIG500MP.jpg",{"$error":"#VALUE!"}]
[583,"Smart MIG 500 MP - 10 metros (Cable masa + tubo de gas)","22300510MPKIT",5299.11,null,"https://galagar.com/wp-content/uploads/2022/01/SmartMIG500MP.jpg"]
[584,"Antorcha MIG 501","880501P",244.79,8430133652821,null,{"$error":"#VALUE!"}]
[585,"Estuche consumibles para antorcha de MIG","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[586,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[587,"Regulador Gasweld argón-Co2",36500001,109.53,8430133653415,"https://galagar.com/wp-content/uploads/2022/01/Modelo-Gasweld.jpg",{"$error":"#VALUE!"}]
[588,"Líquido refrigerante 10 litros",39200094,112.47,8430133658298,"https://galagar.com/wp-content/uploads/2022/07/Refrigerante.jpg",{"$error":"#VALUE!"}]
[589,"Ver catálogo de consumibles hilo - Página 103"]
[590,"Antorcha TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[591,"Estuche consumibles TIG","ETIG",34.159999999999997,8430133682934,"https://galagar.com/wp-content/uploads/2022/01/Estuche_TIG.jpg",{"$error":"#VALUE!"}]
[592,"Caja de tungstenos negro Ø 3,2 mm.","750324C",100.07,8430133569020,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg"]
[593,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[594,"Smart CUT 45 PFC (Equipo + antorcha de plasma PT-40)","2230045PFC",1556.36,8430133683535,null,{"$error":"#VALUE!"}]
[595,"KIT consumibles para antorcha PT-40","KITPT40",118.47,8430133804473,"https://galagar.com/wp-content/uploads/2022/01/KIT-Antorcha-Plasma.jpg",{"$error":"#VALUE!"}]
[596,"Smart CUT 850 (Equipo + antorcha de plasma TH-125)","22300850C",3156.75,8430133835279,"https://galagar.com/wp-content/uploads/2024/06/SmartCUT850.jpg",{"$error":"#VALUE!"}]
[597,"KIT consumibles para antorcha TH-125","KITTH125",284.22000000000003,8430133803988,"https://galagar.com/wp-content/uploads/2022/01/KIT-Antorcha-Plasma.jpg",{"$error":"#VALUE!"}]
[598,"Smart CUT 1050 (Equipo + antorcha de plasma TH-125)","223001050C",4612.43,8430133827939]
[599,"KIT consumibles para antorcha TH-125","KITTH125",284.22000000000003,8430133803988,"https://galagar.com/wp-content/uploads/2022/01/KIT-Antorcha-Plasma.jpg",{"$error":"#VALUE!"}]
[600,"Smart CUT 1250 (Equipo + antorcha de plasma UPH-160)","223001250C",5009.3999999999996,8430133835286,"https://galagar.com/wp-content/uploads/2024/06/SmartCUT1250.jpg",{"$error":"#VALUE!"}]
[601,"KIT consumibles para antorcha UPH-160","KITUPH160",312.47000000000003]
[602,"Smart FLUX 105 Equipo monofásico para soldadura con hilo tubular","22300105AF","CONSULTAR",8430133830137]
[603,"Bobina de hilo tubular 1 Kg.","223300100AF01","CONSULTAR"]
[604,"Gala 1600 MMA SYNER (¡Nueva!)","22300160GS",206,8430133835958]
[605,"Gala 2000 MMA SYNER (¡Nueva!)","22300200GS",283.25,8430133835965]
[606,"Paquete electrodos de rutilo Ø 3,25 mm. (85 uds.)","23301632PQ",14.97,8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[607,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[608,"Antorcha TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[609,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[610,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[611,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[612,"GAR 4TT (rectificador electromecánico)","46886000TT","CONSULTAR",8430133823795]
[613,"GAR 5T (rectificador electromecánico)",2600500,"CONSULTAR",8430133784850,"https://galagar.com/wp-content/uploads/2022/05/Gar5T.jpg",{"$error":"#VALUE!"}]
[614,"GAR 6T (rectificador electromecánico)",2600600,"CONSULTAR",8430133564346,"https://galagar.com/wp-content/uploads/2022/05/Gar6T.jpg",{"$error":"#VALUE!"}]
[615,"Continuos 400 (rectificador electrónico)",41100100,"CONSULTAR",8430133804480,"https://galagar.com/wp-content/uploads/2022/01/Continuos-400.jpg",{"$error":"#VALUE!"}]
[616,"Continuos 600 (rectificador electrónico)",41200100,"CONSULTAR",8430133804497,"https://galagar.com/wp-content/uploads/2022/01/Continuos-600.jpg",{"$error":"#VALUE!"}]
[617,"Paquete electrodos rutilo 3,25 mm. (85 uds.)","23301632PQ",14.97,8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[618,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[619,"Accesorios electrodo (cable masa + pinza masa)",259040,103.67,8430133400026,"https://galagar.com/wp-content/uploads/2022/01/ACC-Atlantic.jpg",{"$error":"#VALUE!"}]
[620,"Antorcha de TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[621,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[622,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[623,"Ver catálogo de consumibles para varillas TIG - Página 103"]
[624,"Gala 2000 MP (cable masa + tubo gas)",54300000,2049.66,8430133790943,"https://galagar.com/wp-content/uploads/2022/01/Gala-2000MP.jpg",{"$error":"#VALUE!"}]
[625,"Antorcha MIG 25 - 4 metros","880025P",120.67,8430133652807,"https://galagar.com/wp-content/uploads/2022/01/7xm-25.jpg",{"$error":"#VALUE!"}]
[626,"Estuche consumibles para antorcha MIG","EMIG25",37.57,8430133682972,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG25.jpg",{"$error":"#VALUE!"}]
[627,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[628,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[629,"Ver catálogo consumibles hilo Página 103"]
[630,"Antorcha de TIG SR26 V - 4 metros","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[631,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[632,"SynergicLine  Gala MIG 2700i (equipo + cable masa + tubo gas + ruleta Ø 37 mm. 0.8-1.0 - x2)",42400000,2289.65,8430133420475,"https://galagar.com/wp-content/uploads/2023/12/New_GalaMIG-2700i.jpg",{"$error":"#VALUE!"}]
[633,"Antorcha MIG 25 - 4 metros","880025P",120.67,8430133652807,"https://galagar.com/wp-content/uploads/2022/01/7xm-25.jpg",{"$error":"#VALUE!"}]
[634,"Estuche consumibles para antorcha MIG","EMIG25",37.57,8430133682972,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG25.jpg",{"$error":"#VALUE!"}]
[635,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[636,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[637,"SynergicLine  Gala MIG 3500i (equipo + cable masa + tubo gas + ruleta Ø 37 mm. 0.8-1.0 - x2)",42500100,2578.19,8430133696887]
[638,"Antorcha MIG 36 - 4 metros","880036P",163.69,8430133652814,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[639,"Estuche consumibles para antorcha MIG","EMIG36",50.64,8430133682989,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG36-M8.jpg",{"$error":"#VALUE!"}]
[640,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[641,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[642,"SynergicLine  Gala MIG 4000i DP (equipo + cable masa + tubo gas + ruleta Ø 37 mm. 0.8-1.0 - x2)","42800000KIT",4020.97,null,"https://galagar.com/wp-content/uploads/2023/09/GalaMIG-Rf_4000i.jpg",{"$error":"#VALUE!"}]
[643,"Devanadora D-R4 I",66800000,"INCLUIDO",8430133802738]
[644,"Conexión devanadora D-4R i (5 metros)","63800000i","INCLUIDO",8430133831912]
[645,"Antorcha MIG 36 - 4 metros","880036P",163.69,8430133652814,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[646,"Estuche consumibles para antorcha MIG","EMIG36",50.64,8430133682989,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG36-M8.jpg",{"$error":"#VALUE!"}]
[647,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[648,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[649,"SynergicLine  Gala MIG 4000i DP Refrigerado (equipo + cable masa + tubo gas + ruleta Ø 37 mm. 0.8-1.0 - x2)","42800000KITR",5047.5200000000004,null,"https://galagar.com/wp-content/uploads/2023/09/GalaMIG-Rf_4000i.jpg",{"$error":"#VALUE!"}]
[650,"Devanadora D-R4 I",66800000,"INCLUIDO",8430133802738]
[651,"Conexión devanadora D-4R i (5 metros)","63900000i","INCLUIDO",8430133833633]
[652,"Módulo de refrigeración WCS-500i",65800000,"INCLUIDO",8430133832643]
[653,"Antorcha MIG 501 - 4 metros","880501P",244.79,8430133652821]
[654,"Estuche consumibles para antorcha MIG","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[655,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[656,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg"]
[657,"SynergicLine  Gala MIG 5000i DPW (equipo + cable masa + tubo gas + ruleta Ø 37 mm. 0.8-1.0 - x2)",42900000,6365.25,8430133837365,"https://galagar.com/wp-content/uploads/2024/02/SinerLIne_GalaMIG_5000i.jpg"]
[658,"Devanadora D-R4 I",66800000,"INCLUIDO",8430133802738]
[659,"Conexión devanadora D-4R i (5 metros)","63900000i","INCLUIDO",8430133833633]
[660,"Módulo de refrigeración WCS-500i",65800000,"INCLUIDO",8430133832643]
[661,"Antorcha MIG 501 - 4 metros","880501P",244.79,8430133652821,null,{"$error":"#VALUE!"}]
[662,"Estuche consumibles para antorcha MIG","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[663,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[664,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[665,"GTS 3200 AC/DC - INOX y ALUMINIO - (equipo + cable masa + tubo gas)",47000000,"CONSULTAR",8430133630188,"https://galagar.com/wp-content/uploads/2022/01/GTS-3200-ACDC_Refrigerada.jpg",{"$error":"#VALUE!"}]
[666,"Estación de trabajo",51712090,"CONSULTAR",8430133404994,"https://galagar.com/wp-content/uploads/2022/01/EstacionTrabajo.jpg",{"$error":"#VALUE!"}]
[667,"Antorcha de TIG SR26 E - 4 metros","19052614P",173.55,8430133652869,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[668,"Estuche consumibles TIG","ETIG",34.159999999999997,8430133682934,"https://galagar.com/wp-content/uploads/2022/01/Estuche_TIG.jpg",{"$error":"#VALUE!"}]
[669,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[670,"Pantalla electrónica automática 4-13 Galaxy especial TIG","51259B",170.1,8430133667641,"https://galagar.com/wp-content/uploads/2022/01/Galaxy_2.jpg",{"$error":"#VALUE!"}]
[671,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg"]
[672,"Equipo montado y testado","GMT",184.65,8430133809171,null,{"$error":"#VALUE!"}]
[673,"Ver catálogo consumibles varilla para TIG Página 103"]
[674,"GTS 3200 AC/DC Refrigerado - INOX y ALUMINIO - (equipo + cable masa + tubo gas)",47000000,"CONSULTAR",8430133630188,"https://galagar.com/wp-content/uploads/2022/01/GTS-3200-ACDC_Refrigerada.jpg"]
[675,"Carro de transporte",64191000,"CONSULTAR",8430133813321,null,{"$error":"#VALUE!"}]
[676,"Antorcha de TIG SR18 E (refrigerada) - 4 metros","19051814P",214.96,8430133652876,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[677,"Estuche consumibles TIG","ETIG",34.159999999999997,8430133682934,"https://galagar.com/wp-content/uploads/2022/01/Estuche_TIG.jpg"]
[678,"Módulo de refrigeración",65982000,"CONSULTAR",8430133664756,null,{"$error":"#VALUE!"}]
[679,"Líquido refrigerante 10 litros",39200094,112.47,8430133658298,"https://galagar.com/wp-content/uploads/2022/07/Refrigerante.jpg",{"$error":"#VALUE!"}]
[680,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[681,"Pantalla electrónica automática 4-13 Galaxy especial TIG","51259B",170.1,8430133667641,"https://galagar.com/wp-content/uploads/2022/01/Galaxy_2.jpg",{"$error":"#VALUE!"}]
[682,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[683,"Equipo montado y testado","GMT",184.65,8430133809171]
[684,"Ver catálogo consumibles varilla para TIG Página 103"]
[685,"Soporte para devanadora de hilo frío",64185101,"CONSULTAR",8430133614041]
[686,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[687,"Mando a distancia para GTS 3200",42312058,677.93,8430133605582]
[688,"Afilador de tungstenos","8044166NT","CONSULTAR"]
[689,"Devanadora de hilo frío",66700000,3012.57,8430133644222,"https://galagar.com/wp-content/uploads/2022/01/Devanadora-DTCW4R-Sincro.jpg",{"$error":"#VALUE!"}]
[690,"Lápiz 3 metros euro 1.2-1.6 mm.","481P001001",741.19,8430133785178]
[691,"Guía TIG euro",66799999,90.39,8430133656652,"https://galagar.com/wp-content/uploads/2022/01/GuiaTIG-euro.jpg",{"$error":"#VALUE!"}]
[692,"Kit sujeción para antorcha TIG","481P101024",424.84,8430133646370,"https://galagar.com/wp-content/uploads/2022/01/Kit-Sujecion.jpg",{"$error":"#VALUE!"}]
[693,"Gala MIG 2600 (equipo + cable masa + tubo gas + ruleta V Ø40 mm. 0.8-1.0 mm.)",43800000,2431,8430133426187,"https://galagar.com/wp-content/uploads/2022/05/GalaMIG2600.jpg",{"$error":"#VALUE!"}]
[694,"Antorcha MIG 25 - 4 metros","880025P",120.67,8430133652807,"https://galagar.com/wp-content/uploads/2022/01/7xm-25.jpg",{"$error":"#VALUE!"}]
[695,"Estuche consumibles para antorcha MIG","EMIG25",37.57,8430133682972,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG25.jpg",{"$error":"#VALUE!"}]
[696,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[697,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[698,"Ver catálogo consumibles hilo Página 103"]
[699,"Kit voltímetro + amperímetro digital",43981075,426.12,8430133439750]
[700,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[701,"Antorcha MIG 25 - 3 metros (para aluminio)","M253000",117.89,8430133804503]
[702,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[703,"Ruleta U Ø 40 mm. 1.0-1.2 mm. (para aluminio)",63106021,27.43,8430133765040]
[704,"Gala MIG 4000 (equipo + cable masa + tubo gas + ruleta V Ø40 mm. 0.8-1.0 mm.)",43988000,3204,8430133603403,"https://galagar.com/wp-content/uploads/2022/05/GalaMIG4000.jpg",{"$error":"#VALUE!"}]
[705,"Antorcha MIG 36 - 4 metros","880036P",163.69,8430133652814,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[706,"Estuche consumibles para antorcha MIG","EMIG36",50.64,8430133682989,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG36-M8.jpg",{"$error":"#VALUE!"}]
[707,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[708,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg"]
[709,"Ver catálogo consumibles hilo Página 103"]
[710,"Kit voltímetro + amperímetro digital",43981075,426.12,8430133439750,null,{"$error":"#VALUE!"}]
[711,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[712,"Antorcha MIG 36 - 3 metros (para aluminio)","M363000",169.52,8430133801496]
[713,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[714,"Ruleta U Ø 30 mm 1.0-1.2 mm. (para aluminio)",62006021,27.43,8430133763442]
[715,"Ruleta U Ø 30 mm 1.2-1.6 mm. (para aluminio)",62006022,27.43,8430133723279]
[716,"Ruleta para tubular Ø 30 mm. 1.2-1.6 mm.",62006015,30.38,8430133723231]
[717,"Gala MIG 3000 (equipo + cable masa + tubo gas + ruleta V Ø40 mm. 0.8-1.0 mm.)","43898000KIT",3251,8430133606350,"https://galagar.com/wp-content/uploads/2022/01/GalaMIG-3000.jpg",{"$error":"#VALUE!"}]
[718,"Antorcha MIG 25 - 4 metros","880025P",120.67,8430133652807,"https://galagar.com/wp-content/uploads/2022/01/7xm-25.jpg",{"$error":"#VALUE!"}]
[719,"Estuche consumibles para antorcha MIG","EMIG25",37.57,8430133682972,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG25.jpg",{"$error":"#VALUE!"}]
[720,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[721,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg"]
[722,"Ver catálogo consumibles hilo Página 103"]
[723,"Kit voltímetro + amperímetro digital",43981075,426.12,8430133439750,null,{"$error":"#VALUE!"}]
[724,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[725,"Antorcha MIG 25 - 3 metros (para aluminio)","M253000",117.89,8430133804503]
[726,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[727,"Ruleta U Ø40 mm. 1.0-1.2 mm. (para aluminio)",63106021,27.43,8430133765040]
[728,"10 metros conexión devanadora",63781000,567.48,8430133402907]
[729,"15 metros conexión devanadora",63787000,952.29,8430133775513]
[730,"20 metros conexión devanadora",63782000,1370.33,8430133353650]
[731,"Devanadora 4 ruletas",62100000,1442.78,8430133402815,"https://galagar.com/wp-content/uploads/2022/01/Devanadora-D20-A.jpg",{"$error":"#VALUE!"}]
[732,"Gala MIG 3800 (equipo + cable masa + tubo gas + ruleta V Ø40 mm. 0.8-1.0 mm.)","43990000KIT",4178,8430133606367,"https://galagar.com/wp-content/uploads/2022/01/GalaMIG-3800.jpg",{"$error":"#VALUE!"}]
[733,"Antorcha MIG 36 - 4 metros","880036P",163.69,8430133652814,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[734,"Estuche consumibles para antorcha MIG","EMIG36",50.64,8430133682989,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG36-M8.jpg",{"$error":"#VALUE!"}]
[735,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[736,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[737,"Ver catálogo consumibles hilo Página 103"]
[738,"Kit voltímetro + amperímetro digital",43981075,426.12,8430133439750]
[739,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[740,"Antorcha MIG 36 - 3 metros (para aluminio)","M363000",169.52,8430133801496]
[741,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[742,"Ruleta U Ø40 mm. 1.0-1.2 mm. (para aluminio)",63106021,27.43,8430133765040]
[743,"10 metros conexión devanadora",63781000,567.48,8430133402907]
[744,"15 metros conexión devanadora",63787000,952.29,8430133775513]
[745,"20 metros conexión devanadora",63782000,1370.33,8430133353650]
[746,"Devanadora 4 ruletas",62100000,1442.78,8430133402815,"https://galagar.com/wp-content/uploads/2022/01/Devanadora-D20-A.jpg",{"$error":"#VALUE!"}]
[747,"Gala MIG 4007","43100000KIT",5746,8430133850128,"https://galagar.com/wp-content/uploads/2022/05/GalaMIG4007.jpg",{"$error":"#VALUE!"}]
[748,"Gala MIG 5100","42100000KIT","CONSULTAR",8430133849641,"https://galagar.com/wp-content/uploads/2022/05/GalaMIG5100.jpg",{"$error":"#VALUE!"}]
[749,"Antorcha MIG 36 - 4 metros","880036P",163.69,8430133652814,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[750,"Estuche consumibles para antorcha MIG","EMIG36",50.64,8430133682989,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG36-M8.jpg",{"$error":"#VALUE!"}]
[751,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[752,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[753,"Ver catálogo consumibles hilo Página 103"]
[754,"Kit voltímetro + amperímetro digital",43981075,426.12,8430133439750]
[755,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[756,"Antorcha MIG 36 - 3 metros (para aluminio)","M363000",169.52,8430133801496]
[757,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[758,"Ruleta U Ø 30 mm. 1.0-1.2 mm. (para aluminio) x2",62006021,27.43,8430133763442]
[759,"Ruleta U Ø 30 mm. 1.2-1.6 mm. (para aluminio) x2",62006022,27.43,8430133723279]
[760,"10 metros conexión devanadora",63881000,567.48,8430133402914]
[761,"15 metros conexión devanadora",63884000,1099,8430133353728]
[762,"20 metros conexión devanadora",63882000,1813.6,8430133403157]
[763,"Devanadora 4 ruletas cerrada D-22C",62900000,1672.66,8430133581763,"https://galagar.com/wp-content/uploads/2022/01/Devanadora-D22C.jpg",{"$error":"#VALUE!"}]
[764,"Gala MIG 4007 REFRIGERADA","43100000RKIT",7287,8430133850135,"https://galagar.com/wp-content/uploads/2022/05/GalaMIG4007.jpg",{"$error":"#VALUE!"}]
[765,"Gala MIG 5100 REFRIGERADA","42100000RKIT","CONSULTAR",8430133849658,"https://galagar.com/wp-content/uploads/2022/05/GalaMIG5100.jpg",{"$error":"#VALUE!"}]
[766,"Antorcha MIG 501 - 4 metros","880501P",244.79,8430133652821]
[767,"Estuche consumibles para antorcha MIG","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[768,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[769,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[770,"Líquido refrigerante 10 litros",39200094,112.47,8430133658298,"https://galagar.com/wp-content/uploads/2022/07/Refrigerante.jpg",{"$error":"#VALUE!"}]
[771,"Ver catálogo consumibles hilo Página 103"]
[772,"Kit voltímetro + amperímetro digital",43981075,426.12,8430133439750]
[773,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[774,"Antorcha MIG 501 - 3 metros (para aluminio)","M503000",301.19,8430133801502]
[775,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[776,"Ruleta U Ø30 mm. 1.0-1.2 mm. (para aluminio) x2",62006021,27.43,8430133763442]
[777,"Ruleta U Ø30 mm. 1.2-1.6 mm. (para aluminio) x2",62006022,27.43,8430133723279]
[778,"10 metros conexión devanadora refrigerado",63981000,812.72,8430133402921]
[779,"15 metros conexión devanadora refrigerado",63983000,1283.73,8430133766139]
[780,"20 metros conexión devanadora refrigerado",63982000,2000.11,8430133403171]
[781,"Devanadora 4 ruletas cerrada D-22C",62900000,1672.66,8430133581763,"https://galagar.com/wp-content/uploads/2022/01/Devanadora-D22C.jpg",{"$error":"#VALUE!"}]
[782,"Gala MIG 6007","43400000RKIT",9917.93,8430133809157,"https://galagar.com/wp-content/uploads/2022/01/Gala-MIG-6007-Dev.jpg",{"$error":"#VALUE!"}]
[783,"Antorcha MIG 501 - 4 metros","880501P",244.79,8430133652821]
[784,"Estuche consumibles para antorcha MIG","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[785,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[786,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[787,"Líquido refrigerante 10 litros",39200094,112.47,8430133658298,"https://galagar.com/wp-content/uploads/2022/07/Refrigerante.jpg",{"$error":"#VALUE!"}]
[788,"Ver catálogo consumibles hilo Página 103"]
[789,"Kit voltímetro + amperímetro digital",43981075,426.12,8430133439750]
[790,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[791,"Antorcha MIG 501 - 3 metros (para aluminio)","M503000",301.19,8430133801502]
[792,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[793,"Ruleta U Ø30 mm. 1.0-1.2 mm. (para aluminio) x2",62006021,27.43,8430133763442]
[794,"Ruleta U Ø30 mm. 1.2-1.6 mm. (para aluminio) x2",62006022,27.43,8430133723279]
[795,"Ruleta tubular Ø30 mm. 1.2-1.6 mm. x2",62006015,30.38,8430133723231]
[796,"Ruleta V Ø30 mm. 1.2-1.6 mm. x2",62006020,27.43,8430133723262]
[797,"10 metros conexión devanadora refrigerado",63981000,812.72,8430133402921]
[798,"15 metros conexión devanadora refrigerado",63983000,1283.73,8430133766139]
[799,"20 metros conexión devanadora refrigerado",63982000,2000.11,8430133403171]
[800,"GPS 2300 BI-Pulse (equipo + cable masa + tubo gas + ruleta Ø 37 mm. 0.8-1.0 - x2)",53200000,2850,8430133584986,"https://galagar.com/wp-content/uploads/2022/07/GPS2300-BiPulse.jpg",{"$error":"#VALUE!"}]
[801,"Antorcha MIG 400 Autorefrigerada - 4 metros","PK4012",253.26,8430133663902,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-400.jpg",{"$error":"#VALUE!"}]
[802,"Estuche consumibles para antorcha MIG 400","EMIGPK400",160.21,8430133804510,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG400.jpg",{"$error":"#VALUE!"}]
[803,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[804,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[805,"Estación de trabajo",51712090,"CONSULTAR",8430133404994,"https://galagar.com/wp-content/uploads/2022/01/EstacionTrabajo.jpg",{"$error":"#VALUE!"}]
[806,"Ruleta Ø 37 mm. 1.0-1.2 aluminio - x2",51716523,46.44,8430133570491]
[807,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[808,"Ver catálogo consumibles hilo Página 103"]
[809,"Antorcha TIG SR26 Euro - 4 metros","T264030",354.36,8430133803957,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[810,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[811,"GPS 4000C Compacta Advanced (equipo + cable masa + tubo gas)",42384000,"CONSULTAR",8430133668105,"https://galagar.com/wp-content/uploads/2022/01/GPS-3000y4000C-Refrigerada.jpg",{"$error":"#VALUE!"}]
[812,"Antorcha MIG 400 Autorefrigerada - 4 metros","PK4012",253.26,8430133663902,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-400.jpg",{"$error":"#VALUE!"}]
[813,"Estuche consumibles para antorcha MIG 400","EMIGPK400",160.21,8430133804510,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG400.jpg",{"$error":"#VALUE!"}]
[814,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[815,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[816,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[817,"Ruleta U (aluminio) Ø 37 mm. 1.0-1.2 mm. (x2)",42316127,27.43,8430133609924]
[818,"Montaje y prueba del equipo","GMT",184.65,8430133809171]
[819,"Ver catálogo consumibles hilo Página 103"]
[820,"GPS 4000C Compacta Advanced REFRIGERADA (cable masa + tubo gas)","42384000-RKIT","CONSULTAR"]
[821,"Antorcha MIG 500W Refrigerada doble circuito - 4 metros","PK555040",541.27,8430133661588,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-500W.jpg",{"$error":"#VALUE!"}]
[822,"Estuche consumibles para antorcha MIG 501","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[823,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[824,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[825,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[826,"Ruleta U Ø 37 mm. 1.0-1.2 mm. (para aluminio) x2",42316127,27.43,8430133609924]
[827,"Montaje y prueba del equipo","GMT",184.65,8430133809171]
[828,"Ver catálogo consumibles hilo Página 103"]
[829,"Adicionales para GPS 4000C Compacta Advanced"]
[830,"Software doble arco-pulsado MIG",42370011,"CONSULTAR",8430133671785]
[831,"Software TIG pulsado",42370020,"CONSULTAR",8430133719999]
[832,"Solfware TIG con aportación de hilo frío",66790000,"CONSULTAR",8430133661731]
[833,"Solfware doble arco estándar / bi-level","------","CONSULTAR"]
[834,"Kit de conexión Telenet -interface-",42612081,"CONSULTAR",8430133675400]
[835,"Kit de conexión a PC -back up-",42612090,"CONSULTAR",8430133675417]
[836,"Mando a distancia (requiere telenet)",66012085,"CONSULTAR",8430133676124]
[837,"Ruleta V Ø 37 mm. 0.8-1.0 mm.",42316121,27.43,8430133609863]
[838,"Ruleta V Ø 37 mm. 1.2-1.6 mm.",42316124,27.43,8430133609894]
[839,"Ruleta R (tubular) Ø 37 mm. 1.2-1.6 mm.",42316125,27.43,8430133609900]
[840,"Ruleta R (tubular) Ø 37 mm. 1.2-1.6 mm.",42316126,27.43,8430133609917]
[841,"Ruleta U (aluminio) Ø 37 mm. 1.2-1.6 mm.",42316128,27.43,8430133609931]
[842,"Kit de conversión de pantalla LCD a TFT / necesario para uso de programas especiales",null,"CONSULTAR"]
[843,"Programa SCA COLD (reduccion 35% aporte térmico)",42370100,"CONSULTAR",8430133804060]
[844,"Programa ARC ROOT (soldadura de raiz)",42370095,"CONSULTAR",8430133811778]
[845,"Programa SPEED ARC (velocidad de desplazamiento 30%)",42370050,"CONSULTAR",8430133804664]
[846,"Programa POWER ARC (penetración 47%)",42370060,"CONSULTAR",8430133804688]
[847,"Programa SPEED ARC UP (velocidad soldadura ascendente)",42370055,"CONSULTAR",8430133804671]
[848,"Programa SPEED ARC UP PLUS (18 % sobre Speed up)",42770057,"CONSULTAR"]
[849,"Programa CEILING ARC (soldadura posición bajo techo)",42370065,"CONSULTAR",8430133811761]
[850,"Antorcha MIG 400 - 4 metros","PK4012",253.26,8430133663902,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-400.jpg",{"$error":"#VALUE!"}]
[851,"Estuche consumible para antorcha PK400","EMIGPK400",160.21,8430133804510,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG400.jpg",{"$error":"#VALUE!"}]
[852,"Antorcha MIG 500W Refrigerada doble circuito - 4 metros","PK555040",541.27,8430133661588,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-500W.jpg",{"$error":"#VALUE!"}]
[853,"Estuche consumibles para antorcha MIG 501","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[854,"Antorcha de TIG SR26 E - 4 metros","19052614P",173.55,8430133652869,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[855,"Antorcha de TIG SR18 E - 4 metros","19051814P",214.96,8430133652876,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[856,"Estuche consumibles para antorcha de TIG","ETIG",34.159999999999997,8430133682934,"https://galagar.com/wp-content/uploads/2022/01/Estuche_TIG.jpg",{"$error":"#VALUE!"}]
[857,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[858,"Pantalla electrónica automática 4-13 Galaxy especial TIG","51259B",170.1,8430133667641,"https://galagar.com/wp-content/uploads/2022/01/Galaxy_2.jpg"]
[859,"Afilador de tungstenos portátil","8044166-NT","CONSULTAR",8430133857264,null,{"$error":"#VALUE!"}]
[860,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[861,"Estufa porta electrodos","1704V10",303.73,8430133566418,"https://galagar.com/wp-content/uploads/2022/01/Estufa-DHF-5T.jpg",{"$error":"#VALUE!"}]
[862,"Calentador de gas Co2",600000,174.09,8430133800369,"https://galagar.com/wp-content/uploads/2022/01/Calentador-Co2_600000.jpg"]
[863,"GPS 4000 DR Advanced Sin Refrigeración (equipo + cable masa + tubo gas)","42381200-KIT","CONSULTAR",null,null,{"$error":"#VALUE!"}]
[864,"Antorcha MIG 500- 4 metros","PK5012",278.43,8430133663971,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-500.jpg",{"$error":"#VALUE!"}]
[865,"Estuche consumible para antorcha PK500","EMIGPK400",160.21,8430133804510,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG400.jpg",{"$error":"#VALUE!"}]
[866,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[867,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[868,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[869,"Ruleta U Ø 37 mm. 1.0-1.2 mm. (para aluminio) x2",42316127,27.43,8430133609924]
[870,"Montaje y prueba del equipo","GMT",184.65,8430133809171]
[871,"Ver catálogo consumibles hilo Página 103"]
[872,"GPS 4000 DR Advanced REFRIGERADA (cable masa + tubo de gas + INCLUIDOS)","42381200-RKIT","CONSULTAR"]
[873,"GPS 5000 DR Advanced REFRIGERADA (cable masa + tubo de gas + INCLUIDOS)","42600200-RKIT","CONSULTAR"]
[874,"Antorcha MIG 500W - 4 metros","PK555040",541.27,8430133661588,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-500W.jpg",{"$error":"#VALUE!"}]
[875,"Estuche consumibles para antorcha MIG 501","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[876,"Pantalla electrónica con visión en color Gasweld DARK","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[877,"Regulador EN-2000 Argón-Co2",37600000,133.13,8430133577834,"https://galagar.com/wp-content/uploads/2022/01/EN2000-ARg.jpg",{"$error":"#VALUE!"}]
[878,"Sirga de grafito (para aluminio)",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[879,"Ruleta U Ø 37 mm. 1.0-1.2 mm. (para aluminio) x2",42316127,27.43,8430133609924]
[880,"Montaje y prueba del equipo","GMT",184.65,8430133809171]
[881,"Ver catálogo consumibles hilo Página 103"]
[882,"Adicionales para GPS 4000/5000 DR Advanced Modular"]
[883,"Software doble arco-pulsado MIG",42370011,"CONSULTAR",8430133671785]
[884,"Software pulsado TIG",42370020,"CONSULTAR",8430133719999]
[885,"Solfware TIG con aportación de hilo frío",66790000,"CONSULTAR",8430133661731]
[886,"Solfware doble arco estándar / bi-level",null,"CONSULTAR"]
[887,"Kit de conexión Telenet -interface-",42612081,"CONSULTAR",8430133675400]
[888,"Kit de conexión a PC -back up-",42612090,"CONSULTAR",8430133675417]
[889,"Mando a distancia (requiere telenet)",66012085,"CONSULTAR",8430133676124]
[890,"Ruleta V Ø 37 mm. 0.8-1.0 mm.",42316121,27.43,8430133609863]
[891,"Ruleta V Ø 37 mm. 1.2-1.6 mm.",42316124,27.43,8430133609894]
[892,"Ruleta R (tubular) Ø 37 mm. 1.2-1.6 mm.",42316125,27.43,8430133609900]
[893,"Ruleta R (tubular) Ø 37 mm. 1.2-1.6 mm.",42316126,27.43,8430133609917]
[894,"Ruleta U (aluminio) Ø 37 mm. 1.2-1.6 mm.",42316128,27.43,8430133609931]
[895,"Juego de cables 10 metros aire",64187200,"CONSULTAR",8430133615734]
[896,"Juego de cables 15 metros aire",64187300,"CONSULTAR",8430133615741]
[897,"Juego de cables 10 metros refrigerado",64187250,"CONSULTAR",8430133615758]
[898,"Juego de cables 15 metros refrigerado",64187350,"CONSULTAR",8430133615765]
[899,"Programa SCA COLD (reduccion 35% aporte termico)",42370100,"CONSULTAR",8430133804060]
[900,"Programa ARC ROOT (soldadura de raiz)",42370095,"CONSULTAR",8430133811778]
[901,"Programa SPEED ARC (velocidad de desplazamiento 30%)",42370050,"CONSULTAR",8430133804664]
[902,"Programa POWER ARC (penetración 47%)",42370060,"CONSULTAR",8430133804688]
[903,"Programa SPEED ARC UP (velocidad soldadura ascendente)",42370055,"CONSULTAR",8430133804671]
[904,"Programa SPEED ARC UP PLUS (18 % sobre Speed up)",42770057,"CONSULTAR"]
[905,"Programa CEILING ARC (soldadura posición bajo techo)",42370065,"CONSULTAR",8430133811761]
[906,"Antorcha MIG 400 Autorefrigerada - 4 metros","PK4012",253.26,8430133663902,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-400.jpg",{"$error":"#VALUE!"}]
[907,"Estuche consumibles para antorcha MIG 400","EMIGPK400",160.21,8430133804510,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG400.jpg",{"$error":"#VALUE!"}]
[908,"Antorcha MIG 500W Refrigerada doble circuito - 4 metros","PK555040",541.27,8430133661588,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-500W.jpg",{"$error":"#VALUE!"}]
[909,"Estuche consumibles para antorcha MIG 501","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[910,"Antorcha de TIG SR26 Euro - 4 metros","T264030",354.36,8430133803957,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[911,"Antorcha de TIG SR18 Euro - 4 metros","T184030",436.34,8430133808402,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[912,"Estuche consumibles para antorcha de TIG","ETIG",34.159999999999997,8430133682934,"https://galagar.com/wp-content/uploads/2022/01/Estuche_TIG.jpg",{"$error":"#VALUE!"}]
[913,"Caja de tungstenos negro Ø 2,4 mm.","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[914,"Pantalla electrónica automática 4-13 Galaxy","51259B",170.1,8430133667641,"https://galagar.com/wp-content/uploads/2022/01/Galaxy_2.jpg",{"$error":"#VALUE!"}]
[915,"Ver catálogo consumibles varilla para TIG Página 103"]
[916,"Afilador de tungstenos portátil","8044166-NT","CONSULTAR",8430133857264]
[917,"Válvula economizadora de gas",35500000,96.46,8430133577575,"https://galagar.com/wp-content/uploads/2022/01/Valvula-ECO-Fija.jpg",{"$error":"#VALUE!"}]
[918,"Estufa porta electrodos","1704V10",303.73,8430133566418,"https://galagar.com/wp-content/uploads/2022/01/Estufa-DHF-5T.jpg",{"$error":"#VALUE!"}]
[919,"Calentador de gas Co2",600000,174.09,8430133800369,"https://galagar.com/wp-content/uploads/2022/01/Calentador-Co2_600000.jpg",{"$error":"#VALUE!"}]
[920,"Gala SPOT 30 mecánica",29080001,"CONSULTAR",8430133565367,"https://galagar.com/wp-content/uploads/2022/05/Spot-Neu_Mecanica-1.jpg",{"$error":"#VALUE!"}]
[921,"Gala SPOT 30 neumática",29080002,"CONSULTAR",8430133565374,"https://galagar.com/wp-content/uploads/2022/05/Spot-Neu.jpg",{"$error":"#VALUE!"}]
[922,"Gala SPOT 50 mecánica",29080003,"CONSULTAR",8430133565381,"https://galagar.com/wp-content/uploads/2022/05/Spot-Neu_Mecanica-1.jpg",{"$error":"#VALUE!"}]
[923,"Gala SPOT 50 neumática",29080004,"CONSULTAR",8430133565398,"https://galagar.com/wp-content/uploads/2022/05/Spot-Neu.jpg",{"$error":"#VALUE!"}]
[924,"Brazos 600 mm (x2)",2910004,"CONSULTAR",8430133804534,"https://galagar.com/wp-content/uploads/2022/05/Brazo-GalaSpot.jpg",{"$error":"#VALUE!"}]
[925,"Brazos 750 mm (x2)",2910800,"CONSULTAR",8430133804541,"https://galagar.com/wp-content/uploads/2022/05/Brazo-GalaSpot.jpg",{"$error":"#VALUE!"}]
[926,"Brazos 1000 mm (x2)",29100100,"CONSULTAR",8430133817596,"https://galagar.com/wp-content/uploads/2022/05/Brazo-GalaSpot.jpg",{"$error":"#VALUE!"}]
[927,"Módulo de refrigeración",63400000,"CONSULTAR",8430133540920,"https://galagar.com/wp-content/uploads/2022/05/Refrigeracion-WCS.jpg"]
[928,"Instalación módulo refrigeración","--------","CONSULTAR",null,null,{"$error":"#VALUE!"}]
[929,"Punto 20x47 estándar CuCrZr",29090001,"CONSULTAR",8430133565404,"https://galagar.com/wp-content/uploads/2022/05/PortaCapsulas-GalaSpot.jpg",{"$error":"#VALUE!"}]
[930,"Punto 20x50 excéntrico CuCrZr",29090006,"CONSULTAR",8430133565459,"https://galagar.com/wp-content/uploads/2022/05/PortaCapsulas-GalaSpot.jpg",{"$error":"#VALUE!"}]
[931,"Punto 20x90 larga",29090002,"CONSULTAR",8430133565411,"https://galagar.com/wp-content/uploads/2022/05/PortaCapsulas-GalaSpot.jpg",{"$error":"#VALUE!"}]
[932,"Punto 25x50 largo rótula",29090003,"CONSULTAR",8430133565428,"https://galagar.com/wp-content/uploads/2022/05/PortaCapsulas-GalaSpot.jpg",{"$error":"#VALUE!"}]
[933,"Punto 20x50 plana","29090003.1","CONSULTAR",8430133804558,"https://galagar.com/wp-content/uploads/2022/05/PortaCapsulas-GalaSpot.jpg",{"$error":"#VALUE!"}]
[934,"Punto 30x50x74x5 tubo exterior",29090005,"CONSULTAR",8430133565442,"https://galagar.com/wp-content/uploads/2022/05/PortaCapsulas-GalaSpot.jpg",{"$error":"#VALUE!"}]
[935,"Punto 20x50 tubo interior Ø 60 mm.",29090004,"CONSULTAR",8430133565435,"https://galagar.com/wp-content/uploads/2022/05/PortaCapsulas-GalaSpot.jpg"]
[936,"Punto cápsula forma A Ø 13 mm.",29090030,"CONSULTAR",8430133681777]
[937,"Punto cápsula forma B Ø 13 mm.",29090034,"CONSULTAR",8430133774059]
[938,"Punto cápsula forma C Ø 13 mm.","290900C13","CONSULTAR",8430133804572]
[939,"Punto cápsula forma D Ø 13 mm.","290900D13","CONSULTAR",8430133804589]
[940,"Punto cápsula forma E Ø 13 mm.","290900E13","CONSULTAR"]
[941,"Punto cápsula forma F Ø 13 mm.","290900F13","CONSULTAR",8430133804619]
[942,"Punto cápsula forma G Ø 13 mm.","290900G13","CONSULTAR",8430133804626]
[943,"Punto cápsula forma A Ø 16 mm.",29090023,"CONSULTAR",8430133672409]
[944,"Punto cápsula forma B Ø 16 mm.","290900B16","CONSULTAR",8430133804565]
[945,"Punto cápsula forma C Ø 16 mm.",29090028,"CONSULTAR",8430133674243]
[946,"Punto cápsula forma D Ø 16 mm.","290900D16","CONSULTAR",8430133804596]
[947,"Punto cápsula forma E Ø 16 mm.",29090032,"CONSULTAR",8430133774035]
[948,"Punto cápsula forma F Ø 16 mm.",29090024,"CONSULTAR",8430133672416]
[949,"Punto cápsula forma G Ø 16 mm.","290900G16","CONSULTAR",8430133804633,null,{"$error":"#VALUE!"}]
[950,"Gala ARC 1000",3005258,"CONSULTAR",8430133682675,"https://galagar.com/wp-content/uploads/2022/01/GalaARC-1000.jpg",{"$error":"#VALUE!"}]
[951,"Pinza arco aire ARC-AIR K4000 con cable 2 m.",61082008,1213.03,8430133679705]
[952,"Cable pinza ARC-AIR (10 m. / 70 mm. 2 / CN 95-120)",43412030,302.68,8430133678722]
[953,"Gala ARC 1500","3005152THT","CONSULTAR",8430133681869,"https://galagar.com/wp-content/uploads/2022/01/THT152_ARC_pq.jpg",{"$error":"#VALUE!"}]
[954,"Pinza arco aire ARC-AIR K5000 con cable 2 m.",61104008,1352.24,8430133680169]
[955,"Cable pinza ARC-AIR (10 m. / 70 mm. 2 / CN 95-120)",43412030,302.68,8430133678722]
[956,"Devanadora D-12 A",61800000,1120.97,8430133402808,"https://galagar.com/wp-content/uploads/2022/01/Devanadora-D12A.jpg",{"$error":"#VALUE!"}]
[957,"Devanadora D-20 A",62100000,1442.78,8430133402815,"https://galagar.com/wp-content/uploads/2022/01/Devanadora-D20-A.jpg",{"$error":"#VALUE!"}]
[958,"Devanadora D-20 AR",62200000,1532.25,8430133579340,"https://galagar.com/wp-content/uploads/2022/01/Devanadora-D20-AR.jpg",{"$error":"#VALUE!"}]
[959,"Devanadora D-22 C",62900000,1672.66,8430133581763,"https://galagar.com/wp-content/uploads/2022/01/Devanadora-D22C.jpg",{"$error":"#VALUE!"}]
[960,"Devanadora D-20 C",62300000,1597.7,8430133353148]
[961,"Devanadora D-GPS 21A (¡Nueva!)",66082100,1962.16,8430133675844,"https://galagar.com/wp-content/uploads/2024/04/Devandora-D-GPS_Web.jpg",{"$error":"#VALUE!"}]
[962,"Devanadora D-4R i (¡Nueva!)",66800000,1151.96,8430133802738]
[963,"Accesorios para electrodos - 300 A -10/25",56612033,97.9,8430133305635,"https://galagar.com/wp-content/uploads/2022/01/ACC-Atlantic.jpg",{"$error":"#VALUE!"}]
[964,"Accesorios para electrodos - 300 A - 35/50",259040,103.67,8430133400026,"https://galagar.com/wp-content/uploads/2022/01/ACC-Atlantic.jpg",{"$error":"#VALUE!"}]
[965,"Accesorios para electrodos - 400 A - 35/50",259048,142.07,8430133604813,"https://galagar.com/wp-content/uploads/2022/01/ACC-Atlantic.jpg",{"$error":"#VALUE!"}]
[966,"Accesorios para electrodos - 500 A - 35/50",259049,172.58,8430133604820,"https://galagar.com/wp-content/uploads/2022/01/ACC-Atlantic.jpg",{"$error":"#VALUE!"}]
[967,"Pinza portaelectrodo abierta - 200 A",68500000,7.18,8430133767051,"https://galagar.com/wp-content/uploads/2022/01/Pinza_68500000.jpg",{"$error":"#VALUE!"}]
[968,"Pinza portaelectrodo abierta - 400 A",67100000,12.01,8430133305802,"https://galagar.com/wp-content/uploads/2022/01/Pinza_68500000.jpg",{"$error":"#VALUE!"}]
[969,"Pinza portaelectrodo abierta - 600 A",68200000,15.88,8430133305888,"https://galagar.com/wp-content/uploads/2022/01/Pinza_68500000.jpg",{"$error":"#VALUE!"}]
[970,"Pinza portaelectrodo cerrada - 400 A",67000000,13.26,8430133305796,"https://galagar.com/wp-content/uploads/2022/01/Pinza_68600000.jpg",{"$error":"#VALUE!"}]
[971,"Pinza portaelectrodo cerrada - 600 A",68600000,18.23,8430133305895,"https://galagar.com/wp-content/uploads/2022/01/Pinza_68600000.jpg",{"$error":"#VALUE!"}]
[972,"Piqueta de acero reforzada",67400010,4.83,8430133766788,"https://galagar.com/wp-content/uploads/2022/05/Piqueta.jpg",{"$error":"#VALUE!"}]
[973,"Cepillo de puas de acero",67700000,4.83,8430133766948,"https://galagar.com/wp-content/uploads/2022/05/Cepillo.jpg",{"$error":"#VALUE!"}]
[974,"Toma de masa Micro - 200 A",67300020,3.92,8430133766764,"https://galagar.com/wp-content/uploads/2022/01/Cincada-Micro.jpg",{"$error":"#VALUE!"}]
[975,"Toma de masa Normal - 400 A",67300000,6.62,8430133305819,"https://galagar.com/wp-content/uploads/2022/01/Cincada-Normal.jpg",{"$error":"#VALUE!"}]
[976,"Toma masa - 500 A",67300500,8.56,8430133305833,"https://galagar.com/wp-content/uploads/2022/01/Cincada-500.jpg",{"$error":"#VALUE!"}]
[977,"Toma de masa Mini - 300 A",68000000,4.55,8430133305864,"https://galagar.com/wp-content/uploads/2022/01/Tornillo-Mini.jpg",{"$error":"#VALUE!"}]
[978,"Toma de masa Gar - 500 A",68100000,9.69,8430133767020,"https://galagar.com/wp-content/uploads/2022/01/Tornillo-GAR.jpg",{"$error":"#VALUE!"}]
[979,"Toma masa de tornillo - 600 A",98100600,17.25,8430133839932]
[980,"Escuadra hasta 12 Kg. de peso - 82x117x14 mm. (¡Nueva!)",700525,5.5,8430133838928,"https://galagar.com/wp-content/uploads/2025/03/Escuadra_Conjunto.jpg",{"$error":"#VALUE!"}]
[981,"Escuadra hasta 22 Kg. de peso - 102x155x16 mm.  (¡Nueva!)",700550,8.9,8430133838379,"https://galagar.com/wp-content/uploads/2025/03/Escuadra_Conjunto.jpg",{"$error":"#VALUE!"}]
[982,"Escuadra hasta 33 Kg. de peso - 122x190x24 mm.  (¡Nueva!)",700575,12,8430133838386,"https://galagar.com/wp-content/uploads/2025/03/Escuadra_Conjunto.jpg",{"$error":"#VALUE!"}]
[983,"Soporte para antorchas magnético - 94x110x130 mm. (¡Nuevo!)",700500,10.25,8430133838362,"https://galagar.com/wp-content/uploads/2025/03/Escuadra_Conjunto.jpg"]
[984,"Cable soldadura goma 1x16 mm2",130032,"CONSULTAR",8430133569297,"https://galagar.com/wp-content/uploads/2022/01/Cable-Goma.jpg",{"$error":"#VALUE!"}]
[985,"Cable soldadura goma 1x25 mm2",130034,"CONSULTAR",8430133569303]
[986,"Cable soldadura goma 1x35 mm2",130035,"CONSULTAR",8430133569310]
[987,"Cable soldadura goma 1x50 mm2",130037,"CONSULTAR",8430133569327]
[988,"Cable soldadura goma 1x70 mm2",130038,"CONSULTAR",8430133569334]
[989,"Cable soldadura goma 1x95 mm2",130040,"CONSULTAR",8430133552312]
[990,"Cable soldadura acrílico 1x16 mm2",130042,"CONSULTAR",8430133345426,"https://galagar.com/wp-content/uploads/2022/01/Cable-Acrilico.jpg",{"$error":"#VALUE!"}]
[991,"Cable soldadura acrílico 1x25 mm2",130044,"CONSULTAR",8430133569259]
[992,"Cable soldadura acrílico 1x35 mm2",130045,"CONSULTAR",8430133569266]
[993,"Cable soldadura acrílico 1x50 mm2",130047,"CONSULTAR",8430133569273]
[994,"Cable soldadura acrílico 1x70 mm2",130048,"CONSULTAR",8430133569280]
[995,"Cable soldadura acrílico 1x95 mm2",130095,"CONSULTAR",8430133570118]
[996,"Conector a panel hembra 10-25",58416024,3.52,8430133720131,"https://galagar.com/wp-content/uploads/2022/01/Conectores-Maquinas-10-25.jpg",{"$error":"#VALUE!"}]
[997,"Conector a panel hembra 35-50",47716035,6.27,8430133775179,"https://galagar.com/wp-content/uploads/2022/01/Conectores-Maquinas-35-50.jpg",{"$error":"#VALUE!"}]
[998,"Conector a panel hembra 70-95",42616035,12.8,8430133672454,"https://galagar.com/wp-content/uploads/2022/07/Conector-70-95.jpg",{"$error":"#VALUE!"}]
[999,"Conector hembra panel 95-120 mm2",43416035,32.39,8430133781422,"https://galagar.com/wp-content/uploads/2022/07/Conector-95-120.jpg",{"$error":"#VALUE!"}]
[1000,"Empalme 10-25 hembra",60400000,5.65,8430133579302,"https://galagar.com/wp-content/uploads/2022/01/Hembra.jpg",{"$error":"#VALUE!"}]
[1001,"Empalme 35-50 hembra",60500000,6.27,8430133579319,"https://galagar.com/wp-content/uploads/2022/01/Hembra.jpg",{"$error":"#VALUE!"}]
[1002,"Empalme rápido 50-70 hembra",60600000,9.0399999999999991,8430133352479,"https://galagar.com/wp-content/uploads/2022/01/Hembra.jpg",{"$error":"#VALUE!"}]
[1003,"Empalme rápido 70-95 hembra",60800000,14.56,8430133775322,"https://galagar.com/wp-content/uploads/2022/01/Hembra.jpg",{"$error":"#VALUE!"}]
[1004,"Empalme 10-25 macho",58416328,5.65,8430133579173,"https://galagar.com/wp-content/uploads/2022/01/Macho.jpg",{"$error":"#VALUE!"}]
[1005,"Empalme 35-50 macho",47716036,6.27,8430133578244,"https://galagar.com/wp-content/uploads/2022/01/Macho.jpg",{"$error":"#VALUE!"}]
[1006,"Empalme 50-70 macho",60700000,9.0399999999999991,8430133352486,"https://galagar.com/wp-content/uploads/2022/01/Macho.jpg",{"$error":"#VALUE!"}]
[1007,"Empalme 70-95 macho",60900000,14.56,8430133352516,"https://galagar.com/wp-content/uploads/2022/01/Macho.jpg",{"$error":"#VALUE!"}]
[1008,"Empalme 95-120 macho",63987036,38.200000000000003,8430133825775,"https://galagar.com/wp-content/uploads/2022/01/Macho.jpg",{"$error":"#VALUE!"}]
[1009,"Spray antiproyecciones sin silicona","3003M",6.15,8430133671365,"https://galagar.com/wp-content/uploads/2022/05/Spray-Antiproyecc.jpg",{"$error":"#VALUE!"}]
[1010,"Spray antiproyecciones CERÁMICO",301920196,"CONSULTAR",8430133820503,"https://galagar.com/wp-content/uploads/2022/05/Spray-Antiproyecc.jpg",{"$error":"#VALUE!"}]
[1011,"Pasta decapante TS-K 2000 - 2 kg.","MP220002",61.5,8430133677510,"https://galagar.com/wp-content/uploads/2022/01/Decapante-2.jpg",{"$error":"#VALUE!"}]
[1012,"Líquido refrigerante antorcha - 10 Litros",39200094,112.47,8430133658298,"https://galagar.com/wp-content/uploads/2022/07/Refrigerante.jpg",{"$error":"#VALUE!"}]
[1013,"Estufa vertical TRC V10 con termómetro y termostato - 50-150º - 10 kg.","1704V10",303.73,8430133566418,"https://galagar.com/wp-content/uploads/2022/01/Estufa-DHF-5T.jpg",{"$error":"#VALUE!"}]
[1014,"Estufa vertical DHF-5T con termómetro y termostato - 50-300º - 5 kg.","1705V5",400.37,8430133605872,"https://galagar.com/wp-content/uploads/2022/01/Estufa-DHF-5T.jpg",{"$error":"#VALUE!"}]
[1015,"Horno de secado GE-24 normalizado hasta 200 Cº",1724000,4829.43,8430133399955,"https://galagar.com/wp-content/uploads/2022/01/HornoSecado.jpg",{"$error":"#VALUE!"}]
[1016,"Horno de secado GE-24 normalizado hasta 300 Cº",1724001,5523.11,8430133399962,"https://galagar.com/wp-content/uploads/2022/01/HornoSecado.jpg",{"$error":"#VALUE!"}]
[1017,"Horno de secado GE-24 normalizado hasta 400 Cº",1724002,6621.18,8430133399979,"https://galagar.com/wp-content/uploads/2022/01/HornoSecado.jpg",{"$error":"#VALUE!"}]
[1018,"Electrodos rutilo 2,00 x 350 mm.","23301620PQ","CONSULTAR",8430133835590]
[1019,"Electrodos rutilo 2,50 x 350 mm.","23301625PQ","CONSULTAR",8430133827687]
[1020,"Electrodos rutilo 3,25 x 350 mm.","23301632PQ","CONSULTAR",8430133679606,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[1021,"Electrodos rutilo 4,00 x 350 mm.","23301644PQ","CONSULTAR",8430133793609]
[1022,"Electrodos inoxidable 2,50 x 300 mm.","2331630025PQ","CONSULTAR",8430133788360,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[1023,"Electrodos inoxidable 3,25 x 350 mm.","2331632PQ","CONSULTAR",8430133777524,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[1024,"Electrodos inoxidable 34,00 x 350 mm.","2331640PQ","CONSULTAR",8430133743260,"https://galagar.com/wp-content/uploads/2022/01/Electrodos-Paquete.jpg",{"$error":"#VALUE!"}]
[1025,"Caja electrodo rutilo Gala-46 2,00 mm.","23301620C","CONSULTAR",8430133563578,"https://galagar.com/wp-content/uploads/2022/01/Caja-Electrodo_Galagar.jpg",{"$error":"#VALUE!"}]
[1026,"Caja electrodo rutilo Gala-46 2,50 mm.","23301625C","CONSULTAR",8430133563585,"https://galagar.com/wp-content/uploads/2022/01/Caja-Electrodo_Galagar.jpg",{"$error":"#VALUE!"}]
[1027,"Caja electrodo rutilo Gala-46 3,25 mm.","23301632C","CONSULTAR",8430133563592,"https://galagar.com/wp-content/uploads/2022/01/Caja-Electrodo_Galagar.jpg",{"$error":"#VALUE!"}]
[1028,"Caja electrodo rutilo Gala-46 4,00 mm.","23301644C","CONSULTAR",8430133568054,"https://galagar.com/wp-content/uploads/2022/01/Caja-Electrodo_Galagar.jpg",{"$error":"#VALUE!"}]
[1029,"Caja electrodo básico 2,5 mm.","23B5025C","CONSULTAR",8430133848491,"https://galagar.com/wp-content/uploads/2022/01/Caja-Electrodo_Galagar.jpg",{"$error":"#VALUE!"}]
[1030,"Caja electrodo básico 3,20 mm.","23B5032C","CONSULTAR",8430133540760,"https://galagar.com/wp-content/uploads/2022/01/Caja-Electrodo_Galagar.jpg",{"$error":"#VALUE!"}]
[1031,"Caja electrodo básico 4 mm.","23B5040C","CONSULTAR",8430133848538,"https://galagar.com/wp-content/uploads/2022/01/Caja-Electrodo_Galagar.jpg",{"$error":"#VALUE!"}]
[1032,"Bobina 15 kg. hilo Co2 capa-capa - Ø 0,8 mm.","B1081132","CONSULTAR",8430133605773,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_2.jpg",{"$error":"#VALUE!"}]
[1033,"Bobina 15 kg. hilo Co2 capa-capa - Ø 1,0 mm.","B1101132","CONSULTAR",8430133605742,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_2.jpg",{"$error":"#VALUE!"}]
[1034,"Bobina 15 kg. hilo Co2 capa-capa - Ø 1,2 mm.","B1121132","CONSULTAR",8430133605698,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_2.jpg",{"$error":"#VALUE!"}]
[1035,"Bobina 15 kg. hilo inoxidable 308 LSI - Ø 0,8 mm.","B108308","CONSULTAR",8430133605766,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_1.jpg",{"$error":"#VALUE!"}]
[1036,"Bobina 15 kg. hilo inoxidable 308 LSI - Ø 1,0 mm.","B110308","CONSULTAR",8430133605711,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_1.jpg",{"$error":"#VALUE!"}]
[1037,"Bobina 15 kg. hilo inoxidable 308 LSI - Ø 1,2 mm.","B112308","CONSULTAR",8430133605667,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_1.jpg",{"$error":"#VALUE!"}]
[1038,"Bobina 15 kg. hilo inoxidable 316 LSI - Ø 0,8 mm.","B108316","CONSULTAR",8430133605759,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_1.jpg",{"$error":"#VALUE!"}]
[1039,"Bobina 15 kg. hilo inoxidable 316 LSI - Ø 1,0 mm.","B110316","CONSULTAR",8430133605704,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_1.jpg",{"$error":"#VALUE!"}]
[1040,"Bobina 15 kg. hilo inoxidable 316 LSI - Ø 1,2 mm.","B112316","CONSULTAR",8430133605650,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_1.jpg",{"$error":"#VALUE!"}]
[1041,"Bobina 7 kg. hilo AISi 5 - Ø 1,0 mm.","B1101232","CONSULTAR",8430133605735,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_3.jpg",{"$error":"#VALUE!"}]
[1042,"Bobina 7 kg. hilo AISi 5 - Ø 1,2 mm.","B1121232","CONSULTAR",8430133605681,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_3.jpg",{"$error":"#VALUE!"}]
[1043,"Bobina 7 kg. hilo AlMg 5 - Ø 1,0 mm. (metálica)","B1101332M","CONSULTAR",8430133777357,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_3.jpg",{"$error":"#VALUE!"}]
[1044,"Bobina 7 kg. hilo AlMg 5 - Ø 1,2 mm. (metálica)","B1121332M","CONSULTAR",8430133681531,"https://galagar.com/wp-content/uploads/2022/01/Bobina-Hilo_3.jpg",{"$error":"#VALUE!"}]
[1045,"Marathon pack - Ø 1,0 bidón 250 kg.",1111132,"CONSULTAR",8430133424466,"https://galagar.com/wp-content/uploads/2023/07/Bidon-Hilo-1.jpg",{"$error":"#VALUE!"}]
[1046,"Marathon pack - Ø 1,2 bidón 250 kg.",1111232,"CONSULTAR",8430133424473,"https://galagar.com/wp-content/uploads/2023/07/Bidon-Hilo-1.jpg",{"$error":"#VALUE!"}]
[1047,"Cono guía de hilo Ø 520 mm.","WW10204C","CONSULTAR",8430133629267]
[1048,"Antorcha MIG 15 - 4 metros","880015P",90.94,8430133652791,"https://galagar.com/wp-content/uploads/2022/04/7xm-15.jpg",{"$error":"#VALUE!"}]
[1049,"Blister 3 uds. Tobera GM-15","5672B3",5.65,8430133589257,"https://galagar.com/wp-content/uploads/2022/11/Toberas-MIG15_5672B3.jpg",{"$error":"#VALUE!"}]
[1050,"Blister 10 uds. Tubo contacto GM-15 - Ø 0,6","6349B10",3.38,8430133589608,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG15_6349B10.jpg",{"$error":"#VALUE!"}]
[1051,"Blister 10 uds. Tubo contacto GM-15 - Ø 0,8","5670B10",3.79,8430133605223,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG15_6349B10.jpg",{"$error":"#VALUE!"}]
[1052,"Blister 10 uds. Tubo contacto GM-15 - Ø 1,0","6128B10",4.1399999999999997,8430133605247,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG15_6349B10.jpg",{"$error":"#VALUE!"}]
[1053,"Muelle sujeción tobera GM-15",5654,0.63,8430133339098,"https://galagar.com/wp-content/uploads/2022/11/Muelles-MIG15-25.jpg",{"$error":"#VALUE!"}]
[1054,"Sirga forrada azul 4 m. - Ø 0,6 - 1 mm.",6363,5.14,8430133339739,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Colores.jpg",{"$error":"#VALUE!"}]
[1055,"Cuello GM-15",5651,7.15,8430133339081,"https://galagar.com/wp-content/uploads/2022/01/Cuello_MIG15.jpg",{"$error":"#VALUE!"}]
[1056,"Cable coaxial goma 15 mm2 - 4 m.",99015,85.35,8430133541460,"https://galagar.com/wp-content/uploads/2022/01/Coaxial_4.jpg",{"$error":"#VALUE!"}]
[1057,"Empuñadura completa 7xm estándar","882514P",46.69,8430133683955]
[1058,"Micro interruptor 7xm","882516P",18.7,8430133683962]
[1059,"Conjunto conector","888015P",26.99,8430133683924]
[1060,"Estuche E-Mig 15","EMIG15",26.99,8430133744595,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG15.jpg",{"$error":"#VALUE!"}]
[1061,"Antorcha MIG 25 - 4 metros","880025P",120.67,8430133652807,"https://galagar.com/wp-content/uploads/2022/01/7xm-25.jpg",{"$error":"#VALUE!"}]
[1062,"Antorcha MIG 25 - 3 metros","8800253P",117.29,8430133785970,"https://galagar.com/wp-content/uploads/2022/01/7xm-25.jpg",{"$error":"#VALUE!"}]
[1063,"Antorcha MIG 25 - 5 metros","8800255P",125.19,8430133785963,"https://galagar.com/wp-content/uploads/2022/01/7xm-25.jpg",{"$error":"#VALUE!"}]
[1064,"Blister 3 uds. Tobera GM-25","880005B3",9.2799999999999994,8430133605261,"https://galagar.com/wp-content/uploads/2022/01/Toberas-MIG25_880005B3.jpg",{"$error":"#VALUE!"}]
[1065,"Blister 10 uds. Tubo contacto GM-25-36 (0,8 mm.) M6","6129B10",8.0299999999999994,8430133589271,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG25_6130B10.jpg",{"$error":"#VALUE!"}]
[1066,"Blister 10 uds. Tubo contacto GM-25-36 (1,0 mm.) M6","6130B10",5.9,8430133589295,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG25_6130B10.jpg",{"$error":"#VALUE!"}]
[1067,"Blister 10 uds. Tubo contacto GM-25-36 (1,2 mm.) M6","5693B10",6.15,8430133589301,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG25_6130B10.jpg",{"$error":"#VALUE!"}]
[1068,"Blister 5 uds. Portatubo M6 GM-25","6288B5",5.65,8430133589264,"https://galagar.com/wp-content/uploads/2022/11/PortaTubo-MIG25_6288B5.jpg"]
[1069,"Blister 5 uds. Muelle sujeción tobera GM-25",6330,0.63,8430133339654,null,{"$error":"#VALUE!"}]
[1070,"Sirga forrada roja 4 m. Ø 1-1,2 mm.",6137,5.14,8430133339487,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Roja.jpg",{"$error":"#VALUE!"}]
[1071,"Cuello GM-25",6331,15.32,8430133339661,"https://galagar.com/wp-content/uploads/2022/01/Cuello_MIG25.jpg",{"$error":"#VALUE!"}]
[1072,"Cable coaxial goma 25 mm2  4 m.",99025,"CONSULTAR",8430133541477,"https://galagar.com/wp-content/uploads/2022/01/Coaxial_4.jpg",{"$error":"#VALUE!"}]
[1073,"Empuñadura completa 7xm estándar","882514P",46.69,8430133683955]
[1074,"Micro interruptor 7xm","882516P",18.7,8430133683962]
[1075,"Conjunto conector","888016P",9.41,8430133683931]
[1076,"Sirga de grafito 4 m.",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[1077,"Estuche Emig-25","EMIG25",37.57,8430133682972,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG25.jpg",{"$error":"#VALUE!"}]
[1078,"Antorcha MIG 36 M6 - 4 metros","880036P",163.69,8430133652814,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[1079,"Antorcha MIG 36 M6 - 3 metros","8800363P",136.09,8430133786014,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[1080,"Antorcha MIG 36 M6 - 5 metros","8800365P",164.73,8430133786007,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[1081,"Blister 3 uds. - Tobera GM-36","5715B3",14.06,8430133589394,"https://galagar.com/wp-content/uploads/2022/01/Toberas_MIG36_5715B3.jpg",{"$error":"#VALUE!"}]
[1082,"Blister 10 uds. - Tubo contacto M6 - GM-25-36 Ø 0,8 mm.","6129B10",8.0299999999999994,8430133589271,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG25_6130B10.jpg",{"$error":"#VALUE!"}]
[1083,"Blister 10 uds. - Tubo contacto M6 - GM-25-36 Ø 1,0 mm.","6130B10",5.9,8430133589295,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG25_6130B10.jpg",{"$error":"#VALUE!"}]
[1084,"Blister 10 uds. - Tubo contacto M6 - GM-25-36 Ø 1,2 mm.","5693B10",6.15,8430133589301,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG25_6130B10.jpg",{"$error":"#VALUE!"}]
[1085,"Blister 5 uds. - Portatubo M6 - GM-36","5843B5",5.27,8430133589332,"https://galagar.com/wp-content/uploads/2022/11/PortaTubo-MIG36_5843B5.jpg",{"$error":"#VALUE!"}]
[1086,"Blister 5 uds. - Distrbuidor de gas M6 - GM-36","5827B5",3.14,8430133589325,"https://galagar.com/wp-content/uploads/2022/11/Difusores-MIG36_5827B5.jpg",{"$error":"#VALUE!"}]
[1087,"Difusor gas GM-36 especial",6475,3.38,8430133339807,"https://galagar.com/wp-content/uploads/2022/11/Difusor-Ceramica_MIG36.jpg",{"$error":"#VALUE!"}]
[1088,"Sirga forrada 4 m. - Amarilla Ø 1,2-1,6 mm.",6141,5.14,8430133339500,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Amarilla.jpg",{"$error":"#VALUE!"}]
[1089,"Cuello GM-36",5704,19.579999999999998,8430133339272,"https://galagar.com/wp-content/uploads/2022/01/Cuello_MIG36.jpg",{"$error":"#VALUE!"}]
[1090,"Cable coaxial MX36 4 m",99036,"CONSULTAR",8430133568023,"https://galagar.com/wp-content/uploads/2022/01/Coaxial_4.jpg",{"$error":"#VALUE!"}]
[1091,"Empuñadura completa 7xm estándar","882514P",46.69,8430133683955]
[1092,"Micro interruptor 7xm","882516P",18.7,8430133683962]
[1093,"Conjunto conector","888016P",9.41,8430133683931]
[1094,"Sirga de grafito 4 m.",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[1095,"Estuche E-Mig 36 M6","EMIG36M6",42.29,8430133683856,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG36-M6.jpg",{"$error":"#VALUE!"}]
[1096,"Antorcha MIG 36 M8 - 4 metros","880036P",163.69,8430133652814,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[1097,"Antorcha MIG 36 M8 - 3 metros","8800363P",136.09,8430133786014,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[1098,"Antorcha MIG 36 M8 - 5 metros","8800365P",164.73,8430133786007,"https://galagar.com/wp-content/uploads/2022/01/7xm-36.jpg",{"$error":"#VALUE!"}]
[1099,"Blister 3 uds. - Tobera GM-36","5715B3",14.06,8430133589394,"https://galagar.com/wp-content/uploads/2022/01/Toberas_MIG36_5715B3.jpg",{"$error":"#VALUE!"}]
[1100,"Blister 10 uds. - Tubo contacto M8 - GM-36 Ø 0,8 mm.","5741B10",12.27,8430133589356,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG36_6129B5.jpg",{"$error":"#VALUE!"}]
[1101,"Blister 10 uds. - Tubo contacto M8 - GM-36-501-500W Ø 1,0 mm.","6134B10",9.0399999999999991,8430133589363,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG501_6134B5.jpg",{"$error":"#VALUE!"}]
[1102,"Blister 10 uds. - Tubo contacto M8 - GM-36-501-500W Ø 1,2 mm.","6131B10",9.5399999999999991,8430133589370,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG501_6134B5.jpg",{"$error":"#VALUE!"}]
[1103,"Blister 5 uds. - Portatubo M8 - GM-36","5888B5",5.27,8430133589349,"https://galagar.com/wp-content/uploads/2022/11/PortaTubo-MIG36_5843B5.jpg",{"$error":"#VALUE!"}]
[1104,"Blister 5 uds. - Distrbuidor de gas M8 - GM-36","5827B5",3.14,8430133589325,"https://galagar.com/wp-content/uploads/2022/11/Difusores-MIG36_5827B5.jpg",{"$error":"#VALUE!"}]
[1105,"Difusor gas GM-36 especial",6475,3.38,8430133339807,"https://galagar.com/wp-content/uploads/2022/11/Difusor-Ceramica_MIG36.jpg",{"$error":"#VALUE!"}]
[1106,"Sirga forrada 4 m. - Amarilla Ø 1,2-1,6 mm.",6141,5.14,8430133339500,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Amarilla.jpg",{"$error":"#VALUE!"}]
[1107,"Cuello GM-36",5704,19.579999999999998,8430133339272,"https://galagar.com/wp-content/uploads/2022/01/Cuello_MIG36.jpg",{"$error":"#VALUE!"}]
[1108,"Cable coaxial MX36 4 m",99036,"CONSULTAR",8430133568023,"https://galagar.com/wp-content/uploads/2022/01/Coaxial_4.jpg"]
[1109,"Empuñadura completa 7xm estándar","882514P",46.69,8430133683955]
[1110,"Micro interruptor 7xm","882516P",18.7,8430133683962]
[1111,"Conjunto conector","888016P",9.41,8430133683931,null,{"$error":"#VALUE!"}]
[1112,"Sirga de grafito 4 m.",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[1113,"Estuche E-Mig 36 M8","EMIG36",50.64,8430133682989,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG36-M8.jpg"]
[1114,"Antorcha MIG 501 - 4 metros","880501P",244.79,8430133652821]
[1115,"Antorcha MIG 501 - 3 metros","8805013P",224.04,8430133785987,null,{"$error":"#VALUE!"}]
[1116,"Blister 3 uds. Tobera cónica M8-501","5875B3",15.57,8430133605230,"https://galagar.com/wp-content/uploads/2022/01/Tobera-MIG501_5875B3.jpgTobera-MIG501_5875B3.jpg",{"$error":"#VALUE!"}]
[1117,"Blister 10 uds. Tubo contacto M8 Ø 1,0 mm.","6134B10",9.0399999999999991,8430133589363,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG501_6134B5.jpg",{"$error":"#VALUE!"}]
[1118,"Blister 10 uds. Tubo contacto M8 Ø 1,2 mm.","6131B10",9.5399999999999991,8430133589370,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG501_6134B5.jpg",{"$error":"#VALUE!"}]
[1119,"Blister 10 uds. Tubo contacto M8 Ø 1,6 mm.","6135B10",9.67,8430133589387,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG501_6134B5.jpg",{"$error":"#VALUE!"}]
[1120,"Blister 5 uds. distribuidor M8-501","5858B5",2.89,8430133589400,"https://galagar.com/wp-content/uploads/2022/11/Difusores-MIG501_5858B5.jpg",{"$error":"#VALUE!"}]
[1121,"Difusor especial",88300570,1.51,8430133644413,"https://galagar.com/wp-content/uploads/2022/11/Difusor-Ceramica_MIG501.jpg",{"$error":"#VALUE!"}]
[1122,"Blister 5 uds. Porta-tubo M8 501","6347B5",8.16,8430133589431,"https://galagar.com/wp-content/uploads/2022/11/PortaTubo-MIG501_6347B5.jpg",{"$error":"#VALUE!"}]
[1123,"Aislante cuello 7xm 38 / 501",88305640,1,8430133644451,"https://galagar.com/wp-content/uploads/2022/01/ArandelaCuello_501-500W.jpg",{"$error":"#VALUE!"}]
[1124,"Sirga forrada 4 m. Amarilla Ø 1,2-1,6 mm.",6141,5.14,8430133339500,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Amarilla.jpg",{"$error":"#VALUE!"}]
[1125,"Cuello mb-501",5857,40.17,8430133581282,"https://galagar.com/wp-content/uploads/2022/01/Cuello_MIG501.jpg",{"$error":"#VALUE!"}]
[1126,"Conjunto cables completo 4 m.",88258414,"CONSULTAR",8430133644482,"https://galagar.com/wp-content/uploads/2022/01/Coaxial_4.jpg",{"$error":"#VALUE!"}]
[1127,"Empuñadura completa 7xm estándar","882514P",46.69,8430133683955]
[1128,"Micro interruptor 7xm","882516P",18.7,8430133683962]
[1129,"Conjunto conector","888016P",9.41,8430133683931]
[1130,"Sirga de grafito 4 m.",5722,17.57,8430133339326,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Grafito.jpg",{"$error":"#VALUE!"}]
[1131,"Estuche E-Mig 501","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[1132,"Antorcha MIG 400 - 4 metros","PK4012",253.26,8430133663902,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-400.jpg",{"$error":"#VALUE!"}]
[1133,"Tobera TR 400","PK401462",11.92,8430133663926,"https://galagar.com/wp-content/uploads/2022/01/Tobera-MIG400_PK401462.jpg",{"$error":"#VALUE!"}]
[1134,"Punta de contacto Ø 1,2 mm. TR 400","PK403145",1.51,8430133664008,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG400-500_PK403145.jpg",{"$error":"#VALUE!"}]
[1135,"Portatubo difusor TR 400","PK4043",7.15,8430133663940,"https://galagar.com/wp-content/uploads/2022/01/PortaTubo_MIG500x10.jpg",{"$error":"#VALUE!"}]
[1136,"Sirga amarilla 4,5 m.","PK41511615B",10.29,8430133821463]
[1137,"Cuello TR 400","PK40560",37.020000000000003,8430133663919,"https://galagar.com/wp-content/uploads/2022/01/Cuello-MIG400.jpg",{"$error":"#VALUE!"}]
[1138,"Conjunto cable 4 m. TR 400","PK41312",265.07,8430133672829,"https://galagar.com/wp-content/uploads/2022/01/Coaxial_4.jpg",{"$error":"#VALUE!"}]
[1139,"Empuñadura completa  MIG 400-500","PK30017K",11.04,8430133804855,"https://galagar.com/wp-content/uploads/2022/01/Empuniadura-MIG400-500.jpg",{"$error":"#VALUE!"}]
[1140,"Interruptor TR 400-500","PK4111",13.68,8430133665722,"https://galagar.com/wp-content/uploads/2022/01/Conmutador-MIG400-500.jpg",{"$error":"#VALUE!"}]
[1141,"KIT consumibles para antorcha MIG 400","EMIGPK400",160.21,8430133804510,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG400.jpg",{"$error":"#VALUE!"}]
[1142,"Antorcha MIG 500 - 4 metros","PK5012",278.43,8430133663971,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-500.jpg",{"$error":"#VALUE!"}]
[1143,"Tobera TR 500","PK401562",11.92,8430133663995,"https://galagar.com/wp-content/uploads/2022/01/Tobera-MIG500_PK401562.jpg",{"$error":"#VALUE!"}]
[1144,"Punta de contacto Ø 1,2 mm. TR 400","PK403145",1.51,8430133664008,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG400-500_PK403145.jpg",{"$error":"#VALUE!"}]
[1145,"Portatubo difusor TR 400","PK4043",7.15,8430133663940,"https://galagar.com/wp-content/uploads/2022/01/PortaTubo_MIG500x10.jpg",{"$error":"#VALUE!"}]
[1146,"Sirga amarilla 4,9 m.","PK41511615B",10.29,8430133821463]
[1147,"Cuello TR 500","PK50560",41.42,8430133663988,"https://galagar.com/wp-content/uploads/2022/01/Cuello-MIG500.jpg",{"$error":"#VALUE!"}]
[1148,"Cable coaxial 4 m. MIG 500","PK51312",331.34,8430133804862,"https://galagar.com/wp-content/uploads/2022/01/Coaxial_4.jpg",{"$error":"#VALUE!"}]
[1149,"Empuñadura completa  MIG 400-500","PK30017K",11.04,8430133804855,"https://galagar.com/wp-content/uploads/2022/01/Empuniadura-MIG400-500.jpg",{"$error":"#VALUE!"}]
[1150,"Interruptor TR 400-500","PK4111",13.68,8430133665722,"https://galagar.com/wp-content/uploads/2022/01/Conmutador-MIG400-500.jpg",{"$error":"#VALUE!"}]
[1151,"KIT consumibles para antorcha MIG 500","EMIGPK500",160.21,8430133824594,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG500.jpg",{"$error":"#VALUE!"}]
[1152,"Antorcha MIG 500W - 3 metros","PK555030",511.8,8430133679651,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-500W.jpg",{"$error":"#VALUE!"}]
[1153,"Antorcha MIG 500W - 4 metros","PK555040",541.27,8430133661588,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-500W.jpg",{"$error":"#VALUE!"}]
[1154,"Blister 3 uds. Tobera cónica M8-501","5875B3",15.57,8430133605230,"https://galagar.com/wp-content/uploads/2022/01/Tobera-MIG501_5875B3.jpgTobera-MIG501_5875B3.jpg",{"$error":"#VALUE!"}]
[1155,"Blister 10 uds. Tubo contacto M8 Ø 1,0 mm.","6134B10",9.0399999999999991,8430133589363,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG501_6134B5.jpg",{"$error":"#VALUE!"}]
[1156,"Blister 10 uds. Tubo contacto M8 Ø 1,2 mm.","6131B10",9.5399999999999991,8430133589370,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG501_6134B5.jpg",{"$error":"#VALUE!"}]
[1157,"Blister 10 uds. Tubo contacto M8 Ø 1,6 mm.","6135B10",9.67,8430133589387,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG501_6134B5.jpg",{"$error":"#VALUE!"}]
[1158,"Blister 5 uds. Difusor de gas M8-501","5858B5",2.89,8430133589400,"https://galagar.com/wp-content/uploads/2022/11/Difusores-MIG501_5858B5.jpg",{"$error":"#VALUE!"}]
[1159,"Difusor especial",88300570,1.51,8430133644413,"https://galagar.com/wp-content/uploads/2022/11/Difusor-Ceramica_MIG501.jpg",{"$error":"#VALUE!"}]
[1160,"Blister 5 uds. Porta Tubo M8-501","6347B5",8.16,8430133589431,"https://galagar.com/wp-content/uploads/2022/11/PortaTubo-MIG501_6347B5.jpg",{"$error":"#VALUE!"}]
[1161,"Aislante cuello 7xm 38 / 501",88305640,1,8430133644451,"https://galagar.com/wp-content/uploads/2022/01/ArandelaCuello_501-500W.jpg",{"$error":"#VALUE!"}]
[1162,"Sirga forrada 4 m. Amarilla Ø 1,2-1,6 mm.",6141,5.14,8430133339500,"https://galagar.com/wp-content/uploads/2022/01/Sirga-Amarilla.jpg",{"$error":"#VALUE!"}]
[1163,"Cuello completo 500W","PK5502",317.16000000000003,8430133672751,"https://galagar.com/wp-content/uploads/2022/01/Cuello-MIG500W.jpg",{"$error":"#VALUE!"}]
[1164,"Cable coaxial 4 m. MIG 500W","PK550640",363.84,8430133804992,"https://galagar.com/wp-content/uploads/2022/01/Coaxial_4.jpg",{"$error":"#VALUE!"}]
[1165,"Empuñadura completa MIG 500W-550W","PK2515",16.57,8430133804978,"https://galagar.com/wp-content/uploads/2022/01/Empuniadura-MIG500W-550W.jpg",{"$error":"#VALUE!"}]
[1166,"Conmutador MIG 500W","PK2516",13.68,8430133804985,"https://galagar.com/wp-content/uploads/2022/01/Conmutador-MIG500W-550W.jpg",{"$error":"#VALUE!"}]
[1167,"Estuche 501 Emig501","EMIG501",52.27,8430133682996,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG501-500W.jpg",{"$error":"#VALUE!"}]
[1168,"Antorcha MIG 550W - 4 metros","PK605040",552.9,8430133661625,"https://galagar.com/wp-content/uploads/2022/01/AntorchaMIG-550W.jpg",{"$error":"#VALUE!"}]
[1169,"Tobera cónica antorcha doble circuito 550W","PK6528",11.92,8430133661687,"https://galagar.com/wp-content/uploads/2022/11/Tobera-MIG550W_PK6528.jpg",{"$error":"#VALUE!"}]
[1170,"Adaptador tobera antorcha 550W","PK6515",8.5399999999999991,8430133661694,"https://galagar.com/wp-content/uploads/2022/11/PortaTobera-MIG550W_PK6515.jpg",{"$error":"#VALUE!"}]
[1171,"Tubo contacto 1,2 mm. para MIG 550W","PK601512",3.38,8430133661649,"https://galagar.com/wp-content/uploads/2022/01/TuboContacto-MIG550W_PK601512.jpg",{"$error":"#VALUE!"}]
[1172,"Difusor de gas para MIG 550W","PK6505",3.26,8430133661670,"https://galagar.com/wp-content/uploads/2022/01/Difusor_MIG550Wx5.jpg",{"$error":"#VALUE!"}]
[1173,"Porta tubo para MIG 550W","PK6501",12.55,8430133661663,"https://galagar.com/wp-content/uploads/2022/01/PortaTubo_MIG550Wx10.jpg",{"$error":"#VALUE!"}]
[1174,"Sirga de 4 m. para MIG 550W","PK503340","CONSULTAR",8430133805104,"https://galagar.com/wp-content/uploads/2022/11/SirgaDesnuda-MIG550W_PK503340.jpg",{"$error":"#VALUE!"}]
[1175,"Cuello completo 650","PK6502",302.33999999999997,8430133672775,"https://galagar.com/wp-content/uploads/2022/01/Cuello-MIG550W.jpg",{"$error":"#VALUE!"}]
[1176,"Cable coaxial 4 m. MIG 500W","PK550640",363.84,8430133804992,"https://galagar.com/wp-content/uploads/2022/01/Coaxial_4.jpg",{"$error":"#VALUE!"}]
[1177,"Empuñadura completa  MIG 550W","PK2515",16.57,8430133804978,"https://galagar.com/wp-content/uploads/2022/01/Empuniadura-MIG500W-550W.jpg",{"$error":"#VALUE!"}]
[1178,"Conmutador MIG 550W","PK2516",13.68,8430133804985,"https://galagar.com/wp-content/uploads/2022/01/Conmutador-MIG500W-550W.jpg",{"$error":"#VALUE!"}]
[1179,"KIT conusmibles para 550W","EMIGPK550W",381.9,8430133805005,"https://galagar.com/wp-content/uploads/2022/01/Estuche_MIG550W.jpg",{"$error":"#VALUE!"}]
[1180,"Antorcha TIG SR 17 V - 4 m. conector 35/50 mm.","T174100",108.54,8430133786670]
[1181,"Antorcha TIG SR 26 V - 4 m. conector 35/50 mm.","19052604P",173.55,8430133652852,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[1182,"Antorcha TIG SR 17 V - 8 m. conector 35/50 mm.","T178100",179.49,8430133787141,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[1183,"Antorcha TIG SR 26 V - 8 m. conector 35/50 mm.","T268100",314.7,8430133808327,"https://galagar.com/wp-content/uploads/2022/01/SR-18v.jpg",{"$error":"#VALUE!"}]
[1184,"Cuerpo estándar antorcha XT 17 V",190520201,33.64,8430133627478,"https://galagar.com/wp-content/uploads/2022/01/Cuello-TIG-17V.jpg",{"$error":"#VALUE!"}]
[1185,"Cuerpo estandar antorcha XT 26 V",190520601,33.64,8430133603823,"https://galagar.com/wp-content/uploads/2022/01/Cuello-TIG-26V.jpg",{"$error":"#VALUE!"}]
[1186,"Válvula XT - 9 /17",19500370,6.15,8430133643522,"https://galagar.com/wp-content/uploads/2022/01/Valvula-TIG_1.jpg",{"$error":"#VALUE!"}]
[1187,"Válvula XT - 26",19500372,6.15,8430133643690,"https://galagar.com/wp-content/uploads/2022/01/Valvula-TIG_1.jpg",{"$error":"#VALUE!"}]
[1188,"Empuñadura y micro XT-17",19051744,47.57,8430133569952,"https://galagar.com/wp-content/uploads/2022/01/EmpuTIG_1.jpg",{"$error":"#VALUE!"}]
[1189,"Empuñadura y micro XT-26",19052644,59.12,8430133569969,"https://galagar.com/wp-content/uploads/2022/01/EmpuTIG_1.jpg",{"$error":"#VALUE!"}]
[1190,"Cable potencia / gas 4 m. 1/4” SR17","19S20000421",132.91,8430133645793,"https://galagar.com/wp-content/uploads/2022/01/Coaxial-TIG_1.jpg",{"$error":"#VALUE!"}]
[1191,"Cable potencia / gas 4 m. 1/4” SR26","19S70000421",179.36,8430133647902,"https://galagar.com/wp-content/uploads/2022/01/Coaxial-TIG_1.jpg"]
[1192,"Antorcha TIG SR 17 electroválvula - 4 m. conector 35/50 mm.","T174000",134.52000000000001,8430133815769,null,{"$error":"#VALUE!"}]
[1193,"Antorcha TIG SR 26 electroválvula - 4 m. conector 35/50 mm.","19052614P",173.55,8430133652869,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1194,"Antorcha TIG SR 18 electroválvula - 4 m. conector 35/50 mm. Refrigerada","19051814P",214.96,8430133652876,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1195,"Antorcha TIG SR 17 electroválvula - 8 m. conector 35-50 mm.","T178000",221.4,8430133808334,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1196,"Antorcha TIG SR 26 electrovalvula - 8 m. conector 35-50 mm.","T268000",338.55,8430133808358,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1197,"Antorcha TIG SR 18 electrovalvula - 8 m. conector 35-50 mm. Refrigerada","T188000",375.85,8430133808341,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1198,"Cuerpo estándar antorcha XT 17 E",190520200,17.82,8430133582616,"https://galagar.com/wp-content/uploads/2022/01/Cuello-TIG-17E.jpg",{"$error":"#VALUE!"}]
[1199,"Cuerpo estándar antorcha XT 26 E",190520600,26.1,8430133582630,"https://galagar.com/wp-content/uploads/2022/01/Cuello-TIG-26E.jpg",{"$error":"#VALUE!"}]
[1200,"Cuerpo estándar antorcha XT 18 E",190520300,27.49,8430133582647,"https://galagar.com/wp-content/uploads/2022/01/Cuello-TIG-26E.jpg",{"$error":"#VALUE!"}]
[1201,"Microrruptor XT",19051746,12.43,8430133636579,"https://galagar.com/wp-content/uploads/2022/01/MicroRuptor_1.jpg",{"$error":"#VALUE!"}]
[1202,"Empuñadura y micro XT-17",19051744,47.57,8430133569952,"https://galagar.com/wp-content/uploads/2022/01/EmpuTIG_1.jpg",{"$error":"#VALUE!"}]
[1203,"Empuñadura y micro XT-26",19052644,59.12,8430133569969,"https://galagar.com/wp-content/uploads/2022/01/EmpuTIG_1.jpg",{"$error":"#VALUE!"}]
[1204,"Cable potencia / gas 4 m. 1/4” SR17","19S20000421",132.91,8430133645793,"https://galagar.com/wp-content/uploads/2022/01/Coaxial-TIG_1.jpg",{"$error":"#VALUE!"}]
[1205,"Cable potencia / gas 4 m. 1/4” SR26","19S70000421",179.36,8430133647902,"https://galagar.com/wp-content/uploads/2022/01/Coaxial-TIG_1.jpg",{"$error":"#VALUE!"}]
[1206,"Cable potencia / agua 4 m. 3/8” SR18","19s30000422",126.64,8430133643720,"https://galagar.com/wp-content/uploads/2022/01/Coaxial-TIG_1.jpg",{"$error":"#VALUE!"}]
[1207,"Antorcha TIG SR 17 - 4 m. Euro","T174030",322.08,8430133808372,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1208,"Antorcha TIG SR 26 - 4 m. Euro","T264030",354.36,8430133803957,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1209,"Antorcha TIG SR 18 - 4 m. Euro - Refrigerada","T184030",436.34,8430133808402,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1210,"Antorcha TIG SR 17 - 8 m. Euro","T178030",417.23,8430133808389,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1211,"Antorcha TIG SR 26 - 8 m. Euro","T268030",475.87,8430133809195,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1212,"Antorcha TIG SR 18 - 8 m. Euro - Refrigerada","T188030",532.92999999999995,8430133808419,"https://galagar.com/wp-content/uploads/2022/01/SR-18eu.jpg",{"$error":"#VALUE!"}]
[1213,"Cuerpo antorcha TIG SR 17 Euro","T170001",15.05,8430133808365,"https://galagar.com/wp-content/uploads/2022/01/Cuello-TIG-17E.jpg",{"$error":"#VALUE!"}]
[1214,"Cuerpo antorcha TIG SR 26 Euro","T260001",17.53,8430133808433,"https://galagar.com/wp-content/uploads/2022/01/Cuello-TIG-26E.jpg",{"$error":"#VALUE!"}]
[1215,"Cuerpo antorcha TIG SR 18 Euro","T180001",22.91,8430133808396,"https://galagar.com/wp-content/uploads/2022/01/Cuello-TIG-26E.jpg",{"$error":"#VALUE!"}]
[1216,"Empuñadura antorcha TIG SR 17-26-18","T993001",28.87,8430133808457,"https://galagar.com/wp-content/uploads/2022/01/EmpuTIG_1.jpg",{"$error":"#VALUE!"}]
[1217,"Cable de potencia antorcha TIG SR 4 m. 16 mm2","T18CA041",84.09,8430133808426,"https://galagar.com/wp-content/uploads/2022/01/Coaxial-TIG_1.jpg",{"$error":"#VALUE!"}]
[1218,"Blister10 uds. Tobera cerámica GR.4","6298B10",6.27,8430133668730,"https://galagar.com/wp-content/uploads/2023/01/Toberas-TIG-GR4.jpg",{"$error":"#VALUE!"}]
[1219,"Blister10 uds. Tobera cerámica GR.5","6444B10",6.27,8430133668747,"https://galagar.com/wp-content/uploads/2023/01/Toberas-TIG-GR5.jpg",{"$error":"#VALUE!"}]
[1220,"Blister10 uds. Tobera cerámica GR.6","6445B10",6.27,8430133668754,"https://galagar.com/wp-content/uploads/2023/01/Toberas-TIG-GR6_B.jpg",{"$error":"#VALUE!"}]
[1221,"Blister10 uds. Tobera cerámica GR.7","6446B10",6.27,8430133668761,"https://galagar.com/wp-content/uploads/2023/01/Toberas-TIG-GR7.jpg",{"$error":"#VALUE!"}]
[1222,"Blister10 uds. Tobera cerámica GR.8","6447B10",6.27,8430133668778,"https://galagar.com/wp-content/uploads/2023/01/Toberas-TIG-GR8_B.jpg",{"$error":"#VALUE!"}]
[1223,"Blister10 uds. Tobera cerámica GR.10","6510B10",6.27,8430133680091,"https://galagar.com/wp-content/uploads/2023/01/Toberas-TIG-GR10_B.jpg",{"$error":"#VALUE!"}]
[1224,"Blister10 uds. Tobera cerámica GR.12","19500532B10",6.27,8430133680527,"https://galagar.com/wp-content/uploads/2023/01/Toberas-TIG-GR12.jpg",{"$error":"#VALUE!"}]
[1225,"Blister10 uds. Portatobera difusor 1,0 mm.","6299B10",13.56,8430133668686,"https://galagar.com/wp-content/uploads/2022/01/PortaTobera-Estandar_Bod.jpg",{"$error":"#VALUE!"}]
[1226,"Blister10 uds. Portatobera difusor 1,6 mm.","6455B10",13.56,8430133668693,"https://galagar.com/wp-content/uploads/2022/11/PortaTobera-TIG.jpg",{"$error":"#VALUE!"}]
[1227,"Blister10 uds. Portatobera difusor 2,0 mm.","6507B10",13.56,8430133680084,"https://galagar.com/wp-content/uploads/2022/01/PortaTobera-Estandar_Bod.jpg",{"$error":"#VALUE!"}]
[1228,"Blister10 uds. Portatobera difusor 2,4 mm.","6456B10",13.56,8430133668709,"https://galagar.com/wp-content/uploads/2022/11/PortaTobera-TIG.jpg",{"$error":"#VALUE!"}]
[1229,"Blister10 uds. Portatobera difusor 3,2 mm.","6457B10",13.56,8430133668716,"https://galagar.com/wp-content/uploads/2022/01/PortaTobera-Estandar_Bod.jpg"]
[1230,"Blister10 uds. Portatobera difusor 4,0 mm.","6458B10",13.56,8430133668723,"https://galagar.com/wp-content/uploads/2022/11/PortaTobera-TIG.jpg",{"$error":"#VALUE!"}]
[1231,"Blister10 uds. Portaelectrodo 1,0 mm.","6300B10",9.48,8430133668631,"https://galagar.com/wp-content/uploads/2022/01/PortaElectrodos-Estandar_Bod.jpg",{"$error":"#VALUE!"}]
[1232,"Blister10 uds. Portaelectrodo 1,6 mm.","6449B10",9.48,8430133668648,"https://galagar.com/wp-content/uploads/2022/11/PortaElectrodos-TIG.jpg",{"$error":"#VALUE!"}]
[1233,"Blister10 uds. Portaelectrodo 2,0 mm.","6450B10",9.48,8430133680510,"https://galagar.com/wp-content/uploads/2022/01/PortaElectrodos-Estandar_Bod.jpg",{"$error":"#VALUE!"}]
[1234,"Blister10 uds. Portaelectrodo 2,4 mm.","6451B10",9.48,8430133668655,"https://galagar.com/wp-content/uploads/2022/11/PortaElectrodos-TIG.jpg",{"$error":"#VALUE!"}]
[1235,"Blister10 uds. Portaelectrodo 3,2 mm.","6452B10",9.48,8430133668662,"https://galagar.com/wp-content/uploads/2022/01/PortaElectrodos-Estandar_Bod.jpg",{"$error":"#VALUE!"}]
[1236,"Blister10 uds. Portaelectrodo 4,0 mm.","6453B10",9.48,8430133668679,"https://galagar.com/wp-content/uploads/2022/11/PortaElectrodos-TIG.jpg",{"$error":"#VALUE!"}]
[1237,"Protección porta tobera",19500402,1.38,8430133643607,"https://galagar.com/wp-content/uploads/2022/01/Proteccion-Estandar.jpg",{"$error":"#VALUE!"}]
[1238,"Tapón largo XT 17/18/26",6297,3.14,8430133342647,"https://galagar.com/wp-content/uploads/2022/11/Capuchon-Largo.jpg",{"$error":"#VALUE!"}]
[1239,"Capuchón medio XT 17/18/26",19500347,1.88,8430133643652,"https://galagar.com/wp-content/uploads/2022/11/Capuchon-Medio.jpg",{"$error":"#VALUE!"}]
[1240,"Tapón corto XT 17/18/26",6280,1.88,8430133342579,"https://galagar.com/wp-content/uploads/2022/11/Capuchon-Corto.jpg",{"$error":"#VALUE!"}]
[1241,"Tobera cerámica Gas Lens GR 4 Ø 6,3 mm. / Pack 10 uds.","T54N18B10",15.06,8430133808624,"https://galagar.com/wp-content/uploads/2022/01/Tobera-GasLens_GR4-Bod.jpg",{"$error":"#VALUE!"}]
[1242,"Tobera cerámica Gas Lens GR 5 Ø 8,0 mm. / Pack 10 uds.","T54N17B10",15.06,8430133808617,"https://galagar.com/wp-content/uploads/2022/01/Tobera-GasLens_GR5-Bod.jpg",{"$error":"#VALUE!"}]
[1243,"Tobera cerámica Gas Lens GR 6 Ø 9,5 mm. / Pack 10 uds.","T54N16B10",15.06,8430133808600,"https://galagar.com/wp-content/uploads/2022/01/Tobera-GasLens_GR6-Bod.jpg",{"$error":"#VALUE!"}]
[1244,"Tobera cerámica Gas Lens GR 7 Ø 11 mm. / Pack 10 uds.","T54N15B10",15.06,8430133809492,"https://galagar.com/wp-content/uploads/2022/01/Tobera-GasLens_GR7-Bod.jpg",{"$error":"#VALUE!"}]
[1245,"Tobera cerámica Gas Lens GR 8 Ø 12,5 mm. / Pack 10 uds.","T54N14B10",15.06,8430133808594,"https://galagar.com/wp-content/uploads/2022/01/Tobera-GasLens_GR8-Bod.jpg",{"$error":"#VALUE!"}]
[1246,"Portatobera difusor Gas Lens Ø 1,0 mm. / Pack 5 uds.","T45V24B5",37.65,8430133808556,"https://galagar.com/wp-content/uploads/2022/01/Difusor-GasLens.jpg",{"$error":"#VALUE!"}]
[1247,"Difusor Gas Lens SR 17-18-26 Ø 1,6 mm.","T45V25B5",37.65,8430133809386,"https://galagar.com/wp-content/uploads/2022/01/Difusor-GasLens.jpg",{"$error":"#VALUE!"}]
[1248,"Portatobera difusor Gas Lens Ø 2,0 mm. / Pack 5 uds.","T45V25MB5",37.65,8430133808563,"https://galagar.com/wp-content/uploads/2022/01/Difusor-GasLens.jpg",{"$error":"#VALUE!"}]
[1249,"Difusor Gas Lens SR 17-18-26 Ø 2,4 mm.","T45V26B5",37.65,8430133809393,"https://galagar.com/wp-content/uploads/2022/01/Difusor-GasLens.jpg",{"$error":"#VALUE!"}]
[1250,"Difusor Gas Lens SR 17-18-26 Ø 3,2 mm.","T45V27B5",37.65,8430133809409,"https://galagar.com/wp-content/uploads/2022/01/Difusor-GasLens.jpg",{"$error":"#VALUE!"}]
[1251,"Portatobera difusor Gas Lens 4,0 mm. / Pack 5 uds.","T45V278B5",37.65,8430133808570]
[1252,"Portatobera aislante Gas Lens / Pack 5 uds.","T54N01B5",15.69,8430133808587,"https://galagar.com/wp-content/uploads/2022/01/Proteccion-GasLens.jpg",{"$error":"#VALUE!"}]
[1253,"Estuche consumibles TIG (35 piezas)","ETIG",34.159999999999997,8430133682934,"https://galagar.com/wp-content/uploads/2022/01/Estuche_TIG.jpg",{"$error":"#VALUE!"}]
[1254,"Caja de tungstenos 1,0 mm. Verde Puro","750100C",19.079999999999998,8430133568610,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Verde.jpg",{"$error":"#VALUE!"}]
[1255,"Caja de tungstenos 1,6 mm. Verde Puro","750160C",22.84,8430133568689,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Verde.jpg",{"$error":"#VALUE!"}]
[1256,"Caja de tungstenos 2,0 mm. Verde Puro","750200C",40.03,8430133568757,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Verde.jpg",{"$error":"#VALUE!"}]
[1257,"Caja de tungstenos 2,4 mm. Verde Puro","750240C",47.69,8430133568917,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Verde.jpg",{"$error":"#VALUE!"}]
[1258,"Caja de tungstenos 3,2 mm. Verde Puro","750320C",82.09,8430133568986,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Verde.jpg",{"$error":"#VALUE!"}]
[1259,"Caja de tungstenos 4,0 mm. Verde Puro","750400C",133.29,8430133569051,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Verde.jpg",{"$error":"#VALUE!"}]
[1260,"Caja de tungstenos 1,0 mm. Rojo 2% TH","750102C",24.48,8430133568634,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Rojo.jpg",{"$error":"#VALUE!"}]
[1261,"Caja de tungstenos 1,6 mm. Rojo 2% TH","750162C",28.62,8430133568702,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Rojo.jpg",{"$error":"#VALUE!"}]
[1262,"Caja de tungstenos 2,0 mm. Rojo 2% TH","750202C",47.57,8430133568771,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Rojo.jpg",{"$error":"#VALUE!"}]
[1263,"Caja de tungstenos 2,4 mm. Rojo 2% TH","750242C",57.24,8430133568931,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Rojo.jpg",{"$error":"#VALUE!"}]
[1264,"Caja de tungstenos 3,2 mm. Rojo 2% TH","750322C",96.02,8430133569006,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Rojo.jpg",{"$error":"#VALUE!"}]
[1265,"Caja de tungstenos 4,0 mm. Rojo 2% TH","750402C",156.38,8430133569075,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Rojo.jpg",{"$error":"#VALUE!"}]
[1266,"Caja de tungstenos 1,0 mm. Gris 2% CE","750103C",19.079999999999998,8430133568641,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Gris.jpg",{"$error":"#VALUE!"}]
[1267,"Caja de tungstenos 1,6 mm. Gris 2% CE","750163C",22.97,8430133568719,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Gris.jpg",{"$error":"#VALUE!"}]
[1268,"Caja de tungstenos 2,0 mm. Gris 2% CE","750203C",40.159999999999997,8430133568870,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Gris.jpg",{"$error":"#VALUE!"}]
[1269,"Caja de tungstenos 2,4 mm. Gris 2% CE","750243C",47.69,8430133568948,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Gris.jpg",{"$error":"#VALUE!"}]
[1270,"Caja de tungstenos 3,2 mm. Gris 2% CE","750323C",81.96,8430133569013,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Gris.jpg",{"$error":"#VALUE!"}]
[1271,"Caja de tungstenos 4,0 mm. Gris 2% CE","750403C",133.29,8430133569082,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Gris.jpg",{"$error":"#VALUE!"}]
[1272,"Caja de tungstenos 1,0 mm. Negro 1% LTH","750104C",26.73,8430133568658,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[1273,"Caja de tungstenos 1,6 mm. Negro 1% LTH","750164C",29.75,8430133568726,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[1274,"Caja de tungstenos 2,0 mm. Negro 1% LTH","750204C",49.58,8430133568887,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[1275,"Caja de tungstenos 2,4 mm. Negro 1% LTH","750244C",58.88,8430133568955,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[1276,"Caja de tungstenos 3,2 mm. Negro 1% LTH","750324C",100.07,8430133569020,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[1277,"Caja de tungstenos 4,0 mm. Negro 1% LTH","750404C",133.29,8430133569099,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Negro.jpg",{"$error":"#VALUE!"}]
[1278,"Caja de tungstenos 1,0 mm. Oro 1,5% LTH","750106C",19.079999999999998,8430133568672,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Dorado.jpg",{"$error":"#VALUE!"}]
[1279,"Caja de tungstenos 1,6 mm. Oro 1,5% LTH","750166C",24.85,8430133568740,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Dorado.jpg",{"$error":"#VALUE!"}]
[1280,"Caja de tungstenos 2,0 mm. Oro 1,5% LTH","750206C",41.92,8430133568900,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Dorado.jpg",{"$error":"#VALUE!"}]
[1281,"Caja de tungstenos 2,4 mm. Oro 1,5% LTH","750246C",51.46,8430133568979,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Dorado.jpg",{"$error":"#VALUE!"}]
[1282,"Caja de tungstenos 3,2 mm. Oro 1,5% LTH","750326C",86.23,8430133569044,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Dorado.jpg",{"$error":"#VALUE!"}]
[1283,"Caja de tungstenos 4,0 mm. Oro 1,5% LTH","750406C",133.29,8430133569112,"https://galagar.com/wp-content/uploads/2022/01/Tungstenos-Dorado.jpg",{"$error":"#VALUE!"}]
[1284,"Afilador de tungstenos","8044166-NT","CONSULTAR",8430133857264]
[1285,"Con filtro de polvo integrado - Se sirve con maletín"]
[1286,"Antorcha Plasma P-50 - 6 metros",1603050,408.01,8430133399139,"https://galagar.com/wp-content/uploads/2022/01/Antorcha-P50-Negra.jpg",{"$error":"#VALUE!"}]
[1287,"Antorcha Plasma P-50 - 12 metros",1603150,532.66999999999996,8430133560867,"https://galagar.com/wp-content/uploads/2022/01/Antorcha-P50-Negra.jpg",{"$error":"#VALUE!"}]
[1288,"KIT consumibles para antorcha P-50","KITP50",76.209999999999994,8430133804718,"https://galagar.com/wp-content/uploads/2022/01/KIT-Antorcha-Plasma.jpg",{"$error":"#VALUE!"}]
[1289,"Cuerpo antorcha manual",1601000,144,8430133399108]
[1290,"Empuñadura con micro-interruptor",1603280,35.76,8430133438074]
[1291,"Junta tórica - 5 uds.","160100060B5",7.45,8430133643157]
[1292,"Electrodo-HF (larga duración) - 5 uds.","1652512B5",14.09,8430133637255]
[1293,"Difusor - VESPEL® - 2 uds.","1660001B2",27.47,8430133605506]
[1294,"Tobera  Ø 1,0 – 50 A (larga duración) - 5 uds.","1651095B5",10.220000000000001,8430133605308]
[1295,"Difusor tobera larga - 2 uds.","160109042B2",18.23,8430133605278]
[1296,"Electrodo largo – HF (larga duración) - 5 uds.","1652513B5",17.25,8430133605452]
[1297,"Tobera larga Ø 1,0 - 50 A (larga duración) - 5 uds.","1651095LB5",14.77,8430133605315]
[1298,"Porta-tobera - 2 uds.","1660320B2",23.06,8430133954536]
[1299,"Llave para difusor",1660368,15.77,8430133399702]
[1300,"Compás para corte",1651850,129.09,8430133399481]
[1301,"Carro compás",1651817,49.29,8430133828295]
[1302,"Antorcha plasma P-150 - 6 metros",1604051,618.33000000000004,8430133734336,"https://galagar.com/wp-content/uploads/2022/01/Antorcha-PT150.jpg",{"$error":"#VALUE!"}]
[1303,"Antorcha plasma P-150 - 12 metros",1604151,728.9,8430133399177]
[1304,"Kit consumibles para antorcha P-150","KITP150",156.52000000000001,8430133804701]
[1305,"Cuerpo antorcha manual",1602000,307.18,8430133399122]
[1306,"Empuñadura con micro-interruptor",1604280,34.24,8430133438081]
[1307,"Junta tórica - 5 uds.","160200060B5",7.6,8430133643034]
[1308,"Aislante interior- VESPEL® - 5 uds.","1660080B5",221.17,8430133637804]
[1309,"Difusor - 5 uds.","1605004B5",19.739999999999998,8430133605285]
[1310,"Electrodo - HF (larga duración) - 5 uds.","1652540B5",18.77,8430133605469]
[1311,"Difusor - VESPEL® - 2 uds.","1660020B2",26.92,8430133605513]
[1312,"Tobera Ø 1,1 - 5 uds.","1651140B5",27.12,8430133605322]
[1313,"Tobera Ø 1,35 (larga duración) - 5 uds.","1651141B5",19.61,8430133605339]
[1314,"Tobera Ø 1,6 (larga duración) - 5 uds.","1651142B5",17.95,8430133605346]
[1315,"Tobera Ø 1,8 (larga duración) - 5 uds.","1651143B5",19.670000000000002,8430133605353]
[1316,"Difusor largo - 2 uds.","1605005B2",22.78,8430133605292]
[1317,"Electrodo largo - HF (larga duración) - 5 uds.","1652549B5",33.82,8430133605476]
[1318,"Tobera larga corte x contacto (máximo 50 A) - 5 uds.","1651148B5",49.5,8430133637965]
[1319,"Tobera larga Ø 1,35 - 90 A - 5 uds.","165114813B5",43.23,8430133605360]
[1320,"Tobera larga Ø 1,6 - 120 A","165114816B5",38.79,8430133605377]
[1321,"Tobera larga Ø 1,8 - 150 A - 5 uds.","165114818B5",38.79,8430133605384]
[1322,"Porta-tobera (posibilidad corte a contacto)","1660350R",51.77,8430133570811]
[1323,"Distanciador corte manual a contacto (para toberas marca 6 ÷ 6c) - 5 uds.","1651950B5",62.27,8430133637811]
[1324,"Protección metálica exterior de cierre (para muelle distanciador) - 2 uds.","1651952B2",19.05,8430133605438]
[1325,"Muelle distanciador - 5 uds.","1651911B5",45.04,8430133605421]
[1326,"Protección corte contacto (tobera larga marca 9 máx. 50A) - 5 uds.","1651958B5",108.24,8430133637996]
[1327,"Espaciador para toberas largas de alto amperaje - 2 uds.","1651974B2",36.17,8430133637835]
[1328,"Tuerca exterior de cierre - 5 uds.","1651959B5",32.299999999999997,8430133637842]
[1329,"Extractor para difusor",1660369,24.3,8430133399719]
[1330,"Llave para electrodo",1660368,15.77,8430133399702]
[1331,"Compás para corte",1651851,142.76,8430133399498]
[1332,"Guía de corte",1651807,58.54,8430133399467]
[1333,"Antorcha plasma PT-40 - 4 m.",1609630,286.89,8430133560911,"https://galagar.com/wp-content/uploads/2022/01/Antorcha-PT40-1609630.jpg",{"$error":"#VALUE!"}]
[1334,"Antorcha plasma PT-40 - 6 m.",1609631,292.43,8430133560928]
[1335,"Antorcha plasma PT-40 - 6 m. Euroconector","1609635G",336.25,8430133746360]
[1336,"KIT consumibles para antorcha PT-40","KITPT40",118.47,8430133804473,"https://galagar.com/wp-content/uploads/2022/01/KIT-Antorcha-Plasma.jpg",{"$error":"#VALUE!"}]
[1337,"Conjunto de c. manual, 4 m., cable coaxial",1609685,178.24,8430133644932]
[1338,"Conjunto de c. manual, 6 m., cable coaxial",1609686,234.56,8430133644949]
[1339,"Cabezal antorcha manual PT-40",1609602,153.11000000000001,8430133560898]
[1340,"Junta tórica - 5 uds.","165162060B5",6.12,8430133605414]
[1341,"Empuñadura con interruptor",1609605,28.44,8430133560904]
[1342,"Interruptor",160730120,4.7,8430133560881]
[1343,"Electrodo corto Back Striking - 5 uds.","1652582B5",16.84,8430133605483]
[1344,"Difusor - 2 uds.","1660028B2",24.3,8430133605520]
[1345,"Tobera, corte contacto, Ø 0.65 - 10-20A, Back Striking - 5 uds.","165131806B5",18.23,8430133644857]
[1346,"Tobera, corte contacto, Ø 0.8 - 20-30A, Back Striking - 5 uds.","165131808B5",17.25,8430133644864]
[1347,"Tobera, corte contacto, Ø 0.9 - 30-40A, Back Striking- 5 uds.","165131809B5",17.25,8430133644871]
[1348,"Tobera, corte contacto Ø 0.9 - 30-40A, Back Striking - 5 uds.","165131209B5",17.95,8430133605391]
[1349,"Tobera plana, corte, Ø 1.0 - 40-50A, Back Striking- 5 uds.","165131310B5",19.05,8430133644895]
[1350,"Electrodo largo, Back Striking - 5 uds.","1652583B5",37.14,8430133605490]
[1351,"Tobera larga, corte contacto - Ø 0,65, 10-20 A, Back Striking - 5 uds.","1651318L06B5",35.76,8430133644901]
[1352,"Tobera larga, corte contacto - Ø 0,8, 20-30A, Back Striking - 5 uds.","1651318L08B5",35.76,8430133644918]
[1353,"Tobera larga, corte contacto - Ø 0,9, 30-40A, Back Striking - 5 uds.","165131409B5",40.729999999999997,8430133605407]
[1354,"Porta-tobera, 4 orificios - 2 uds.","1660389k4B2",32.17,8430133605544]
[1355,"Porta-tobera, 6 orificios estándar - 2 uds.","1660389B2",27.05,8430133605537]
[1356,"Compás PT-40",1651866,140.13,8430133561000]
[1357,"Espaciador 2 puntas - Para usar con ítem 5 y 7 solamente - 2 uds.","1660432B2",23.19,8430133605551]
[1358,"Llave para electrodo",1660368,15.77,8430133399702]
[1359,"Antorcha completa PT-106 - 6 metros",1609740,483.39,8430133799649,"https://galagar.com/wp-content/uploads/2022/01/Antorcha-PT106.jpg",{"$error":"#VALUE!"}]
[1360,"Antorcha completa PT-106 - 12 metros",1609726,836.44,8430133802615]
[1361,"KIT consumibles para antorcha PT-106","KITPT106",196.04,8430133804695]
[1362,"Cuerpo antorcha manual","GG1609700",162.08000000000001,8430133799823]
[1363,"Junta tórica","165119041B10",14.77,8430133637859]
[1364,"Tubo de refrigeración - 2 uds.","160970048B2",26.92,8430133637651]
[1365,"Mango con interruptor",169705,31.47,8430133645175]
[1366,"Interruptor",160730120,4.7,8430133560881]
[1367,"Electrodo, Back Striking (hexagonal) - 5 uds.","GG1652556B5",23.74,8430133800932]
[1368,"Difusor, 30-70 A - 2 uds.","1660025B2",32.450000000000003,8430133637675]
[1369,"Difusor, 80-100 A y desbaste - 2 uds.","1660026B2",39.07,8430133637712]
[1370,"Tobera, corte contacto Ø 0,9, 30-40 A, Back Striking - 5 uds.","165124509B5",33.39,8430133637682]
[1371,"Tobera, corte, Ø 1,0 - 40-50 A, Back Striking - 5 uds.","165124610B5",27.75,8430133637699]
[1372,"Tobera, corte, Ø 1,1 - 50-60 A, Back Striking - 5 uds.","165124611B5",28.03,8430133645182]
[1373,"Tobera, corte, Ø 1,2 - 60-70 A, Back Striking - 5 uds.","165124612B5",27.33,8430133637705]
[1374,"Tobera, corte, Ø 1,4 - 80-90 A, Back Striking - 5 uds.","165124814B5",29.14,8430133645199]
[1375,"Tobera, corte, Ø 1,5 - 100 A, Back Striking - 5 uds.","165124815B5",29.82,8430133637729]
[1376,"Capuchón de retención, 30-70 A - 2 uds.","1660500B2",73.17,8430133637866]
[1377,"Capuchón de retención, 80-100 A - 2 uds.","1660501B2",72.900000000000006,8430133637873]
[1378,"Separador de doble punta (para su uso con a. 7 y 8 solamente) - 2 uds.","1660444B2",31.34,8430133637897]
[1379,"Llave para electrodo",1660368,15.77,8430133399702]
[1380,"Punta de contacto, Ø 1,0 - 40-50 A, Back Striking - 5 uds.","165127610B5",46.8,8430133645212]
[1381,"Punta de contacto, Ø 1,1 - 50-60 A, Back Striking - 5 uds.","165127611B5",28.99,8430133645236]
[1382,"Punta de contacto, Ø 1,2 - 60-70 A, Back Striking - 5 uds.","165127612B5",28.35,8430133637736]
[1383,"Punta de contacto, Ø 1,4 - 80-90 A, Back Striking - 5 uds.","165127814B5",28.21,8430133645243]
[1384,"Punta de contacto, Ø 1,5 - 100 A, Back Striking - 5 uds.","165127815B5",27.75,8430133637743]
[1385,"Porta-tobera - 2 uds.","1660502B2",78.84,8430133651121]
[1386,"Protección porta-tobera, manual, 40-70 A - 5 uds.","1660504B5",91.12,8430133637903]
[1387,"Protección porta-tobera, manual, 80-100 A - 5 uds.","1660505B5",96.92,8430133637910]
[1388,"Compás",1651864,159.46,8430133658311]
[1389,"Antorcha TH-125 - 6 metros","1603721CX",1011.87,8430133661892,"https://galagar.com/wp-content/uploads/2022/01/Antorcha-TH125.jpg",{"$error":"#VALUE!"}]
[1390,"KIT consumibles para antorcha TH-125","KITTH125",284.22000000000003,8430133803988,"https://galagar.com/wp-content/uploads/2022/01/KIT-Antorcha-Plasma.jpg",{"$error":"#VALUE!"}]
[1391,"Cabezal antorcha",1603700,278.47000000000003,8430133662783]
[1392,"Junta tórica",160103560,1.52,8430133662837]
[1393,"Mango con interruptor",1603705,54.79,8430133662844]
[1394,"Interruptor",160730120,4.7,8430133560881]
[1395,"Difusor 45-85 A",1660042,37,8430133662851]
[1396,"Difusor 100-125A",1660040,36.450000000000003,8430133662868]
[1397,"Electrodo, 45-125 A",1652677,7.18,8430133662875]
[1398,"Tobera, 45 A, corte precisión",1651415,8.84,8430133662998]
[1399,"Tobera, 45 A",1651416,4.7,8430133662882]
[1400,"Tobera, 65 A",1651417,4.7,8430133662899]
[1401,"Tobera, 85 A",1651418,4.7,8430133662905]
[1402,"Tobera, 105 A",1651419,5.1100000000000003,8430133662912]
[1403,"Tobera, 125 A",165141916,5.1100000000000003,8430133662929]
[1404,"Porta-tobera 45-85 A","1660309TA",64.75,8430133662936]
[1405,"Porta-tobera 100-125 A","1660309TC",69.3,8430133662943]
[1406,"Protección porta-tobera 45 A, Corte de precisión",1651928,10.35,8430133662981]
[1407,"Protección porta-tobera 45-85 A",1651921,20.84,8430133662950]
[1408,"Protección porta-tobera 100-125 A",1651926,19.739999999999998,8430133662967]
[1409,"Protección porta-tobera 100-125 A",1651927,19.739999999999998,8430133663049]
[1410,"Compás de corte",1651865,135.57,8430133789510]
[1411,"Antorcha TM-125 - 6 metros - Recta máquina","1603731CX",1133.3399999999999,8430133663513]
[1412,"Antorcha TM-125 -12 metros - Recta máquina","1603736CX",1304.6600000000001,8430133671815]
[1413,"Antorcha UPH-160 - 6 metros","1603921CX",1408.15,8430133834500,"https://galagar.com/wp-content/uploads/2024/07/Antorcha-UPH160.jpg",{"$error":"#VALUE!"}]
[1414,"Antorcha UPH-160 - 6 metros recta","1603931CX",1520.8,8430133836832]
[1415,"Antorcha UPH-160 - 12 metros recta","1603936CX",2083.02,8430133836849]
[1416,"KIT consumibles para antorcha UPH-160","KITUPH160",312.47000000000003]
[1417,"Cabezal antorcha para UPH 160",1603900,405.4,8430133836146]
[1418,"O-ring para UPH 160","160390060B20",43.86,8430133836153]
[1419,"Mango con interruptor para UPH 160",1605505,57.32,8430133836856]
[1420,"Electrodo, 45-160 A para UPH 160","1652678B5",39.85,8430133836160]
[1421,"Difusor, 45-160A para UPH 160","1660039B2",109.52,8430133836177]
[1422,"Tobera, 45 A para UPH 160","1651420B10",68.760000000000005,8430133836184]
[1423,"Tobera, 65 A para UPH 160","1651421B10",68.760000000000005,8430133836191]
[1424,"Tobera, 85 A para UPH 160","1651422B10",68.760000000000005,8430133836207]
[1425,"Tobera, 105-125 A para UPH 160","1651425B10",60.44,8430133836214]
[1426,"Tobera, 160 A para UPH 160","1651426B10",78.58,8430133836221]
[1427,"Porta-tobera,  45-85 A para UPH 160","1660311TA",94.86,8430133836238]
[1428,"Porta-tobera, 105-160 A para UPH 160","1660311TB",94.86,8430133836245]
[1429,"Protección porta-tobera, 45-85 A para UPH 160","1651916TB2",67.680000000000007,8430133836252]
[1430,"Protección porta-tobera, 105-160 A para UPH 160","1651917TB2",54.96,8430133836269]
[1431,"Tober de gubiado, 160 A para UPH 160","1651425GB10",99.46,8430133836276]
[1432,"Protección porta-tobera gubiado para UPH 160","1651919GB2",45.75,8430133836283]
[1433,"Flatcut cartucho 160 A para UPH 160",1653638,214.4,8430133836290]
[1434,"Compás de corte para UPH 160",1651868,161.05000000000001,8430133836306]
[1435,"Pantalla Gasweld DARK - Clásica","5998F",93.25,8430133824723,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK.jpg",{"$error":"#VALUE!"}]
[1436,"Pantalla Gasweld DARK - Calavera","5998FC",104.22,8430133824730,"https://galagar.com/wp-content/uploads/2022/11/Gasweld-DARK_C.jpg",{"$error":"#VALUE!"}]
[1437,"Cubrefiltro Gasweld exterior 115x95 mm.","5998F03",1.57,8430133824792]
[1438,"Cubrefiltro Gasweld interior 96x50 mm.","5998F02",1.29,8430133824778]
[1439,"Pantalla Gasweld BASIC (¡Nueva!)","59999A",66.88]
[1440,"Pantalla electrónica Galaxy","51259B",170.1,8430133667641,"https://galagar.com/wp-content/uploads/2022/01/Galaxy_2.jpg",{"$error":"#VALUE!"}]
[1441,"Cubrefiltro Galaxy exterior 124x106 mm. Galaxy",5125905,2.97,8430133670986]
[1442,"Cubrefiltro Galaxy interior 106x68 mm. Galaxy",5125906,2.59,8430133670962]
[1443,"Pantalla Servore V2","30144000VN",383.99,8430133815318,"https://galagar.com/wp-content/uploads/2022/05/ServoreVN.jpg",{"$error":"#VALUE!"}]
[1444,"Cubrefiltro Servore exterior 122x86 mm.",30140002,3.23,8430133817671]
[1445,"Cubrefiltro Servore interior 120x48 mm.",30140015,2.06,8430133815912]
[1446,"Gafas electrónicas Modelo Basic",301450001,362.38,8430133789794,"https://galagar.com/wp-content/uploads/2022/01/Gafas-Basic-1.jpg",{"$error":"#VALUE!"}]
[1447,"Gafas electrónicas Modelo PRO",301450002,441.27,8430133789817,"https://galagar.com/wp-content/uploads/2022/01/Gafas-PRO-1.jpg",{"$error":"#VALUE!"}]
[1448,"Pantalla Galaxy PRO Cassette100x67 mm. Soldar/esmerilar","30058S13",1464.32,8430133787547,"https://galagar.com/wp-content/uploads/2022/01/Galaxy-PRO-2.jpg",{"$error":"#VALUE!"}]
[1449,"Pantalla Galaxy PRO Cassette 93x43 mm. Soldar/esmerilar","30058S4",1260.94,8430133785147,"https://galagar.com/wp-content/uploads/2022/01/Galaxy-PRO-2.jpg",{"$error":"#VALUE!"}]
[1450,"Pantalla Galaxy PRO Para Plasma y autógena - Tono DIN5",3007705,1071.1199999999999,8430133788025,"https://galagar.com/wp-content/uploads/2022/01/Galaxy-PRO-2.jpg",{"$error":"#VALUE!"}]
[1451,"Pantalla Galaxy PRO Para esmerilar - Tono transparente",3007700,989.77,8430133785949,"https://galagar.com/wp-content/uploads/2022/01/Galaxy-PRO-2.jpg",{"$error":"#VALUE!"}]
[1452,"Aspirador con tubo flexible - Motor aspirador",7130500000,"CONSULTAR",8717491004425]
[1453,"Tubo 5 m. con boquilla de embudo",7900068010,"CONSULTAR",8717491005217]
[1454,"Tubo 5 m. de escape",7900068020,"CONSULTAR",8717491005224]
[1455,"KIT aspirador FAN28 - Motor aspirador",7905220040,"CONSULTAR",8717491005378,"https://galagar.com/wp-content/uploads/2023/04/MotorAspirador-Fijo.jpg",{"$error":"#VALUE!"}]
[1456,"Soporte pared para motor de aspiracion FAN28",795301000,"CONSULTAR",8430133808648]
[1457,"Interruptor Magnético-térmico FAN28",328270160,"CONSULTAR",8717491001370]
[1458,"Brazo flex 3 m. Ø 203 mm. + Kit FAN28",7925160090,"CONSULTAR",8717491005897,"https://galagar.com/wp-content/uploads/2023/04/Brazo_3-4m.jpg",{"$error":"#VALUE!"}]
[1459,"Brazo flex 4 m. Ø 203 mm. + Kit FAN28",7925210090,"CONSULTAR",8717491005965,"https://galagar.com/wp-content/uploads/2023/04/Brazo_3-4m.jpg",{"$error":"#VALUE!"}]
[1460,"Brazo extensor de 2 m.",792012200,"CONSULTAR",8430133808631,"https://galagar.com/wp-content/uploads/2023/04/BrazoExtensor.jpg",{"$error":"#VALUE!"}]
[1461,"Aspirador portátil + Brazo flexible (2 m. - Ø160 mm. - Filtro de 15 m2)",111449,"CONSULTAR",8430133680466,"https://galagar.com/wp-content/uploads/2022/01/MobileGala.jpg",{"$error":"#VALUE!"}]
[1462,"Aspirador portátil + Brazo flexible (3 m. - Ø160 mm. - Filtro de 15 m2)",111470,"CONSULTAR",8430133676711,"https://galagar.com/wp-content/uploads/2022/01/MobileGala.jpg",{"$error":"#VALUE!"}]
[1463,"Aspirador portátil + Brazo de aluminio (2 m. - Ø160 mm. - Filtro de 26 m2)",111452,"CONSULTAR",8430133680473,"https://galagar.com/wp-content/uploads/2022/01/Mobile-GalaAlu.jpg",{"$error":"#VALUE!"}]
[1464,"Aspirador portátil + Brazo de aluminio (3 m. - Ø160 mm. - Filtro de 26 m2)",111473,"CONSULTAR",8430133684051,"https://galagar.com/wp-content/uploads/2022/01/Mobile-GalaAlu.jpg",{"$error":"#VALUE!"}]
[1465,"Casette de pre-filtros (G4) 1 m2",111637,"CONSULTAR",8430133710965]
[1466,"Casette filtro HEPA (E12 / MERV 16) 15 m²",111628,"CONSULTAR",8430133711412]
[1467,"Casette filtro HEPA (E12 / MERV 16) 26 m²",111636,"CONSULTAR",8430133680268]
[1468,"Filtro recambio de carbón activo 15 kg.",112427,"CONSULTAR",8430133809102]
[1469,"Aspirador fijo + Brazo flexible de 2 m.- Ø160 mm.",111455,"CONSULTAR",8430133680480,"https://galagar.com/wp-content/uploads/2022/01/AspiradorMonoBrazo-Flex.jpg",{"$error":"#VALUE!"}]
[1470,"Aspirador fijo + Brazo flexible de 3 m.- Ø160 mm.",111476,"CONSULTAR",8430133809096,"https://galagar.com/wp-content/uploads/2022/01/AspiradorMonoBrazo-Flex.jpg",{"$error":"#VALUE!"}]
[1471,"Aspirador fijo + Brazo flexible de 4 m.- Ø160 mm.",111488,"CONSULTAR",8430133802974,"https://galagar.com/wp-content/uploads/2022/01/AspiradorMonoBrazo-Flex.jpg",{"$error":"#VALUE!"}]
[1472,"Aspirador fijo + Brazo aluminio de 2 m.- Ø160 mm.",111459,"CONSULTAR",8430133680497,"https://galagar.com/wp-content/uploads/2022/01/aspirador-fino1brazofoto.jpg",{"$error":"#VALUE!"}]
[1473,"Aspirador fijo + Brazo aluminio de 3 m.- Ø160 mm.",111479,"CONSULTAR",8430133682408,"https://galagar.com/wp-content/uploads/2022/01/aspirador-fino1brazofoto.jpg",{"$error":"#VALUE!"}]
[1474,"Aspirador fijo + Brazo aluminio de 4 m.- Ø160 mm.",111491,"CONSULTAR",8430133793227,"https://galagar.com/wp-content/uploads/2022/01/aspirador-fino1brazofoto.jpg",{"$error":"#VALUE!"}]
[1475,"Aspirador fijo + Brazo flexible de 2+2 m.- Ø160 mm.",111462,"CONSULTAR",8430133679781,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_2.jpg",{"$error":"#VALUE!"}]
[1476,"Aspirador fijo + Brazo flexible de 3+3 m.- Ø160 mm.",111482,"CONSULTAR",8430133774134,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_2.jpg",{"$error":"#VALUE!"}]
[1477,"Aspirador fijo + Brazo flexible de 4+4 m.- Ø160 mm.",111494,"CONSULTAR",8430133678197,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_2.jpg",{"$error":"#VALUE!"}]
[1478,"Aspirador fijo + Brazo aluminio de 2+2 m.- Ø160 mm.",111465,"CONSULTAR",8430133680503,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_1.jpg",{"$error":"#VALUE!"}]
[1479,"Aspirador fijo + Brazo aluminio de 3+3 m.- Ø160 mm.",111485,"CONSULTAR",8430133808662,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_1.jpg",{"$error":"#VALUE!"}]
[1480,"Aspirador fijo + Brazo aluminio de 4+4 m.- Ø160 mm.",111497,"CONSULTAR",8430133799601,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_1.jpg",{"$error":"#VALUE!"}]
[1481,"Casette de pre-filtros (G4)  1m2",111637,"CONSULTAR",8430133710965]
[1482,"Casette filtro HEPA (HE12 / MERV 16)  15 m2",111628,"CONSULTAR",8430133711412]
[1483,"Casette filtro HEPA (HE12 / MERV 16)  26 m2",111636,"CONSULTAR",8430133680268]
[1484,"Filtro de carbón activo de 15 Kg.",112427,"CONSULTAR",8430133809102]
[1485,"Casette adaptador salida de aire rectangular a circular Ø 250 mm.",111197,"CONSULTAR",8430133808655]
[1486,"Silenciador salida recta Ø 250 mm.",117554,"CONSULTAR",8430133808679]
[1487,"Aspirador portátil modelo PHV",7603001400,"CONSULTAR",8430133605889,"https://galagar.com/wp-content/uploads/2022/01/PHV-portatil.jpg",{"$error":"#VALUE!"}]
[1488,"Prefiltro PHV - Categoría G2",102275,"CONSULTAR",8717491148099]
[1489,"Filtro cartucho desechable para PHV / con prefiltro de aluminio integrado",9850060230,"CONSULTAR",8430133809126]
[1490,"Filtro HEPA para PHV / CategorÍa E12",9850060140,"CONSULTAR",8717491011874]
[1491,"Soporte para montaje en pared del equipo PHV",791503000,"CONSULTAR",8430133808686]
[1492,"Manguera de aspiración Ø 45 mm. 5 m.",9880020110,"CONSULTAR",8717491007082]
[1493,"Pieza de conexión para 2 mangueras Ø 45 mm",809010040,"CONSULTAR",8430133683542]
[1494,"KIT Tobera",7900060030,"CONSULTAR",8717491005187]
[1495,"Boquilla 40 cm. con sistema E, sujeción magnética y conexión de manguera.",7900060010,"CONSULTAR",8717491005163]
[1496,"Aspirador movil MFD + Brazo flexible 3 m. Ø 203 mm.","7025100000+7925160090","CONSULTAR"]
[1497,"Aspirador movil MFD + Brazo flexible 4 m. Ø 203 mm.","7025100000+7925210090","CONSULTAR"]
[1498,"Prefiltro / apaga chispas de aluminio",9820310110,"CONSULTAR",8430133625351]
[1499,"Filtro cartucho 50 m²",9850060050,"CONSULTAR",8717491011782]
[1500,"Lámpara de trabajo + interruptor automático de arranque / paro",7900010190,"CONSULTAR",8717491005019]
[1501,"Opción 1 - Banco de trabajo ECO",7204700000,"CONSULTAR",8430133798062,"https://galagar.com/wp-content/uploads/2023/04/Banco-ECO.jpg",{"$error":"#VALUE!"}]
[1502,"Opción 2 - Banco de trabajo BASIC",111745,"CONSULTAR",8430133815479,"https://galagar.com/wp-content/uploads/2023/04/Banco-Ultra.jpg",{"$error":"#VALUE!"}]
[1503,"Opción 3 - Banco de trabajo ULTRA",111746,"CONSULTAR",8430133776244,"https://galagar.com/wp-content/uploads/2023/04/Banco-Ultra.jpg",{"$error":"#VALUE!"}]
[1504,"Pre-filtro apagachispas (2 uds.)",40000040,"CONSULTAR",8430133637262]
[1505,"Filtro principal apagachispas (2 uds.)",40100060,"CONSULTAR",8430133637279]
[1506,"Filtro FCC 52",40000020,"CONSULTAR",8430133637286]
[1507,"Filtro HEPA",40000030,"CONSULTAR",8430133637293]
[1508,"Aspirador fijo + Brazo flexible de 4+4 m.- Ø160 mm.",111494,"CONSULTAR",8430133678197,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_2.jpg",{"$error":"#VALUE!"}]
[1509,"Aspirador fijo + Brazo aluminio de 2+2 m.- Ø160 mm.",111465,"CONSULTAR",8430133680503,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_1.jpg",{"$error":"#VALUE!"}]
[1510,"Aspirador fijo + Brazo aluminio de 3+3 m.- Ø160 mm.",111485,"CONSULTAR",8430133808662,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_1.jpg",{"$error":"#VALUE!"}]
[1511,"Aspirador fijo + Brazo aluminio de 4+4 m.- Ø160 mm.",111497,"CONSULTAR",8430133799601,"https://galagar.com/wp-content/uploads/2022/01/Fijos-DobleBrazo_1.jpg",{"$error":"#VALUE!"}]
[1512,"Casette de pre-filtros (G4)  1m2",111637,"CONSULTAR",8430133710965]
[1513,"Casette filtro HEPA (HE12 / MERV 16)  15 m2",111628,"CONSULTAR",8430133711412]
[1514,"Casette filtro HEPA (HE12 / MERV 16)  26 m2",111636,"CONSULTAR",8430133680268]
[1515,"Filtro de carbón activo de 15 Kg.",112427,"CONSULTAR",8430133809102]
[1516,"Casette adaptador salida de aire rectangular a circular Ø 250 mm.",111197,"CONSULTAR",8430133808655]
[1517,"Silenciador salida recta Ø 250 mm.",117554,"CONSULTAR",8430133808679]
[1518,"Aspirador portátil modelo PHV",7603001400,"CONSULTAR",8430133605889,"https://galagar.com/wp-content/uploads/2022/01/PHV-portatil.jpg",{"$error":"#VALUE!"}]
[1519,"Prefiltro PHV - Categoría G2",102275,"CONSULTAR",8717491148099]
[1520,"Filtro cartucho desechable para PHV / con prefiltro de aluminio integrado",9850060230,"CONSULTAR",8430133809126]
[1521,"Filtro HEPA para PHV / CategorÍa E12",9850060140,"CONSULTAR",8717491011874]
[1522,"Soporte para montaje en pared del equipo PHV",791503000,"CONSULTAR",8430133808686]
[1523,"Manguera de aspiración Ø 45 mm. 5 m.",9880020110,"CONSULTAR",8717491007082]
[1524,"Pieza de conexión para 2 mangueras Ø 45 mm",809010040,"CONSULTAR",8430133683542]
[1525,"KIT Tobera",7900060030,"CONSULTAR",8717491005187]
[1526,"Boquilla 40 cm. con sistema E, sujeción magnética y conexión de manguera.",7900060010,"CONSULTAR",8717491005163]
[1527,"Aspirador movil MFD + Brazo flexible 3 m. Ø 203 mm.","7025100000+7925160090","CONSULTAR"]
[1528,"Aspirador movil MFD + Brazo flexible 4 m. Ø 203 mm.","7025100000+7925210090","CONSULTAR"]
[1529,"Prefiltro / apaga chispas de aluminio",9820310110,"CONSULTAR",8430133625351]
[1530,"Filtro cartucho 50 m²",9850060050,"CONSULTAR",8717491011782]
[1531,"Lámpara de trabajo + interruptor automático de arranque / paro",7900010190,"CONSULTAR",8717491005019]
[1532,"Opción 1 - Banco de trabajo ECO",7204700000,"CONSULTAR",8430133798062,"https://galagar.com/wp-content/uploads/2023/04/Banco-ECO.jpg",{"$error":"#VALUE!"}]
[1533,"Opción 2 - Banco de trabajo BASIC",111745,"CONSULTAR",8430133815479,"https://galagar.com/wp-content/uploads/2023/04/Banco-Ultra.jpg",{"$error":"#VALUE!"}]
[1534,"Opción 3 - Banco de trabajo ULTRA",111746,"CONSULTAR",8430133776244,"https://galagar.com/wp-content/uploads/2023/04/Banco-Ultra.jpg",{"$error":"#VALUE!"}]
[1535,"Pre-filtro apagachispas (2 uds.)",40000040,"CONSULTAR",8430133637262]
[1536,"Filtro principal apagachispas (2 uds.)",40100060,"CONSULTAR",8430133637279]
[1537,"Filtro FCC 52",40000020,"CONSULTAR",8430133637286]
[1538,"Filtro HEPA",40000030,"CONSULTAR",8430133637293]
[1539,"Manta protección 550º C - 100x100 cm.",1065061,36.85,8430133804947,"https://galagar.com/wp-content/uploads/2022/01/Mantas-Casic.jpg",{"$error":"#VALUE!"}]
[1540,"Manta protección 550º C - 200x100 cm.",1065062,65.099999999999994,8430133558086,"https://galagar.com/wp-content/uploads/2022/01/Mantas-Casic.jpg",{"$error":"#VALUE!"}]
[1541,"Manta protección 550º C - 200x200 cm.",1065065,130.21,8430133558093,"https://galagar.com/wp-content/uploads/2022/01/Mantas-Casic.jpg",{"$error":"#VALUE!"}]
[1542,"Manta protección 550º C - 200x100 cm. (¡Nueva!)","1065062F",37.880000000000003,8430133838416]
[1543,"Manta protección 550º C - 200x200 cm. (¡Nueva!)","1065065F",72.099999999999994,8430133838423]
[1544,"Manta protección 550º C - Rollo 25 m. x 1 m.",105650061025,487.25,8430133630171,"https://galagar.com/wp-content/uploads/2022/01/Mantas-Casic.jpg",{"$error":"#VALUE!"}]
[1545,"Manta protección 550º C - Rollo 50 m. x 2 m.",165650061550,2088.54,8430133808716,"https://galagar.com/wp-content/uploads/2022/01/Mantas-Casic.jpg",{"$error":"#VALUE!"}]
[1546,"Manta protección 550º C - Rollo 50 m. x 1 m. (¡Nueva!)","105650062050F",931.5,8430133838454]
[1547,"Manta protección 550º C - Rollo 50 m. x 1,5 m. (¡Nueva!)","105650061050F",465.75,8430133838461]
[1548,"Manta protección 1100º C - 100x90 cm.",1065091,101.27,8430133558109,"https://galagar.com/wp-content/uploads/2022/01/Mantas-PRO.jpg",{"$error":"#VALUE!"}]
[1549,"Manta protección 1100º C - 200x90 cm.",10650910,168.79,8430133558116,"https://galagar.com/wp-content/uploads/2022/01/Mantas-PRO.jpg",{"$error":"#VALUE!"}]
[1550,"Manta protección 1100º C - 90x300 cm.",10565093,253.67,8430133808693,"https://galagar.com/wp-content/uploads/2022/01/Mantas-PRO.jpg",{"$error":"#VALUE!"}]
[1551,"Manta protección 1100º C - 90x200 cm. (¡Nueva!)","10650910F",108.16,8430133838430]
[1552,"Manta protección 1100º C - Rollo 50 m. x 0.9 m.",105650090950,3482.26,8430133808709,"https://galagar.com/wp-content/uploads/2022/01/Mantas-PRO.jpg",{"$error":"#VALUE!"}]
[1553,"Cortina roja 140x160 cm. Tono 4",1061516,50.41,8430133557959,"https://galagar.com/wp-content/uploads/2022/01/Cortina-Roja.jpg",{"$error":"#VALUE!"}]
[1554,"Cortina roja 140x180 cm. Tono 4",1061518,53.35,8430133557966,"https://galagar.com/wp-content/uploads/2022/01/Cortina-Roja.jpg",{"$error":"#VALUE!"}]
[1555,"Cortina rojo 140x200 cm. Tono 4",1061520,58.29,8430133557973,"https://galagar.com/wp-content/uploads/2022/01/Cortina-Roja.jpg",{"$error":"#VALUE!"}]
[1556,"Cortina verde 9 140x160 cm. Tono 9",1061916,50.41,8430133557980,"https://galagar.com/wp-content/uploads/2022/01/Cortina-Verde.jpg",{"$error":"#VALUE!"}]
[1557,"Cortina verde 9 140x180 cm. Tono 9",1061918,53.35,8430133557997,"https://galagar.com/wp-content/uploads/2022/01/Cortina-Verde.jpg",{"$error":"#VALUE!"}]
[1558,"Cortina verde 9 140x200 cm. Tono 9",1061920,58.29,8430133558000,"https://galagar.com/wp-content/uploads/2022/01/Cortina-Verde.jpg",{"$error":"#VALUE!"}]
[1559,"Cortina transparente 140x160 cm.",1061016,61.74,8430133647353,"https://galagar.com/wp-content/uploads/2022/01/Cortina-Transparente.jpg",{"$error":"#VALUE!"}]
[1560,"Cortina transparente 140x180 cm.",1061018,67.39,8430133647360,"https://galagar.com/wp-content/uploads/2022/01/Cortina-Transparente.jpg",{"$error":"#VALUE!"}]
[1561,"Cortina transparente 140x200 cm.",1061020,73.02,8430133647377,"https://galagar.com/wp-content/uploads/2022/01/Cortina-Transparente.jpg",{"$error":"#VALUE!"}]
[1562,"Estructura 140 cm. con cortina verde",100363919,221.56,8430133605926,"https://galagar.com/wp-content/uploads/2022/01/Estructura-Verde.jpg",{"$error":"#VALUE!"}]
[1563,"Estructura 140 cm. con cortina roja",100363915,221.56,8430133605933,"https://galagar.com/wp-content/uploads/2022/01/Estructura-Roja.jpg",{"$error":"#VALUE!"}]
[1564,"Estructura 200 cm. con cortina verde",100363929,247.01,8430133605575,"https://galagar.com/wp-content/uploads/2022/01/Estructura-Verde.jpg",{"$error":"#VALUE!"}]
[1565,"Estructura 200 cm. con cortina roja",100363925,247.01,8430133605568,"https://galagar.com/wp-content/uploads/2022/01/Estructura-Roja.jpg",{"$error":"#VALUE!"}]
[1566,"Esmeriladora NSLEM-05 - 0,50cv",82800000,1006.95,8430133355357,"https://galagar.com/wp-content/uploads/2022/02/esmeriladora-NSLEM-05.jpg",{"$error":"#VALUE!"}]
[1567,"Esmeriladora NSLE-1 - 2800 rpm.",81200000,1030.28,8430133838973]
[1568,"Esmeriladora E-2 2800 rpm. - Trifásica",80700000,2426.62,8430133315801,"https://galagar.com/wp-content/uploads/2022/02/e-2.jpg",{"$error":"#VALUE!"}]
[1569,"Pulidora P-2 2.800 rpm. - Trifásica",83600000,2532.67,8430133315900,"https://galagar.com/wp-content/uploads/2022/02/p-2foto.jpg",{"$error":"#VALUE!"}]
[1570,"Máquina oxi-corte lineal completa",70748201,1241.3800000000001,8430133626938,"https://galagar.com/wp-content/uploads/2022/01/Carro-Oxicorte.jpg",{"$error":"#VALUE!"}]
[1571,"Gala Cleaner BASIC - limpieza de inox",52500000,1226.72,8430133683009,"https://galagar.com/wp-content/uploads/2022/01/GalaCleaner-Basic_2.jpg",{"$error":"#VALUE!"}]
[1572,"Cable con pincel Gala Cleaner",52512010,236.31,8430133683108]
[1573,"Cable de masa Gala Cleaner",52512011,36.51,8430133683115]
[1574,"Portapincel Gala Cleaner",52512500,126.72,8430133683146]
[1575,"Protección pincel Gala Cleaner BASIC",52512600,25.35,8430133683153]
[1576,"Pincel de grafito M6 Azul para BASIC",52516012,105.6,8430133684778]
[1577,"Líquido limpieza soladadura (1 litro)",52516013,62.75,8430133721268]
[1578,"Gala Cleaner 800 - limpieza de inox",52800000,1963.81,8430133824235,"https://galagar.com/wp-content/uploads/2022/11/GalaCleaner-800-1.jpg",{"$error":"#VALUE!"}]
[1579,"Portapincel Gala Cleaner",52512500,126.72,8430133683146]
[1580,"Líquido limpieza soladadura (1 litro)",52516013,62.75,8430133721268]
[1581,"Kit marcado Gala Cleaner 800",52520700,273.94,8430133823948]
[1582,"Cable sin pincel Gala Cleaner 800",52812009,29.02,8430133824358]
[1583,"Cable de masa Gala Cleaner 800",52812013,45.34,8430133824365]
[1584,"Protección pincel Gala Cleaner 800",52812600,25.35,8430133824266]
[1585,"Pincel de Grafito M6 Negro para Gala Cleaner 800",52816012,116.15,8430133824273]